{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["STOPWATCH01B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"STOPWATCH01B","index":0,"n_rows":43,"n_cols":8,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["STOPWATCH01B"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[7,"R1, R2, R3, R4, R6, R7, R14",100,"R0805","RR-100R SMD","901-002",1,"SMD odpor"]
[1,"R10","1k","R0805","RR-1K SMD","901-029",1,"SMD odpor"]
[6,"R5, R8, R9, R11, R12, R13","10k","R0805","RR-10K SMD","901-003",1,"SMD odpor"]
["Odporové trimry"]
[2,"P1, P2","250/PT10MVE250","PT10V","PT10VE250","112-042",8,"Trimr na ležato"]
[3,"P3, P4, P5","10k/PT10MVK010","PT10V","PT10VK010","112-049",8,"Trimr na ležato"]
["Kondenzátory"]
[2,"C8, C9","22pF","C0805","CK-22P NPO","906-079",2,"SMD keramický kondenzátor"]
[2,"C4, C5","33nF","C0805","CK-33N X7R","906-092",2,"SMD keramický kondenzátor"]
[9,"C2, C3, C6, C7, C10, C11, C12, C13, C14","100nF","C0805","CK-100N Z5U","906-110",2,"SMD keramický kondenzátor"]
[1,"C1","1000uF/16V","CE050X10/L","E1000M/16V","123-172",5,"Elektrolyt, ohnutý na ležato"]
["Diody"]
[1,"D1","1N4007","DO41","1N4007","220-002",1,"Dioda 1A"]
["Tranzistory"]
[2,"Q1, Q2","BC846SMD","SOT23","BC846B","912-009",1,"SMD tranzistor NPN"]
["Integrované obvody"]
[1,"U1",7805,"TO220/L",7805,"330-001",8,"Stabilizátor +5V/1A"]
[1,"U2","LCD_MODULE","LCD_SC1602A","SC1602A","www.hw.cz",120,"LCD displej 2*16 znaků"]
[1,"U3","PIC16F84/SO","SO18_300","PIC16F84-04/SO","967-051",120,"Procesor"]
[1,"U4","MAX232","SO16_150","MAX232 SMD",null,30,"Převodník pro RS232, úzké SO pouzdro"]
["Krystaly"]
[1,"X1","QM4.0MHz","XTAL050","QM 4.000MHZ","131-076",9.9,"Krystal, nízký"]
["Mechanické součásti"]
[1,"J1","K375A","K375A","K375A","806-049",8,"Napájecí konektor souosý"]
[1,"J2","JUMP2X10","JUMP2X10_90","S2G20W","832-024",5,"Hřebínek dvouřadý 90 stupňů, láme se dle potřeby"]
[1,"J3","DB9M_90","CANNON9M_90","CAN9V90","801-037",8,"Konektor RS232"]
[1,"J6","JUMP2","JUMP2","KBI-1541","641-020",10,"Piezoelement, lepí se na plošný spoj"]
[1,"J7","PIC_ISP","PIC_ISP","S1G20S","832-090",5,"Programovací hřebínek, láme se dle potřeby"]
[1,"SW0","P-B143","P-B143/L","P-B143","631-141",5.1,"Přepínač, ohnutý o 90 stupňů"]
[3,"SW1, SW2, SW3","P-DT6BL","PUSH120","P-DT6GE","630-041",12,"Kulaté tlačítko"]
[1,"SW4","P-B1720","PUSH050x050","P-B1720","630-008",3,"Hranaté tlačítko 5x5mm, reset"]
["Konstrukční součásti"]
[5,null,"Jumper",null,"JUMP-SW BLACK","832-013",1,"Propojka"]
[4,null,"Šroub M2.5x8, válcová hlava",null,"Železářství",null,null,"Šrouby pro připevnění LCD displeje"]
[4,null,"Matice M2.5",null,"Železářství",null,null,"Matice pro připevnění LCD displeje"]
[4,null,"Matice M3",null,"Železářství",null,null,"Distanční podložka pod LCD displej"]
[4,null,"Šroub M3x12, křížový, válcová hlava",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]