{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["TRAIN02A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"TRAIN02A","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["TRAIN02A"]
[]
["Počet","Reference","Part","PCB Footprint","Obj číslo","Dodavatel","Cena za kus","Cena","Poznámka"]
["Odpory"]
[1,"R7",1,"R1206",null,null,0.36,0.36]
[2,"R4, R3",27,"R0805",null,null,0.36,0.72]
[2,"R5, R6",330,"R0805",null,null,0.36,0.72]
[10,"R2, R8, R100-R107","1k","R0805",null,null,0.36,3.5999999999999996]
[8,"R200-R207","1k8","RL090","M0.4W-1K8","TME",0.37,2.96,"Drátový R 0.4W"]
[1,"R1","10k","R0805",null,null,0.36,0.36]
["Kondenzátory"]
[2,"C4, C5","#33pF","C0805",null,null,0.3,0.6,"Doporučuji osadit"]
[2,"C10, C11","47pF","C0805",null,null,0.3,0.6]
[9,"C2, C3, C6, C7, C8, C12, C13, C15, C17","100nF","C0805",null,null,0.3,2.6999999999999997]
[4,"C1, C9, C14, C16","4u7/16V","C0805","CL21A475KOFNNNG","TME",0.56,2.24]
["Indukčnosti"]
[1,"L1","MI0805K400R-10","R1206",null,null,null,0]
["Diody"]
[8,"D200-D207","1N4148SMD","SOD87","1N4148-0805","TME",0.3,2.4,"Dioda 500mA (je nějak moc malé pouzdro)"]
[1,"D4","M6","SMA","M6","TME",0.3,0.3,"Dioda 800V/1A"]
[1,"D3","10MQ040N","SMA","10MQ040N","TME",0.3,0.3,"Dioda Schottky 1.5A"]
["Diody LED"]
[9,"D1, D220-D227","HCL-1503-4(GREEN)","LED1206REV","OF-SMD3216G","TME",2.86,25.74,"Želená SMD LED, krásně svítí"]
[10,"D2, D5, D100-D107","HCL-1505-4(RED)","LED1206REV","OF-SMD3216R","TME",3.75,37.5,"Červená SMD LED, krásně svítí"]
["Integrované obvody"]
[1,"U1","ATmega8L-8PU","DIP28_300","ATmega8L-8PU","TME",25.69,25.69,"Procesor"]
[1,"U2","FT230XS","SSO16_154","FT230XS-R","TME",50.07,50.07,"USB - RS232"]
[1,"U3","ULN2803A","DIP18_300","ULN2803A","TME",6.82,6.82,"Budič darlingtony"]
[1,"U4","LM7805T","TO220/L",7805,"TME",3.98,3.98,"Stabilizátor 5V"]
["Krystal"]
[1,"X1","#8MHz","XTAL050",null,null,null,0,"Doporučuji osadit kontakty"]
["Optrony"]
[8,"Q200-Q207","PC357","PC357","PC357N3TJ00F","TME",3.98,31.84,"Optron SMD obyčejný"]
["Relé"]
[8,"RE0-RE7","FTR-F1CA012V","RELAY29x13_8pin","FTR-F1CA012V","TME",33.92,271.36,"Relé 12V, kontakty 5A/24VDC 5A/250VAC"]
["Tlačítka"]
[8,"SW0-SW7","P-DT6GE","PUSH120","KS01-BV-RED","TME",6.16,49.28,"Ovládací tlačítka"]
[1,"SW8","P-B1720","PUSH050x050","B3F-1000","TME",0.4,0.4,"Reset tlačítko 5x5mm"]
["Svorky WAGO"]
[8,"J0-J7","WAGO256_x04","WAGO256_x04",null,null,0,0]
[1,"J9","WAGO256_x16","WAGO256_x16",null,null,0,0]
[48,null,null,"Základní svorka",null,"UST",6.1,292.79999999999995]
[9,null,null,"Čelíčko",null,"UST",2.2,19.8]
["Konektory"]
[1,"J13","K375A","K375A","PC-GK2.1/SMD","TME",14.7,14.7,"Napájecí konektor"]
[1,"J10","USB_B_01","USB_B_01","TUEB4F2D0B","TME",18.8,18.8,"USB konektor typ B"]
["Jumpery"]
[2,"J8, J16","JUMP9","JUMP9",null,null,0,0]
[1,"J11","JUMP2X2","JUMP2X2",null,null,0,0]
[2,"J12, J15","JUMP2x3","JUMP2x3",null,null,0,0]
[1,"J14","JUMP2X4","JUMP2X4",null,null,0,0]
[0.45,null,"S1G40",null,"Jednořadý hřebínek 40 pinů","GME",8.9,4.005]
[0.3,null,"S2G80",null,"Dvouřadý hřebínek 2x40 pinů","GME",15.5,4.6499999999999995]
["Ostatní materiál"]
[1,"M101","PCB_TRAIN01A","Plošný spoj",null,null,100,100]
[1,"M102","Power Supply 12V","Napájecí zdroj 12V/1.2A","ZSI12/1.25A","TME",156.8,156.8,"Napájecí zdroj, pěkný malý a netopí"]
[2,"M201, M202","JUMPER","Jumper propojka",null,null,1,2]
[1,"M203","DIL28_300 Socket","Precizní patice DIL28 úzká",null,null,16,16]
[5,null,"Šroub M3x6 pozink, válcová hlava",null,null,null,1,5]
[1,null,"Matice M3 pozink",null,null,null,1,1]
[4,null,"Podložka M3 pozink",null,null,null,0.2,0.8]
[4,null,"Sloupek M3x5 šroub/matice",null,null,null,2,8]
[{"$nulls":7},1164.8949999999998]