{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":37,"n_cols":4,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Bill Of Materials          April 9,2009      8:30:23","Page1"]
[]
["Quantity","Reference","Part","PCB Footprint"]
["______________________________________________"]
[]
[1,"C1","470uF/16V","CE050X10"]
[10,"C2,C4,C5,C6,C7,C8,C9,C10,","100nF","C0805"]
[null,"C11,C16"]
[1,"C3","10uF/6.3V","ELYTB"]
[1,"C12","1uF","C0805"]
[1,"C13","#","ELYTB"]
[2,"C14,C15","22pF","C0805"]
[1,"D2","BRIDGE-DIL","DI1106"]
[1,"D3","1N4148SMD","SOD87"]
[1,"EA1","PIEZO","BEPEER"]
[1,"F1","FUSE_F1812","CE050X10"]
[2,"J1,J2","ARK210/3","ARK210/3"]
[1,"J3","JUMP2x3","JUMP2x3/B"]
[1,"J4","PT100","ARK210/2"]
[1,"L1","10uH","L1210"]
[1,"P1","10k","PT6V"]
[1,"Q1","SHARP_S202S01","TRIAC_S202S01"]
[1,"Q2","BC817SMD","SOT23"]
[1,"R1",180,"R0805"]
[2,"R5,R2","10k","R0805"]
[4,"R3,R4,R6,R7","4k7","R0805"]
[1,"R8","1k","R0805"]
[2,"SW1,SW2","P-B1720","PUSH050x050"]
[1,"T1","trafo","TRAFO-HAHN2_6VA"]
[1,"U1","ATmega8L-8AU","TQFP32"]
[1,"U2","LExxD","SO8_150"]
[1,"U3","TLC27L2","SO8_150"]
[1,"U4","LCD_MODULE 8x2","LCD_MC0802A"]
[1,"U5","MCP1525","SOT23"]
[1,"X1","XTAL050","XTAL050"]
[]
[1,"PT1000"," teplotní čidlo např.: od TME PT106052"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}