{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["VZOR"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"VZOR","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["VZOR"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[3,"R1,R3,R6",100,"R0805","RR-100R SMD","901-002",1]
[1,"R10",220,"R0805","RR-220R SMD","901-055",1]
["Odporové trimry"]
[2,"P1,P2","100k","TRIMB","4312-SMD 100K","903-024",13]
["Keramické kondenzátory"]
[2,"C7,C8","10nF","C0805","CK-10N X7R","906-089",2,"Blokovací kondenzátor"]
[2,"C5,C6","100nF","C0805","CK-100N X7R","906-096",2,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
["Elektrolytické kondenzátory"]
[1,"C1","1000uF/6.3V","CE035X8",null,null,null,"Kondenzátor z mainboardu (je menší)"]
[1,"C4","10G/16V","CE075X18","E10000M/16V","123-209",45,"Hlavní akumulační kondenzátor"]
["Indukčnosti"]
[1,"TR1","L-TR-1P1S_DOT","TOROID4",null,null,null,"Trafo na toroidu H22, 10mm, 2x70 závitů, vzduchová mezera"]
["Diody"]
[1,"D1","BZV55C5.6SMD","MINIMELF","BZV55C5.6SMD","919-010",1.3,"Ochranná Zenerova dioda"]
[2,"D2,D3","SK54ASMD","SMC","SK54ASMD","920-108",12,"Výkonová Schottkyho dioda"]
["Tranzistory"]
[1,"Q1","IRF7301","SO8_150","IRF7301","213-156",17,"Výkonový dvojitý N-FET v pouzdru SO8, min na 20V"]
[1,"Q2","2N7002SMD","SOT23","2N7002SMD","912-040",2.3,"N-FET signálový tranzistor"]
["Integrované obvody"]
[1,"U1","PIC16F88/SO","SO18_300","PIC16F88-I/SO","967-113",91,"Procesor"]
[1,"U2","LM385-1.2_SO8","SO8_150","LM385D-1,2-SMD","934-046",10.5,"Referenční zdroj"]
["Mechanické součástky "]
[1,"J1","BAT","JUMP2","S1G20","832-017",4,"Konektor připojení slunečních článků, nalámat dle potřeby"]
[3,"J2,J3,J6","JUMP2","JUMP2","\"",null,null,"Pomocné konektory"]
[]
[]
[]
["Úkony:"]
[null,"Uložit pod novým jménem"]
[null,"Přejmenovat list"]
[null,"Přepsat jméno modulu na první řádce tabulky"]
[null,"Otevřít seznam jako další tabulku (textový soubor s tabulátory jako oddělovači)"]
[null,"Seřadit řádky v tabulce, seřadit reference podle logického pořadí."]
[null,"Nakopírovat příslušná data do vzorové tabulky"]
[null,"Vymazat pomocný list"]
[null,"Vymazat tento návod"]
[null,"Uložit seznam"]