{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["05-60009"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":101,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"05-60009","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["02-01841 Rev 5",null,null,null,"Ethernet PICtail"]
["Note: Use Vendor part number for reference, a few Digikey part numbers may be the lead version"]
["Count","ComponentName","RefDes","Value","Description","Vendor","Vendor #","Digikey #","RoHS"]
[]
[1,"BRRECT-W02M","CR1",null,"RECTIFIER BRIDGE 1.5A 200V WOG","General Semiconductor","W02G-E4","W02GGI-ND",true]
[1,null,"U1","25C256","EEPROM","Microchip","25LC256-I/SN",null,true]
[1,null,"U3","ENC28J60","Ethernet IC","Microchip","ENC28J60-I/ML",null,true]
[1,"MC74VHCT125A-D","U2",null,"IC QUAD BUFF HS TRI-ST 14-SOIC","On Semiconductor","MC74VHCT125A-D","Newark 75C3053",true]
[1,"MC78XX_DPAC","Q2",null,"IC REGULATOR LDO 1A TO-263","National Semiconductor","LM2940S-5.0/NOPB","LM2940S-5.0-ND",true]
[0,"MC78XX_DPAC","Q1","No Load","IC REGULATOR LDO TO-263","National Semiconductor","LM3940IS-3.3","LM3940IS-3.3-ND","N/A"]
[1,"MC78XX_DPAC","Q1",null,"500mA Fixed Output CMOS LDO","Microchip","TC1262-3.3VEB",null,true]
[12,"CAP0603","C1, C2, C3, C4, C6, C7, C8, C9, C11, C13, C14, C18",".1uF","CAP SMT, 0.1uF 0603 CER 16V 10% X7R","NIC COMPONENTS CORP","NMC0603X7R104K16TRPF",null,true]
[2,"CAP0603","C5, C17","33pf","CAP CER 33PF 50V C0G 5% 0603","TDK Corporation","C1608C0G1H330J","445-1275-1-ND",true]
[1,"CAP0805","C12","10uF","CAP CER 10UF 6.3V Y5V 0805","Murata","GRM21BF50J106ZE01L","490-1746-1-ND",true]
[2,"CAP B","C15, C16","33uF","CAP 33UF 10V ELECT VS SMD","Panasonic - ECG","EEE1AA330WR","PCE3175CT-ND",true]
[1,"CAP_SMT_F","C10","220uF","CAP 220UF 25V ELECT VS SMD","Panasonic - ECG","EEE1EA221UP","PCE3187TR-ND",true]
[1,"CRYSTAL_CS10","Y1","25Mhz","CRYSTAL 25.0000 MHZ 18PF SMD","CITIZEN","CS10-25.000MABJTR","300-8105-1-ND",true]
[4,"RES0603","R3, R4, R5, R6","49.9, 1%","RES 49.9 OHM 1/16W 1% 0603 SMD","Rohm","MCR03EZPFX49R9","RHM49.9HCT-ND",true]
[6,"RES0603","R2, R7, R9, R10, R11, R12","180","RES 180 OHM 1/10W 5% 0603 SMD","Rohm","MCR03EZPJ181","RHM180GCT-ND",true]
[1,"RES0603","R8","2.7K, 1%","RES 2.70K OHM 1/10W 1% 0603 SMD","Rohm","MCR03EZPFX2701","RHM2.70KHCT-ND",true]
[1,"RES0603","R1","100K","RES SMT, 100K-OHM 1/16W 5% 0603","KOA","RK73B1JTTD104J",null,true]
[1,"DJ005B","J11",null,"CONN, JACK, 2.5mm DC PC MOUNT","KYCON","KLD-0202-B",null,true]
[1,"INDUCTOR-1210","L1","60ohm","FERRITE 1.5A 60 OHM 1210 SMD","Steward","MI1210K600R-10","240-2416-1-ND",true]
[1,"LED-0805","D1","GREEN","LED THIN 565NM GRN DIFF 0805 SMD","Lumex Opto","SML-LXT0805GW-TR","67-1553-1-ND",true]
[1,null,"J1",null,"Mag Jack","Bel Stewart","08B0-1X1T-36-F",null,true]
[0,"Alternate","J1",null,"Pulse Jack","Pulse Engineering","JP011821UNL",null,true]
[1,null,"J2",null,"CONN HEADER .100 DUAL R/A 28POS","SAMTEC","TSW-114-08-G-D-RA",null,true]
[1,null,"J3",null,"2x14 header female","SAMTEC","SSW-114-01-T-D",null,true]
[1,null,"None",null,"2x14 header female (ship loose in box)",null,null,null,true]
[0,null,"J8, JP1, JP2, JP3","No Load",{"$nulls":4},"N/A"]
[0,null,"J4, J5, J6, J7","No Load",{"$nulls":4},"N/A"]
[1,null,"J9",null,"1x3 header","SAMTEC","TSW-103-07-S-S",null,true]
[1,"Load @","J9 (pins 2&3)",null,"2 pin shorting jumper","AMP/TYCO","382811-6","A26227-ND",true]
[0,null,"J10","No Load","2x6 header",null,null,null,"N/A"]
[1,null,"TP2",null,"TEST POINT, BLACK (0.063\" HOLE)","COMPONENTS CORP","TP-106-01-00",null,true]
[2,null,"TP1, TP3",null,"TEST POINT, RED (0.063\" HOLE)","COMPONENTS CORP","TP-106-01-02",null,true]
[]
["Changes from Rev 3"]
["C3","Change from .01uF to .1uF"]
["C12","Change from electrolitic to ceramic"]
["R12","Add 200 ohm (new value)"]
["R9","Change from 100K to 200 ohm"]
["R11","Change from NL to 200 ohm"]
["JP1, JP2, JP3","Add No Load"]
["C19","Delete"]
["Y1","Change to new part"]
["L1","Change to RoHS part (-10 suffix)"]
[]
["C5, C17","Change to 33pf"]
["R9, R10, R11, R12","Change to 180 Ohm"]