{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["05-60009"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":101,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"05-60009","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["02-01898 Rev 5",null,null,null,"PICtail Plus Ethernet"]
["Count","ComponentName","RefDes","Value","Description","Vendor","Vendor #","Digikey #","RoHS"]
[]
[1,null,"U3","ENC28J60","Ethernet IC","Microchip",null,null,true]
[7,"CAP0603","C2, C3, C4, C6, C7, C13, C14",".1uF","CAP SMT, 0.1uF 0603 CER 16V 10% X7R","NIC COMPONENTS CORP","NMC0603X7R104K16TRPF",null,true]
[2,"CAP0603","C5, C17","33pf","CAP CER 33PF 50V C0G 5% 0603","TDK Corporation","C1608C0G1H330J","445-1275-1-ND",true]
[1,"CAP0805","C12","10uF","CAP CER 10UF 6.3V Y5V 0805","Murata","GRM21BF50J106ZE01L","490-1746-1-ND",true]
[1,"CRYSTAL_CS10","Y1","25Mhz","CRYSTAL 25.0000 MHZ 18PF SMD","CITIZEN","CS10-25.000MABJTR","300-8105-1-ND",true]
[4,"RES0603","R3, R4, R5, R6","49.9, 1%","RES 49.9 OHM 1/16W 1% 0603 SMD","Rohm","MCR03EZPFX49R9","RHM49.9HCT-ND",true]
[5,"RES0603","R2, R7, R9, R11, R12","180","RES 180 OHM 1/10W 5% 0603 SMD","Rohm","MCR03EZPJ181","RHM180GCT-ND",true]
[0,"RES0603","R10","No Load",{"$nulls":4},"N/A"]
[1,"RES0603","R8","2.32K, 1%","RES 2.32K OHM 1/10W 1% 0603 SMD","Rohm","MCR03EZPFX2321","RHM2.32KHCT-ND",true]
[1,"INDUCTOR-1210","L1","60ohm","FERRITE 1.5A 60 OHM 1210 SMD","Steward","MI1210K600R-10","240-2416-1-ND",true]
[1,null,"J1",null,"Mag Jack","Bel Stewart","08B0-1X1T-36-F",null,true]
[0,"Alternate","J1",null,"Pulse Jack","Pulse Engineering","JP011821UNL",null,true]