{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["05-60009"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":102,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"05-60009","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["02-02027","Rev 2",null,null,"Internet Radio"]
["Count","ComponentName","RefDes","Value","Description","Vendor","Vendor #","Digikey #","RoHS"]
[1,"DIODE","D4",null,"SMD Transient Voltage Suppression Arrays","AVX","MG054S05X150DP",null,true]
[1,"DIODE_SOD-323","D5",null,"DIODE SCHOTTKY 0.5A 20V SOD-123","Fairchild Semiconductor","MBR0520L","MBR0520LCT-ND",true]
[1,"MGSF1N02LT1_SOT23","Q1",null,"MOSFET N-CHAN 750MA 20V SOT23","ON Semiconductor","MGSF1N02LT1G","MGSF1N02LT1GOSCT-ND",true]
[1,"PIC18F67J60","U1",null,null,"Microchip","PIC18F67J60-I/PT",null,true]
[1,"TC55-SOT89","U5",null,"Voltage Regulator","Microchip","MCP1703T-3302E/MB",null,true]
[2,"N256S0818_SOIC150","U4, U6",null,"32K x 8 serial SRAM","AMERICAN MICROSYSTEMS","N256S0830HDAS2-20I",null,true]
[1,"VS1011_LQFP48","U2",null,"MP3 Decoder IC","VLSI","VS1011E-L",null,true]
[1,"OLED_HS1101A","LCD1",{"$nulls":5},true]
[1,"LED-0805","D3",null,"LED THIN 565NM GRN DIFF 0805 SMD","Lumex Opto/Components","SML-LXT0805GW-TR","67-1553-1-ND",true]
[2,"CAP0603","C27, C28","22pf","CAP CER 22PF 50V C0G 5% 0603","TDK Corporation","C1608C0G1H220J","445-1273-1-ND",true]
[2,"CAP0603","C7, C8","33pf","CAP CER 33PF 50V C0G 5% 0603","TDK Corporation","C1608C0G1H330J","445-1275-1-ND",true]
[1,"CAP0603","C30","1nF","CAP 1000PF 100V CERAMIC X7R 0603","Panasonic - ECG","ECJ-1VB2A102K","PCC1952TR-ND",true]
[2,"CAP0603","C35, C36","10nF","CAP 10000PF 25V CERM X7R 0603","Panasonic - ECG","ECJ-1VB1E103K","PCC1763TR-ND",true]
[2,"CAP0603","C26, C37","47nF","CAP 47000PF 50V CERM Y5V 0603","Panasonic - ECG","ECJ-1VF1H473Z","PCC1805TR-ND",true]
[17,"CAP0603","C1, C2, C3, C4, C5, C6, C10, C11, C14, C15, C18, C23, C25, C29, C32, C38,C39",".1uF","CAP .1UF 16V CERAMIC Y5V 0603","Panasonic - ECG","ECJ-1VF1C104Z","PCC1788TR-ND",true]
[3,"CAP0603","C9, C16, C19","1uF","CAP SMT, 1.0uF 0603 CER 16V 10% X5R","PANASONIC","ECJ-1VB1C105K","PCC2224CT-ND",true]
[1,"CAP0603","C13","4.7uF","CAP CERAMIC 4.7UF 6.3V X5R 0603","Panasonic - ECG","ECJ-1VB0J475M","PCC2318CT-ND",true]
[1,"CAP0805","C31","2.2uF","CAP 2.2UF 25V CERAMIC F 0805","Panasonic - ECG","ECJ-2FF1E225Z","PCC2231CT-ND",true]
[1,"CAP0805","C20","10uF","CAP CER 10UF 6.3V Y5V 0805","Murata","GRM21BF50J106ZE01L","490-1746-1-ND",true]
[1,"CAP3528","C34","6.8uF","CAP TANTALUM 6.8UF 16V 20% SMD","Kemet","B45196H3685M209","495-2235-1-ND",true]
[1,"CAP_POL_3528","C17","10uF","CAPACITOR TANT 10UF 16V 10% SMD","Kemet","T491B106K016AT","399-3706-1-ND",true]
[1,"CAP_SMT_F","C33","220uF","CAP 220UF 25V ELECT VS SMD","Panasonic - ECG","ECE-V1EA221UP","PCE3187CT-ND",true]
[1,"CC_1008LS","L3","10uH","1008PS Series Power Chip Inductors","COILCRAFT","1008PS-103KLB",null,true]
[1,"DO1606","L2","10uH","1606 Series Power Chip Inductors","COILCRAFT","DO1606T-103MBL",null,true]
[1,"INDUCTOR-1210","L1","60ohm","FERRITE 1.5A 60 OHM 1210 SMD","Steward","MI1210K600R-10","240-2416-1-ND",true]
[1,"CRYSTAL_CS10","Y1","25Mhz","CRYSTAL 25.0000 MHZ 18PF SMD","CITIZEN","CS10-25.000MABJTR","300-8105-1-ND",true]
[1,"CRYSTAL_CS10","Y2","24.576Mhz","CRYSTAL 24.5760 MHZ 18PF SMD","CITIZEN","CS10-24.576MABJ-UT","300-8104-1-ND",true]
[1,null,"J1",null,"Mag Jack","Bel Stewart","08B0-1X1T-36-F",null,true]
[1,"DJ005B","J3",null,"CONN JACK POWER 2.1MM PCB","CUI Inc","PJ-102A","CP-102A-ND",true]
[1,"PHONE_SJ3505","J2",null,"CONN 3.5MM RTANG STEREO JACK PCB","CUI Inc","SJ-3505","CP-3505-ND",true]
[1,"RJ11_6PIN","J4",null,"CONN, MOD JACK 6-6 SIDE ENTRY LOW PROFILE","AMP/TYCO","555165-1","A9031-ND",true]
[3,"RES0603","R29, R30, R31","10 Ohm","RES 10 OHM 1/10W 5% 0603 SMD","Panasonic - ECG","ERJ-3GEYJ100V","P10GTR-ND",true]
[2,"RES0603","R20, R21","20 Ohm","RES 20 OHM 1/10W 5% 0603 SMD","Panasonic - ECG","ERJ-3GEYJ200V","P20GTR-ND",true]
[4,"RES0603","R4, R5, R7,R8","49.9, 1%","RES 49.9 OHM 1/16W 1% 0603 SMD","Rohm","MCR03EZPFX49R9","RHM49.9HCT-ND",true]
[3,"RES0603","R6, R9, R12","180","RES 180 OHM 1/10W 5% 0603 SMD","Rohm","MCR03EZPJ181","RHM180GCT-ND",true]
[1,"RES0603","R2","2.26K, 1%","RES 2.26K OHM 1/10W 1% 0603 SMD","Panasonic - ECG","ERJ-3EKF2261V","P2.26KHCT-ND",true]
[6,"RES0603","R10, R11, R14, R17, R18, R23","10K","RES SMT, 10K-OHM 1/10W 5% 0603","Panasonic - ECG","ERJ-3GEYJ103V","P10KGTR-ND",true]
[4,"RES0603","R22, R32, R33, R34","100K","RES 100K OHM 1/10W 5% 0603 SMD","Panasonic - ECG","ERJ-3GEYJ104V","P100KGTR-ND",true]
[1,"RES0603","R16","110K 1%","RES 110K OHM 1/10W 1% 0603 SMD","Panasonic - ECG","ERJ-3EKF1103V","P110KHTR-ND",true]
[1,"RES0603","R13","820K","RES 820K OHM 1/10W 5% 0603 SMD","Panasonic - ECG","ERJ-3GEYJ824V","P820KGTR-ND",true]
[1,"RES0603","R15","931K 1%","RES 931K OHM 1/10W 1% 0603 SMD","Panasonic - ECG","ERJ-3EKF9313V","P931KHTR-ND",true]
[1,"RES0603","R19","1M","RES SMT, 1.0M-OHM 1/10W 5% 0603","YAGEO/PHYCOMP","RC0603JR-071ML",null,true]
[1,"RES0805","R24","0.12 ohm","RES .12 OHM 1/2W 1% 1206 SMD","Susumu Co Ltd","RL1632R-R120-F","RL16R.12FCT-ND",true]
[2,"RES1206","R25, R26","2 Ohm","RES 2.00 OHM 1/4W 1% 1206 SMD","Rohm","MCR18EZHFL2R00","RHM2.00FCT-ND",true]
[3,"SW-PUSH_SMT","S1, S2, S3",null,"SWITCH LT TOUCH 6X3.5 100GF SMD","Panasonic - ECG","EVQ-PJS04K","P8048SCT-ND",true]
[4,null,null,null,"BUMPON TALL TAPER SQ .50X.23 BK","3M/ESM","SJ-5518 (BLACK)","SJ5518-0-ND",true]
[0,"SIP_4",null,"No Load"]
[1,"PCB",null,null,null,"Advanced Circuits","05-60142_REV_C",null,true]