{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["05-60009"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":101,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"05-60009","index":0,"n_rows":66,"n_cols":9,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["02-01935 Rev 4",null,null,null,"PICDEM.net 2"]
["Count","ComponentName","RefDes","Value","Description","Vendor","Vendor #","Digikey #","RoHS"]
[]
[1,null,"D10","IN4001","RECTIFIER GPP 400V 1A SMB","DIODES INC","S1GB-13-F","S1GB-FDICT-ND",true]
[1,null,"U4","25C256","EEPROM","Microchip","25LC256-I/SN",null,true]
[1,null,"U2","ENC28J60","Ethernet IC","Microchip","ENC28J60-I/ML",null,true]
[1,"TC1047_SOT23","U1",null,"IC SMT, TC1047A, 3L SOT-23","Microchip","TC1047AVNBTRG",null,true]
[32,"CAP0603","C1, C10, C11, C12, C13, C15, C16, C17, C18, C20, C21, C22, C23, C24, C26, C28, C29, C31, C32, C33, C36, C37, C38, C39, C40, C41, C42, C43, C44, C47, C50, C52",".1uF","CAP SMT, 0.1uF 0603 CER 16V 10% X7R","NIC COMPONENTS CORP","NMC0603X7R104K16TRPF",null,true]
[1,"CAP0603","C34","1Uf","CAP SMT, 1.0uF 0603 CER 16V 10% X5R","PANASONIC","ECJ-1VB1C105K","PCC2224CT-ND",true]
[4,"CAP0603","C19, C25,C30,C35","33pf","CAP CER 33PF 50V C0G 5% 0603","TDK Corporation","C1608C0G1H330J","445-1275-1-ND",true]
[2,"CAP0603","C45, C46","22pf","CAP SMT, 22pF 0603 CER 50V 5% NP0","PANASONIC","ECJ-1VC1H220J","PCC220ACVTR-ND",true]
[1,"CAP0805","C27","10uF","CAP CER 10UF 6.3V Y5V 0805","Murata","GRM21BF50J106ZE01L","490-1746-1-ND",true]
[2,"CAP_SMT_D","C48, C51","47uF","CAP 47UF 16V VS ELECT SMD","Panasonic - ECG","ECE-V1CA470SP","PCE3064CT-ND",true]
[1,"CA-_SMT_F","C49","220uF","CAP ELECT 220UF 25V VS SMD","Panasonic - ECG","EEE-1EA221UP","PCE3902CT-ND",true]
[0,"CONN_FPC_SD_54132","J3","No Load",{"$nulls":4},"N/A"]
[1,"CRYSTAL_32KHZ","Y3","32Khz","CRYSTAL 32.768KHZ CYLINDER","ECS Inc.","ECS-3X8","X801-ND",true]
[2,"CRYSTAL_CS10","Y1, Y2","25Mhz","CRYSTAL 25.0000 MHZ 18PF SMD","CITIZEN","CS10-25.000MABJTR","300-8105-1-ND",true]
[1,"DE9S-FRS","P1","RS-232","CONN, D-SUB, 9P RECPT RT ANGLE W/ JACK SCREWS","TYCO","7-747844-0",null,true]
[1,"DJ005B","J7",null,"CONN, JACK, 2.5mm DC PC MOUNT","KYCON","KLD-0202-B",null,true]
[1,"RJ11_6PIN","J4",null,"CONN, MOD JACK 6-6 SIDE ENTRY LOW PROFILE","AMP/TYCO","555165-1","A9031-ND",true]
[1,"HDR2X6","J6",null,"2x6 Header","3M Electronic Solutions","929852-01-06-10","517-852-01-06 Mouser",true]
[1,"HDR2X14","J5",null,"2x14 Header","3M Electronic Solutions","929852-01-14-10","517-852-01-14 Mouser",true]
[0,"ICE header","U1A","No Load","25 pin male header","Samtec","MTMS-125-01-G-S-230",null,true]
[1,"JUMPER","JP9",null,"1x2 Header",null,null,null,true]
[0,"JUMPER","JP1, JP2, JP3, JP4, JP6, JP7, JP8, JP10, JP11, JP12, JP13, JP14, JP15, JP16, JP17, JP18, JP19, JP20, JP21, JP22, ","No Load","1x2 Header",null,null,null,true]
[1,"SIP_3","JP5",null,"1x3 Header",null,null,null,true]
[1,null,"LCD",null,"LCD MODULE 16X2 CHARACTER","Lumex Opto","LCM-S01602DTR/M","67-1781-ND",true]
[9,"LED_LTL-PGK-TA","D1, D2, D3, D4, D5, D6, D7, D8, D9",null,"LED SMT, 2.7x3.5mm GREEN CLEAR PLCC-2","FAIRCHILD SEMI","QTLP670NC-4",null,true]
[1,"MAX232A-SO16","U5","MAX232","IC DRVR/RCVR MULTCH RS232 16SSOP","Texas Instruments","MAX3232CDBR","296-13093-1-ND",true]
[1,"MC78XX_DPAK","Q1",null,"IC SMT, REG, +5V 1A SOT-263","NATIONAL SEMI","LM2940CS-5.0 NOPB","LM2940S-5.0-ND",true]
[1,"MC78XX_DPAK","Q2",null,"IC SMT, TC1262-3.3, DDPAK","Microchip","TC1262-3.3VEB",null,true]
[1,"PIC18F97J60-TQF","U3",null,null,"Microchip","PIC18F97J60",null,true]
[0,"CAP3528","C6, C7, C8, C9, C14","No Load",{"$nulls":4},"N/A"]
[0,"CAP3528","C2, C3, C4, C5","No Load",{"$nulls":4},"N/A"]
[1,"POT_MIN","R38","10K","POT 10K OHM THUMBWHEEL CERM ST","Bourns Inc.","3352T-1-103LF","3352T-103-ND",true]
[2,"RES0603","R30, R31","0 ohm","RES SMT, 0-OHM 0603","PANASONIC","ERJ-3GSY0R00V","P0.0GTR-ND",true]
[1,"RES0603","R36","10 ohm","RES SMT, 10-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GEYJ100V","P10GTR-ND",true]
[1,"RES0603","R21","100 ohm","RES SMT, 100-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GEYJ101V","P100GTR-ND",true]
[5,"RES0603","R7, R8, R9, R14, R39","180 ohm","RES SMT, 180-OHM 1/10W 5% 0603","Rohm","MCR03EZPJ181","RHM180GCT-ND",true]
[8,"RES0603","R3, R4, R5, R6, R10, R11, R12, R13","49.9, 1%","RES 49.9 OHM 1/16W 1% 0603 SMD","Rohm","MCR03EZPFX49R9","RHM49.9HCT-ND",true]
[13,"RES0603","R22, R23, R24, R25, R26, R27, R28, R29, R37, R40, R41, R42, R43","470 ohm","RES SMT, 470-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GEYJ471V","P470GTR-ND",true]
[1,"RES0603","R33","1K","RES SMT, 1.0K-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GEYJ102V","P1.0KGCT-ND",true]
[1,"RES0603","R17","1.3K","RES 1.3K OHM 1/10W 5% 0603 SMD","PANASONIC","ERJ-3GEYJ132V","P1.3KGTR-ND",true]
[1,"RES0603","R15","2.32K 1%","RES 2.32K OHM 1/10W 1% 0603 SMD","PANASONIC","ERJ-3EKF2321V","P2.32KHTR-ND",true]
[1,"RES0603","R20","2.26K 1%","RES 2.26K OHM 1/10W 1% 0603 SMD","PANASONIC","ERJ-3EKF2261V","P2.26KHTR-ND",true]
[3,"RES0603","R1, R2, R32","4.7K","RES SMT, 4.7K-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GEYJ472V","P4.7KGTR-ND",true]
[7,"RES0603","R16, R44, R45, R46, R47, R50, R51","10K","RES SMT, 10K-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GSYJ103V","P10KGTR-ND",true]
[1,"RES0603","R34","100K","RES SMT, 100K-OHM 1/10W 5% 0603","PANASONIC","ERJ-3GSYJ104V","P100KGTR-ND",true]
[1,"RES0603","R35","1M","RES 1.0M OHM 1/10W 5% 0603 SMD","PANASONIC","ERJ-3GEYJ105V","P1.0MGCT-ND",true]
[2,"RES1206","R48, R49","2 ohm 1%","RES 2.00 OHM 1/4W 1% 1206 SMD","Rohm","MCR18EZHFL2R00","RHM2.00FCT-ND",true]
[0,"RES0603","R18, R19","No Load"]
[2,"INDUCTOR-1210","L1, L2","60ohm","FERRITE 1.5A 60 OHM 1210 SMD","Steward","MI1210K600R-10","240-2416-1-ND",true]
[0,"RES0603","R10","No Load",{"$nulls":4},"N/A"]
[5,"SW-PUSH_SMT","S1, S2, S3, S4, S5",null,"SWITCH TACT 6MM SMD MOM 230GF","Omron Electronics","B3S-1002","SW416-ND",true]
[2,null,"J1, J2",null,"Mag Jack","Bel Stewart","08B0-1X1T-36-F",null,true]
[0,"Alternate","J1, J2",null,"Pulse Jack","Pulse Engineering","JP011821UNL",null,true]
[2,null,"TP3, TP5",null,"TEST POINT PC MULTI PURPOSE BLK","COMPONENTS CORP","TP-106-01-00",null,true]
[2,null,"TP2, TP4",null,"TEST POINT PC MULTI PURPOSE RED","COMPONENTS CORP","TP-106-01-02",null,true]
[1,null,"TP1",null,"TEST POINT PC MULTI PURPOSE WHT","Keystone Electronics","5012","5012K-ND",true]
[5,null,null,null,"BUMPON TALL TAPER SQ .50X.23 BK","3M/ESM","SJ-5518 (BLACK)","SJ5518-0-ND",true]
[1,null,null,null,"PCB","Advanced Circuits","05-60079_REV4",null,true]
[]
[]
[]
["Changes from Rev 3"]
["Add","R50, R51","0603  10K"]