{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ATmega801B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ATmega801B","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["ATmega801B"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R1",100,"R0805","RR-100R SMD","901-002",1]
[4,"R2, R101, R102, R103","10k","R0805","RR-10K SMD","901-003",1]
[1,"R3","#R","R0805",null,null,1,"Osazuje se pouze při použití RC oscilátoru"]
["Keramické kondenzátory"]
[2,"C4, C5","22pF","C0805","CK-22P NPO","906-079",2]
[3,"C101, C102, C103","10nF","C0805","CK-10N X7R","906-089",2,"Blokovací kondenzátor"]
[4,"C2, C3, C6, C7","100nF","C0805","CK-100N X7R","906-096",2,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
["Elektrolytické kondenzátory"]
[1,"C1","22uF/6.3V","ELYTC","CTS 22M/6.3V C","907-032",4,"SMD elyt, velikost C"]
["Indukčnosti"]
[1,"L1","10uH","L1210","TL.10uH SMD","965-001",7.5,"SMD tlumivka"]
["Diody"]
[1,"D1","1N4007SMD","MELF","1N4007SMD","917-005",2,"Dioda 1A"]
["Integrované obvody"]
[1,"U1","ATmega8L-8AU","TQFP32","ATmega8L-8AU","958-109",39,"Procesor ATMEL, možno i verze AC nebo AI"]
["Krystaly"]
[1,"X1","8MHz","XTAL050/LG","Q 8MHZ","131-059",9.9,"Krystal dle potřeby a procesoru, možno i QM 8MHZ 131-073"]
[0,"X2","#32768Hz","XTAL010/LG","Q 32.768KHZ","131-036",5,"Hodinkový krystal, osazuje se buď X1 nebo X2"]
["Mechanické součástky "]
[4,"J1..J8, J9..J16, J17..J24, J25..J32","JUMP2x8","JUMP2x8","S2G80","832-033",14,"Dvouřadý hřebínek nalámat dle potřeby"]
[2,"J33, J35","JUMP2X3","JUMP2X3/B","\"",null,null,"Napájecí a programovací hřebínek"]
[4,"J101+J103+J105, J102+J104+J106, J107+J109+J111, J108+J110+J112","JUMP3","JUMP3","S1G20","832-017",4,"Jednořadý hřebínek"]
[1,"SW1","P-B1720","PUSH050x050","P-B1720","630-008",3,"Obyčejné tlačítko 5x5mm"]
["Konstrukční součástky"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]