{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ATmegaTQ6401A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ATmegaTQ6401A","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["ATmegaTQ6401A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[2,"R1, R4","1k","R0805","RR-1K SMD","901-178",2]
[4,"R2, R101, R102, R103","10k","R0805","RR-10K SMD","901-003",2]
[1,"R3","#","R0805",null,null,2,"Osazuje se pouze při použití RC oscilátoru"]
["Keramické kondenzátory"]
[2,"C8, C9","15pF","C0805","CK-15P NPO","906-078",2,"Hodnota podle krystalu nebo RC oscilátoru"]
[3,"C101, C102, C103","10nF","C0805","CK-10N X7R","906-089",2,"Blokovací kondenzátor"]
[5,"C2, C3, C4, C5, C6","100nF","C0805","CK-100N X7R","906-096",2,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
[1,"C7","#100nF","C0805","CK-100N X7R","906-096",2,"Do not use with JTAG interface"]
["Elektrolytické kondenzátory"]
[1,"C1","22uF/6.3V","ELYTC","CTS 22M/6.3V C","907-032",null,"SMD elyt, velikost C"]
["Indukčnosti"]
[1,"L1","10uH","L1210","TL.10uH SMD","965-001",7.5,"SMD tlumivka"]
["Diody"]
[1,"D1","1N4007SMD","MELF","1N4007SMD","917-005",2,"Dioda 1A"]
["Integrované obvody"]
[1,"U1","Atmega64_128_TQ64","TQFP64_08","select","select",null,"Procesor ATMEL, vyberte si vhodný typ (například ATmega64-8AU)"]
["Krystaly"]
[1,"X1","8MHz","XTAL050/LG","Q 8MHZ","131-059",9.9,"Krystal dle potřeby a procesoru, možno i QM 8MHZ 131-073"]
[2,"X2, X3","#32768Hz","XTAL010/LG","Q 32.768KHZ","131-036",5,"Hodinkový krystal, osazuje se volitelně"]
["Mechanické součástky "]
[4,"J1-J16, J17-J32, J33-J48, J49-64","JUMP2x16","JUMP2x16","S2G80","832-033",14,"Dvouřadý hřebínek nalámat dle potřeby"]
[1,"J69","JUMP2","JUMP2","\""]
[3,"J65,J66,J67","JUMP2x3","JUMP2x3/B","\"",null,null,"Napájecí a ISP konektor, ISP konektor se osazuje jen jeden!"]
[1,"J68","JUMP2x5","JUMP2x5/B","S1G20","832-017",4,"JTAG ladicí konektor"]
[4,"J101+J103+J105, J102+J204+J106, J107+J109+J111, J108+J110+J112","JUMP3","JUMP3"]
[1,"SW1","P-B1720","PUSH050x050","P-B1720","630-008",3,"Obyčejné tlačítko 5x5mm"]
["Konstrukční součástky"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]