{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ATtinySO801B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ATtinySO801B","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["ATtinySO801B"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
["1","R2","100","R0805","R0805 100R","901-002",2]
["1","R1","10k","R0805","R0805 10K","901-003",2]
["Keramické kondenzátory"]
["1","C2","100nF","C0805","CK-100N X7R","906-096",2.5,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
["1","C3","#100nF","C0805","CK-100N X7R","906-096",2.5]
["Elektrolytické kondenzátory"]
["1","C1","10uF/6.3V","ELYTB","CTS 10M/6.3V B","907-109",3]
["Diody"]
["1","D1","1N4007SMD","MELF","1N4007SMD","917-005","1"]
["Integrované obvody"]
["1","U1","ATtiny","SO8_210",null,null,null,"Procesor dle potřeby v pouzdru SO8"]
["Mechanické součástky "]
["1","SW1","PUSH050x050","PUSH050x050","P-B1720","630-008","3","Malé tlačítko 5x5mm"]
["2","J1, J4","JUMP2x3","JUMP2x3/B","S2G26","832-025","5","Nalámat dle potřeby"]
["2","J2, J3","JUMP2X4","JUMP2X4/B","\""]
["Konstrukční součástky"]
[4,null,"Šroub M3x12",null,"Železářství",null,null,"Pozinkovaný křížový šroub M3x12 s válcovou hlavou"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Pozinkvaná podložka pro šroub M3"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026","2,5","Mosazný sloupek M3 výšky 5mm"]