{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["HT675101A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"HT675101A","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["HT675101A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[6,"R4, R5, R6, R10, R11, R12","100k","R0805","R0805 100K","901-001",2,"Osazuje se pokud se použije HT6751B"]
[6,"R1, R2, R3, R7, R8, R9","#100k","R0805","R0805 100K","901-001",2,"Osazuje se pokud se použije HT6751A"]
["Keramické kondenzátory"]
[4,"C1, C2, C4, C5","100nF","C0805","CK-100N X7R","906-096",2.5,"Běžný SMD kondenzátor"]
["Elektrolytické kondenzátory"]
[1,"C3","33uF/10V","ELYTC","CTS 33M/10V C","907-114",5.5,"Co největší SMD tantal na alespoň 6.3V ve velikosti C"]
["Diody"]
[2,"D1, D2","1N4007SMD","MELF","1N4007 SMD","917-005",1,"Běžná SMD dioda 1A"]
[1,"D3","BZV55C6.8SMD","MINIMELF","BZV55C6.8SMD","919-023",1,"Zenerova dioda 6.8V 0.5W"]
["Integrované obvody"]
[2,"U1, U2","HT6751B","SO8_150",null,null,77,"Dodá http://www.snailinstruments.com"]
["Mechanické součástky "]
[6,"J1-J6","JUMP2X3","JUMP2X3","S2G40","832-050",3.3,"Nalámat dle potřeby, cena za 1/6 hřebínku"]
["Konstrukční součástky"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]