{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Vstupní charakteristika","Závislost na napájení"],"not_rendered":{"charts":3,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Vstupní charakteristika","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["TTLPROBE01A"]
[]
["Vstupní charakteristika"]
[]
["Obvod PHILIPS 74HCT00"]
[]
["Vin","Iin"]
["[V]","[uA]"]
[0,-221]
[0.1]
[0.2,-196]
[0.3,-185]
[0.4,-171]
[0.5,-157]
[0.6,-145]
[0.7,-130]
[0.8,-116]
[0.9,-105]
[1,-91]
[1.1,-77]
[1.2,-64]
[1.3,-50]
[1.4,-38]
[1.5,-25]
[1.6,-11]
[1.7,1]
[1.8,14]
[1.9,27]
[2,40]
[2.1,54]
[2.2,66]
[2.3,79]
[2.4,92]
[2.5,105]
[2.6,118]
[2.7,130,null,null,null,"Vstupní odpor"]
[2.8,143]
[2.9,155,null,null,null,"Zin 1",7667.731629392971,"Ohm"]
[3,167,null,null,null,"Zin 2",14285.714285714286,"Ohm"]
[3.1,179]
[3.2,192]
[3.3,203]
[3.4,214]
[3.5,224]
[3.6,234]
[3.7,242]
[3.8,250]
[3.9,258]
[4,265]
[4.1,273]
[4.2,280]
[4.3,287]
[4.4,293]
[4.5,300]
[4.6,307]
[4.7,314]
[4.8,320]
[4.9,326]
[5,334]

{"sheet":"Závislost na napájení","index":1,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["TTLPROBE01A"]
[]
["Závislost rozhodovací úrovně na napájecím napětí"]
[]
["Obvod PHILIPS 74HCT00 - má hysterezi"]
[]
["Vcc","V lx low","V lx high","V xh low","V xh high"]
["[V]","[V]","[V]","[V]","[V]"]
[4,0.56,0.67,1.55,1.73]
[4.5,0.7,0.78,1.72,1.94]
[5,0.87,0.89,2,2.1]
[5.5,0.98,1,2.2,2.32]
[6,1.12,1.14,2.45,2.52]
[]
[]
[]
[]
["Obvod ST 74HCT00 - nemá hysterezi"]
[]
["Vcc","V lx low","V lx high","V xh low","V xh high"]
["[V]","[V]","[V]","[V]","[V]"]
[4,0.55,0.59,1.59,1.64]
[4.5,0.66,0.7,1.75,1.82]
[5,0.76,0.8,1.93,2]
[5.5,0.86,0.9,2.1,2.2]
[6,0.95,1,2.25,2.34]