{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PIC16F84DIL1801A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PIC16F84DIL1801A","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PIC16F84DIL1801A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[4,"R1,R3,R4,R5","10k","R0805","RR-10K SMD","901-003",1,"SMD Odpor"]
[1,"R2",100,"R0805","RR-100R SMD","901-002",1,"SMD Odpor"]
["Kondenzátory"]
[2,"C3,C4","22pF","C0805","CK-22P NPO","906-079",2,"SMD kondenzátor"]
[3,"C5,C6,C7","10nF","C0805","CK-10N X7R","906-089",2,"SMD kondenzátor"]
[1,"C1","100nF","C0805","CK-100N Z5U","906-110",2,"SMD kondenzátor"]
[1,"C2","10uF/6.3V","ELYTB","CTS 10M/6.3V B","907-109",4,"SMD elektrolyt, velikost B"]
["Polovodiče"]
[1,"D1","1N4004","DO41","1N4007","220-002",1,"Dioda 1A"]
[1,"U1","PIC16F84","DIP18_300","PIC16F84A-04/P","434-121",92,"Procesor PIC v pouzdru DIL18 dle potřeby"]
["Krystaly"]
[1,"X1","XTAL050/LG","XTAL050/LG","Q 4MHz","131-045",9.9,"Krystal standardní (HC18/HC49U), možno použít i miniaturní (HC49U/S)"]
["Mechanické součástky"]
[1,"SW1","PUSH050x050","PUSH050x050","P-B1720","630-008",3,"Tlačítko 5x5mm"]
[4,"J22+J24+J26,J23+J25+J27,J28+J30+J32,J29+J31+J33","JUMP3","JUMP3","S1G20","832-017",4,"Jumper jednořadý 3 piny, lámou se dle potřeby"]
[1,"J21","PIC_ISP","PIC_ISP","\"",null,null,"Programovací jumper 6 pinů, 1 pin odstraněn, lámou se dle potřeby"]
[2,"J1+J2+J3+J4+J5+J6+J7+J8+J9,J10+J11+J12+J13+J14+J15+J16+J17+J18","JUMP 2X9","JUMP 2X9","S2G20","832-023",4,"Jumper dvouřadý 2x9 pinů, lámou se dle potřeby"]
[1,"J20+J19","JUMP2X3","JUMP2X3","\"",null,null,"Jumper dvouřadý 2x3 piny, lámou se dle potřeby"]
["Konstrukční součástky"]
[4,null,"Šroub M3x12, křížový, válcová hlava",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]
[1,null,"SOKL DIL18",null,"SOKL 18","823-003",1.9,"Patice na procesor DIL18"]