{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PIC16F87XDIL2801A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PIC16F87XDIL2801A","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PIC16F87XDIL2801A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R2",100,"R0805","RR-100R SMD","901-002",1,"SMD Odpor"]
[6,"R1,R3,R4,R5,R6,R7","10k","R0805","RR-10K SMD","901-003",1,"SMD Odpor"]
["Keramické kondenzátory"]
[2,"C5,C6","22pF","C0805","CK-22P NPO","906-079",2,"SMD kondenzátor"]
[2,"C7,C8","33pF","C0805","CK-33P NPO","906-080",2,"SMD kondenzátor"]
[5,"C3,C4,C9,C10,C11","10nF","C0805","CK-10N X7R","906-089",2,"SMD kondenzátor"]
[1,"C1","100nF","C0805","CK-100N Z5U","906-110",2,"SMD kondenzátor"]
["Tantalové kondenzátory"]
[1,"C2","10uF/6.3V","ELYTB","CTS 10M/6.3V B","907-109",4,"SMD tantal 10M na min. 6.3V, velikost B"]
["Diody"]
[1,"D1","1N4007","DO41","1N4007","220-002",1,"Dioda 1A"]
["Integrované obvody"]
[1,"U1","PIC16F873A/SO","SO28_300",null,null,null,"Procesor dle aktuální potřeby"]
["Krystaly"]
[1,"X2","32768Hz","XTAL010/LG","Q 32.768KHZ","131-036",5,"Krystal válcový"]
[1,"X1","4.0MHz","XTAL050/LG","Q 4MHz","131-045",9.9,"Krystal standardní (HC18/HC49U), možno použít i miniaturní (HC49U/S)"]
["Mechanické součástky"]
[1,"SW1","P-B1720","PUSH050x050","P-B1720","630-008",3,"Tlačítko 5x5mm"]
[1,"J38","JUMP2","UNIPAD2","S1G20","832-017",4,"Jumper jednořadý 2 piny, láme se dle potřeby"]
[4,"J39+J41+J43, J40+J42+J44, J45+J47+J49, J46+J48+J50","JUMP3","UNIPAD3","\"","\"","\"","Jumper jednořadý 3 piny, láme se dle potřeby"]
[1,"J29","PIC_ISP (JUMP6)","PIC_ISP","\"","\"","\"","Jumper jednořadý, 6 pinů, láme se dle potřeby"]
[2,"J34+J35,J36+J37","JUMP2X2","UNIPAD2X2","S2G20","832-023",4,"Jumper dvouřadý, láme se dle potřeby"]
[1,"J51+J52","JUMP2x3","UNIPAD2X3","\"","\"","\"","Jumper dvouřadý, láme se dle potřeby"]
[1,"J30+J31+J32+J33","JUMP2X4","UNIPAD2X4","\"","\"","\"","Jumper dvouřadý, láme se dle potřeby"]
[2,"J1-J14,J15-J28","JUMP2X14","UNIPAD2X14","\"","\"","\"","Jumper dvouřadý, láme se dle potřeby"]
["Konstrukční součásti"]
[4,null,"Šroub M3x12, křížový, válcová hlava",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]