{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PIC16F87xTQ4401A "],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PIC16F87xTQ4401A ","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PIC16F87xTQ4401A "]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R2","100","R0805",null,null,null,"SMD odpor"]
[6,"R1, R3, R4, R5, R6, R7","10k","R0805",null,null,null,"SMD odpor"]
["Keramické kondenzátory"]
[2,"C6, C7","22pF","C0805",null,null,null,"Kondenzátor ke krystalu"]
[2,"C8, C9","33pF","C0805",null,null,null,"Kondenzátor ke krystalu"]
[5,"C4, C5, C10, C11, C12","10nF","C0805",null,null,null,"Pomocné kondenzátory"]
[2,"C1, C2","100nF","C0805",null,null,null,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
["Elektrolytické kondenzátory"]
[1,"C3","10uF/6.3V","ELYTB",null,null,null,"Blokovací elyt, na hodnotě nezáleží, velikost B"]
["Diody"]
[1,"D1","1N4007","DO41",null,null,null,"Ochranná dioda, obyčejná, 1A"]
["Integrované obvody"]
[1,"U1","PIC16F877A/PT","TQFP44",null,null,null,"Procesor v pouzdru TQFP44"]
["Krystaly"]
[1,"X1","4.0MHz","XTAL050/LG",null,null,null,"Hlavní krystal, zvolte vhodou frekvenci"]
[1,"X2","32768Hz","XTAL010/LG",null,null,null,"Hodinový krystal (volitelně)"]
["Mechanické součástky"]
[9,"J47, J48, J49, J50, J51, J52, J53, J54, J55","JUMP2","UNIPAD2",null,null,null,"Jednořadé hřebínky, nalámat"]
[1,"J46","JUMP6","PIC_ISP",null,null,null,"Jednořadé hřebínky, nalámat"]
[4,"J56+J58+J60, J57+J59+J61, J62+J64+J66, J63+J65+J67","JUMP3","UNIPAD1",null,null,null,"Jednořadé hřebínky, nalámat"]
[4,"J1-J11, J12-J22, J23-J33, J34-J44","JUMP2x11","UNIPAD2",null,null,null,"Dvouřadé hřebínky, nalámat"]
[1,"J45","JUMP2X3","JUMP2X3",null,null,null,"Dvouřadé hřebínky, nalámat"]
[1,"SW1","P-B1720","PUSH050x050",null,null,null,"Tlačítko RESET"]
["Konstrukční součástky"]
[4,"Šroub M3x12",{"$nulls":5},"Pozinkovaný, válcová hlava, křížový"]
[4,"Podložka M3",{"$nulls":5},"Pozinkovaná"]
[4,"Sloupek M3x5",{"$nulls":5},"Sloupek matička, možno nahradit dvěma maticemi M3"]