{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PIC18F8x2001A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PIC18F8x2001A","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PIC18F8x2001A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R2",100,"R0805","RR-100R SMD","901-002",1,"SMD Odpor"]
[4,"R1,R5,R6,R7","10k","R0805","RR-10K SMD","901-003",1,"SMD Odpor"]
["Kondenzátory"]
[2,"C6,C7","22pF","C0805","CK-22P NPO","906-079",2,"SMD kondenzátor"]
[2,"C8,C9","33pF","C0805"]
[3,"C10,C11,C12","10nF","C0805","CK-10N X7R","906-089",2,"SMD kondenzátor"]
[5,"C1,C2,C3,C4,C5","100nF","C0805","CK-100N Z5U","906-110",2,"SMD kondenzátor"]
["Diody"]
[1,"D1","1N4004","DO41","1N4007","220-002",1,"Dioda 1A"]
["Integrované obvody"]
[1,"U1","PIC18F8720","TQFP80","PIC18F8720-I/PT","MES PRAHA",null,"Procesor dle potřeby"]
["Krystaly"]
[1,"X1","6.0MHz","XTAL050/LG","Q 6MHz","131-053",9.9,"Krystal standardní (HC18/HC49U), možno použít i miniaturní (HC49U/S)"]
[1,"X2","32768Hz","XTAL010/LG","Q 32.768KHZ","131-036",5,"Krystal hodinkový (d3x8mm)"]
["Mechanické součásti"]
[1,"SW1","P-B1720","PUSH050x050","P-B1720","630-008",3,"Tlačítko 5x5mm"]
[1,"J103","PIC_ISP","PIC_ISP","S1G20","832-017",4,"Jumper jednořadý 6 pinů, lámou se dle potřeby"]
[4,"J106+J108+J110, J107+J109+J111, J112+J114+J116, J113+J115+J117","JUMP3","UNIPAD3","\"","\"","\"","Jumper jednořadý 3 piny, lámou se dle potřeby"]
[1,"J104+J105","JUMP2X1","JUMP2X1","S2G20","832-023",4,"Jumper dvouřadý 2x10 pinů, lamou se dle potřeby"]
[1,"J101+J102","JUMP2X3","JUMP2X3","\"","\"","\"","\""]
[4,"J1-J20, J21-J40, J41-J60, J61-J80","JUMP2X20","UNIPAD2X20","S2G40","832-050",8,"Jumper dvouřadý 2x20 pinů"]
["Konstrukční součásti"]
[4,null,"Šroub M3x12, křížový, válcová hlava",null,"Železářství",null,null,"Šroub M3x12, válcová hlava, křížový"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka M3"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Sloupek M3x5mm"]
[3,null,"Pin z precizní patice",null,"DIL08PZ","824-002",3.9,"3 piny z precizního soklu jako patice pro krystal X1"]