{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PICPGR301A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PICPGR301A","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PICPGR301A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[4,"R9,R10,R11,R12",100,"RL090","RR 100R","110-049",0.8,"Miniaturní odpor"]
[2,"R4,R13",470,"RL090","RR 470R","110-065",0.8,"Miniaturní odpor"]
[6,"R1,R2,R3,R5,R6,R7","1k","RL090","RR 1K","110-073",0.8,"Miniaturní odpor"]
[4,"R8,R14,R15,R16","4k7","RL090","RR 4K7","110-089",0.8,"Miniaturní odpor"]
["Kondenzátory"]
[4,"C2,C3,C5,C6","M1","CK050","CK100N/63V","120-060",1,"Keramický kondenzátor"]
[1,"C4","10uF/35V","CE020X5","E10M/35V","123-053",1,"Elektrolyt"]
[1,"C1","220uF/25V","CE035X8","E220M/25V","123-137",1.5,"Elektrolyt"]
["Diody"]
[1,"D1","1N4007","DO41","1N4007","220-002",1,"Dioda 1A"]
[1,"D2","1N4148","DO35","1N4148","220-003",1,"Malá Si dioda"]
[1,"D3","LED3mm, zelená","LED3","L-HLMP-1700","511-021",5.5,"LED průměr 3mm, nízkoproudová"]
[1,"D4","LED3mm, červená","LED3","L-HLMP-1790","511-024",4,"LED průměr 3mm, nízkoproudová"]
[1,"D5","BZX85V006.2","DO41","BZX85V006.2","222-020",1,"Zenerova dioda 6.2V"]
["Tranzistory"]
[3,"Q1,Q3,Q5","BC337","TO92/B","BC337-25","210-018",1.5,"Tranzistor NPN"]
[2,"Q2,Q4","BC640","TO92/B","BC640","210-109",3,"Tranzistor PNP"]
["Integrované obvody"]
[1,"U1","LM7805T","TO220/L",7805,"330-001",8,"Stabilizátor +5V/1A"]
[1,"U2","LM78L12Z","TO92/B","78L12","330-016",6,"Stabilizátor +12V/0.1A"]
[1,"U3","GAL16V8","DIP20_300",null,null,null,"Obvod GAL, nutno naprogramovat obsah"]
["Mechanické součásti"]
[1,"J1","K375A","K375A","K375A","806-049",8,"Napájecí konektor souosý"]
[1,"J2","DB25F_90","DB25F_90","CAN 25 Z 90","801-021",12,"Cannon konektor DB25 samička do plošného spoje"]
[1,"J3","JUMP3","JUMP3","S1G20","832-017",4,"Propojka 3x1 pin, láme se"]
[1,"J4","PIC_ISP","PIC_ISP","\"",null,null,"Propojka 6x1 pin s vynechaným pinem 4, láme se"]
[1,"J5","JUMP2","JUMP2","\"",null,null,"Propojka 2x1 pin, láme se"]
[1,"SW1","P-B143","P-B143","P-B143","631-141",5.1,"Šoupací přepínač"]
["Konstrukční součásti"]
[1,null,"Patice DIL 20 obyčejná",null,"SOKL 20","823-004",2.1,"Patice obyčejná DIL 20"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]