{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PICICD01A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PICICD01A","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PICICD01A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory SMD"]
["1","R18",33,"R0805","RR-33R SMD","901-085",1]
["9","R2,R3,R4,R5,R6,R7,R8,R12,R21",100,"R0805","RR-100R SMD","901-002",1]
["4","R13,R28,R30,R32",330,"R0805","RR-330R SMD","901-083",1]
["3","R9,R10,R23","1k","R0805","RR-1K SMD","901-029",1]
["2","R22,R25","4k7","R0805","RR-4K7 SMD","901-115",1]
["12","R11,R14,R15,R16,R17,R19,R20,R24,R26,R27,R29,R31","10k","R0805","RR-10K SMD","901-003",1]
["1","R1","22K","R0805","RR-22K SMD","901-056",1]
["Kondenzátory keramické SMD"]
["2","C2,C3","22pF","C0805","CK-22P NPO","906-079",2]
["10","C1,C4,C5,C6,C7,C8,C9,C10,C12,C13","100nF","C0805","CK-100N X7R","906-096",2,"Libovolná hmota"]
["Kondenzátory elektrolytické drátové"]
["2","C11,C14","47uF/25V","CE020X5","E47M/25V","123-094",1]
["Tlumivky axální"]
["1","L1","330uH","LL120","TL.330uH","611-031",6,"Tlumivka axiální"]
["Krystaly"]
["1","X1","3.6864MHz","XTAL050","Q 3.6864MHZ","131-101",9.9,"Nízkoprofilový, možno i standardní velikost"]
["Diody SMD"]
["6","D1,D2,D4,D6,D7,D9","1N4148SMD","SOD87","1N4148SMD","917-001",2,"Signálová dioda"]
["1","D5","BAT48SMD","SOD87","BAT48SMD","920-007",4.5,"Schottkyho dioda"]
["1","D10","BZV55C5.6SMD","MINIMELF","BZV55C5.6SMD","919-010",1.3,"Zenerova dioda 5.6V"]
["1","D3","BZV55C16SMD","MINIMELF","BZV55C16SMD","919-068",1.3,"Zenerova dioda 16V"]
["Diody LED"]
["1","D8","LED3mm","LED3","L-HLMP-1790","511-024",4,"LED Červená"]
["Tranzistory SMD"]
["3","Q1,Q2,Q4","BC817-25SMD","SOT23","BC817-25SMD","912-006",1.5,"NPN tranzistor 0.5A"]
["1","Q3","BC807-25SMD","SOT23","BC807-25SMD","912-002",1.5,"PNP tranzistor 0.5A"]
["Integrované obvody"]
["1","U1","PIC16LF876-04/SO","SO28_300","PIC16LF876-04/SO","967-109",300,"Procesor PIC"]
["1","U2","MAX232SMD","SO16_150","MAX232SMD",null,null,"Převodník pro RS232, úzké SO pouzdro"]
["1","U3","LM78L12M_SO8","SO8_150","78L12 SMD","934-002",10,"Stabilizátor 12V 100mA SMD SO8"]
["Mechanické součástky"]
["1","J1","RS232DB9M","DB9M_90",null,null,null,"Cannon konektor samička do plošných spojů"]
["2","J2,J3","PIC_ISP_ICD","JUMP8","S1G20","832-017",4,"Lámecí hřebínek jednořadý"]
["Konstrukční součásti"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]