{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["VZOR"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"VZOR","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Power SW"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
[5,"D1 - D5","1N5818","DO41",null,null,"co dům dá","Libovolná spínací nebo shottkiho dioda"]
[1,"J1","JUMP2X1","JUMP2X1"]
[1,"J2","JUMP2X4","JUMP2X4"]
[4,"J3 - J6","ARK210/2","ARK210/2",null,null,2.5]
[2,"Q1, Q2","SO8_2xNFET_9926","SO8_2FET",null,null,14,"Dvojitý NFET s nízkým threshodl (např CEM9926 nebo IRF7301)"]
[4,"R1 - R4",47,"R0805"]
[4,"M1 - M4","HOLE_M3","HOLE_M3",null,null,null,"Šroubky, podložky a matičky jako u každého modulu"]