{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["NFET2X01A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"NFET2X01A","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["NFET2X01A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[4,"R1, R3","100","R0805","R0805 100R","901-212",0.39,"Na toleranci nezáleží"]
[4,"R2, R4","100k","R0805","R0805 100K","901-172",0.39,"Na toleranci nezáleží"]
["Keramické kondenzátory"]
[2,"C1, C2","100nF","C0805","CK-100N X7R","906-096",2.5,"Blokovací kondenzátor, může být i Y5V nebo Z5U"]
["Elektrolytické kondenzátory"]
[1,"C3","470M/35V","CE050X10","E470M/35V","123-159",4]
["Diody"]
[2,"D1, D3","BAT43SMD","SOD87","BAT43 SMD","920-021",3]
[2,"D2, D4","1N5818","DO41","1N5818","223-055",2]
["Tranzistory"]
[2,"Q1, Q2","AP60N03S","TO263_3",null,null,null,"Tranzistory z mainboardu (N-FET 30V/30A)"]
["Mechanické součástky "]
[2,"J1, J3","JUMP2X2","JUMP2X2","S2G80","832-033",14]
[1,"J5","JUMP2X4","JUMP2X4","\"","\""]
[2,"J6, J7","JUMP3","JUMP3","S1G40","832-021",8]
[2,"J2, J4","ARK210/2","ARK210/2","ARK210/2","821-003",7]
["Konstrukční součástky"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]