(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 352)
    (no_connects 0)
    (area 103.119943 46.868 198.690954 132.008)
    (thickness 1.6)
    (drawings 124)
    (tracks 1549)
    (zones 0)
    (modules 162)
    (nets 128)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 0.5 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.70002 2.70002)
    (pad_drill 2.30124)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 81.28 152.4)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C10-Pad1)")
  (net 3 "Net-(C18-Pad1)")
  (net 4 "Net-(C27-Pad1)")
  (net 5 "Net-(C28-Pad1)")
  (net 6 +5V)
  (net 7 "Net-(J33-Pad2)")
  (net 8 "Net-(J33-Pad3)")
  (net 9 "Net-(CON1-Pad6)")
  (net 10 "Net-(R4-Pad1)")
  (net 11 "Net-(R5-Pad1)")
  (net 12 "Net-(J41-Pad1)")
  (net 13 3V3)
  (net 14 "Net-(CON1-Pad1)")
  (net 15 "Net-(CON1-Pad3)")
  (net 16 "Net-(CON1-Pad5)")
  (net 17 "Net-(CON1-Pad9)")
  (net 18 "Net-(F1-Pad1)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "Net-(J2-Pad1)")
  (net 21 "Net-(J3-Pad1)")
  (net 22 "Net-(J4-Pad1)")
  (net 23 "Net-(J5-Pad1)")
  (net 24 "Net-(J6-Pad1)")
  (net 25 "Net-(J7-Pad1)")
  (net 26 "Net-(J8-Pad1)")
  (net 27 "Net-(J9-Pad1)")
  (net 28 "Net-(J10-Pad1)")
  (net 29 "Net-(J11-Pad1)")
  (net 30 "Net-(J12-Pad1)")
  (net 31 "Net-(J13-Pad1)")
  (net 32 "Net-(J14-Pad1)")
  (net 33 "Net-(J15-Pad1)")
  (net 34 "Net-(J16-Pad1)")
  (net 35 "Net-(J17-Pad1)")
  (net 36 "Net-(J18-Pad1)")
  (net 37 "Net-(J19-Pad1)")
  (net 38 "Net-(J20-Pad1)")
  (net 39 "Net-(J21-Pad1)")
  (net 40 "Net-(J22-Pad1)")
  (net 41 "Net-(J23-Pad1)")
  (net 42 "Net-(J24-Pad1)")
  (net 43 "Net-(J25-Pad1)")
  (net 44 "Net-(J26-Pad1)")
  (net 45 "Net-(J27-Pad1)")
  (net 46 "Net-(J28-Pad1)")
  (net 47 "Net-(J29-Pad1)")
  (net 48 "Net-(J30-Pad1)")
  (net 49 "Net-(J31-Pad1)")
  (net 50 "Net-(J32-Pad1)")
  (net 51 "Net-(J33-Pad1)")
  (net 52 "Net-(J34-Pad1)")
  (net 53 "Net-(J35-Pad1)")
  (net 54 "Net-(J38-Pad1)")
  (net 55 "Net-(J39-Pad1)")
  (net 56 "Net-(J40-Pad1)")
  (net 57 "Net-(J42-Pad1)")
  (net 58 "Net-(J43-Pad1)")
  (net 59 "Net-(J44-Pad1)")
  (net 60 "Net-(J45-Pad1)")
  (net 61 "Net-(J46-Pad1)")
  (net 62 "Net-(J47-Pad1)")
  (net 63 "Net-(J48-Pad1)")
  (net 64 "Net-(J49-Pad1)")
  (net 65 "Net-(J50-Pad1)")
  (net 66 "Net-(J51-Pad1)")
  (net 67 "Net-(J52-Pad1)")
  (net 68 "Net-(J53-Pad1)")
  (net 69 "Net-(J54-Pad1)")
  (net 70 "Net-(J55-Pad1)")
  (net 71 "Net-(J56-Pad1)")
  (net 72 "Net-(J57-Pad1)")
  (net 73 "Net-(J58-Pad1)")
  (net 74 "Net-(J59-Pad1)")
  (net 75 "Net-(J60-Pad1)")
  (net 76 "Net-(J61-Pad1)")
  (net 77 "Net-(J62-Pad1)")
  (net 78 "Net-(J63-Pad1)")
  (net 79 "Net-(J64-Pad1)")
  (net 80 "Net-(J65-Pad1)")
  (net 81 "Net-(J66-Pad1)")
  (net 82 "Net-(J67-Pad1)")
  (net 83 "Net-(J68-Pad1)")
  (net 84 "Net-(J69-Pad1)")
  (net 85 "Net-(J70-Pad1)")
  (net 86 "Net-(J71-Pad1)")
  (net 87 "Net-(J72-Pad1)")
  (net 88 "Net-(J73-Pad1)")
  (net 89 "Net-(J74-Pad1)")
  (net 90 "Net-(J75-Pad1)")
  (net 91 "Net-(J76-Pad1)")
  (net 92 "Net-(J77-Pad1)")
  (net 93 "Net-(J78-Pad1)")
  (net 94 "Net-(J79-Pad1)")
  (net 95 "Net-(J80-Pad1)")
  (net 96 "Net-(J81-Pad1)")
  (net 97 "Net-(J82-Pad1)")
  (net 98 "Net-(J83-Pad1)")
  (net 99 "Net-(J84-Pad1)")
  (net 100 "Net-(J85-Pad1)")
  (net 101 "Net-(J86-Pad1)")
  (net 102 "Net-(J87-Pad1)")
  (net 103 "Net-(J88-Pad1)")
  (net 104 "Net-(J89-Pad1)")
  (net 105 "Net-(J90-Pad1)")
  (net 106 "Net-(J91-Pad1)")
  (net 107 "Net-(J92-Pad1)")
  (net 108 "Net-(J93-Pad1)")
  (net 109 "Net-(J94-Pad1)")
  (net 110 "Net-(J95-Pad1)")
  (net 111 "Net-(J96-Pad1)")
  (net 112 "Net-(J97-Pad1)")
  (net 113 "Net-(J98-Pad1)")
  (net 114 "Net-(J99-Pad1)")
  (net 115 "Net-(J100-Pad1)")
  (net 116 "Net-(J101-Pad1)")
  (net 117 "Net-(J102-Pad1)")
  (net 118 "Net-(J103-Pad1)")
  (net 119 "Net-(J104-Pad1)")
  (net 120 "Net-(J105-Pad1)")
  (net 121 "Net-(J106-Pad1)")
  (net 122 "Net-(J107-Pad1)")
  (net 123 "Net-(J108-Pad1)")
  (net 124 "Net-(J109-Pad1)")
  (net 125 "Net-(J110-Pad1)")
  (net 126 "Net-(J111-Pad1)")
  (net 127 "Net-(C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(CON1-Pad6)")
    (add_net "Net-(CON1-Pad9)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J100-Pad1)")
    (add_net "Net-(J101-Pad1)")
    (add_net "Net-(J102-Pad1)")
    (add_net "Net-(J103-Pad1)")
    (add_net "Net-(J104-Pad1)")
    (add_net "Net-(J105-Pad1)")
    (add_net "Net-(J106-Pad1)")
    (add_net "Net-(J107-Pad1)")
    (add_net "Net-(J108-Pad1)")
    (add_net "Net-(J109-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J110-Pad1)")
    (add_net "Net-(J111-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J22-Pad1)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J25-Pad1)")
    (add_net "Net-(J26-Pad1)")
    (add_net "Net-(J27-Pad1)")
    (add_net "Net-(J28-Pad1)")
    (add_net "Net-(J29-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J30-Pad1)")
    (add_net "Net-(J31-Pad1)")
    (add_net "Net-(J32-Pad1)")
    (add_net "Net-(J33-Pad1)")
    (add_net "Net-(J33-Pad2)")
    (add_net "Net-(J33-Pad3)")
    (add_net "Net-(J34-Pad1)")
    (add_net "Net-(J35-Pad1)")
    (add_net "Net-(J38-Pad1)")
    (add_net "Net-(J39-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J40-Pad1)")
    (add_net "Net-(J41-Pad1)")
    (add_net "Net-(J42-Pad1)")
    (add_net "Net-(J43-Pad1)")
    (add_net "Net-(J44-Pad1)")
    (add_net "Net-(J45-Pad1)")
    (add_net "Net-(J46-Pad1)")
    (add_net "Net-(J47-Pad1)")
    (add_net "Net-(J48-Pad1)")
    (add_net "Net-(J49-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J50-Pad1)")
    (add_net "Net-(J51-Pad1)")
    (add_net "Net-(J52-Pad1)")
    (add_net "Net-(J53-Pad1)")
    (add_net "Net-(J54-Pad1)")
    (add_net "Net-(J55-Pad1)")
    (add_net "Net-(J56-Pad1)")
    (add_net "Net-(J57-Pad1)")
    (add_net "Net-(J58-Pad1)")
    (add_net "Net-(J59-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J60-Pad1)")
    (add_net "Net-(J61-Pad1)")
    (add_net "Net-(J62-Pad1)")
    (add_net "Net-(J63-Pad1)")
    (add_net "Net-(J64-Pad1)")
    (add_net "Net-(J65-Pad1)")
    (add_net "Net-(J66-Pad1)")
    (add_net "Net-(J67-Pad1)")
    (add_net "Net-(J68-Pad1)")
    (add_net "Net-(J69-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J70-Pad1)")
    (add_net "Net-(J71-Pad1)")
    (add_net "Net-(J72-Pad1)")
    (add_net "Net-(J73-Pad1)")
    (add_net "Net-(J74-Pad1)")
    (add_net "Net-(J75-Pad1)")
    (add_net "Net-(J76-Pad1)")
    (add_net "Net-(J77-Pad1)")
    (add_net "Net-(J78-Pad1)")
    (add_net "Net-(J79-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J80-Pad1)")
    (add_net "Net-(J81-Pad1)")
    (add_net "Net-(J82-Pad1)")
    (add_net "Net-(J83-Pad1)")
    (add_net "Net-(J84-Pad1)")
    (add_net "Net-(J85-Pad1)")
    (add_net "Net-(J86-Pad1)")
    (add_net "Net-(J87-Pad1)")
    (add_net "Net-(J88-Pad1)")
    (add_net "Net-(J89-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J90-Pad1)")
    (add_net "Net-(J91-Pad1)")
    (add_net "Net-(J92-Pad1)")
    (add_net "Net-(J93-Pad1)")
    (add_net "Net-(J94-Pad1)")
    (add_net "Net-(J95-Pad1)")
    (add_net "Net-(J96-Pad1)")
    (add_net "Net-(J97-Pad1)")
    (add_net "Net-(J98-Pad1)")
    (add_net "Net-(J99-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net 3V3)
    (add_net GND)
  )
  (module SMD_Packages:TQFP144 placed (layer B.Cu) (tedit 53B886C5)
    (at 147.574 88.9)
    (attr smd)
    (fp_text reference U1 (at 0 1.905) (layer B.SilkS))
    (fp_text value AT32UC3A3 (at 0 -1.905) (layer B.SilkS))
    (pad 1 smd rect (at 8.7503 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 8.2423 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 3 smd rect (at 7.747 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C18-Pad1)"))
    (pad 4 smd rect (at 7.2517 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 6.7437 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J33-Pad2)"))
    (pad 6 smd rect (at 6.2484 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J33-Pad3)"))
    (pad 7 smd rect (at 5.7531 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 5.2451 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 9 smd rect (at 4.7498 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 10 smd rect (at 4.2545 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 11 smd rect (at 3.7465 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(J43-Pad1)"))
    (pad 12 smd rect (at 3.2512 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(J34-Pad1)"))
    (pad 13 smd rect (at 2.7559 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(J35-Pad1)"))
    (pad 14 smd rect (at 2.2479 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (pad 15 smd rect (at 1.7526 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(J30-Pad1)"))
    (pad 16 smd rect (at 1.2573 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J41-Pad1)"))
    (pad 17 smd rect (at 0.7493 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(J42-Pad1)"))
    (pad 18 smd rect (at 0.254 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C28-Pad1)"))
    (pad 19 smd rect (at -0.254 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C27-Pad1)"))
    (pad 20 smd rect (at -0.7493 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -1.2573 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 22 smd rect (at -1.7526 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(J47-Pad1)"))
    (pad 23 smd rect (at -2.2479 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (pad 24 smd rect (at -2.7559 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(J48-Pad1)"))
    (pad 25 smd rect (at -3.2512 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(J49-Pad1)"))
    (pad 26 smd rect (at -3.7465 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J5-Pad1)"))
    (pad 27 smd rect (at -4.2545 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(J50-Pad1)"))
    (pad 28 smd rect (at -4.7498 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 29 smd rect (at -5.2451 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (pad 30 smd rect (at -5.7531 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(J51-Pad1)"))
    (pad 31 smd rect (at -6.2484 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(J40-Pad1)"))
    (pad 32 smd rect (at -6.7437 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(J68-Pad1)"))
    (pad 33 smd rect (at -7.2517 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(J65-Pad1)"))
    (pad 34 smd rect (at -7.747 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(J64-Pad1)"))
    (pad 35 smd rect (at -8.2423 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(J71-Pad1)"))
    (pad 36 smd rect (at -8.7503 10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(J92-Pad1)"))
    (pad 66 smd rect (at -10.9855 -5.7531) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(J96-Pad1)"))
    (pad 67 smd rect (at -10.9855 -6.2484) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(J63-Pad1)"))
    (pad 68 smd rect (at -10.9855 -6.7437) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(J66-Pad1)"))
    (pad 69 smd rect (at -10.9855 -7.2517) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(J94-Pad1)"))
    (pad 70 smd rect (at -10.9855 -7.747) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(J97-Pad1)"))
    (pad 71 smd rect (at -10.9855 -8.2423) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(J93-Pad1)"))
    (pad 72 smd rect (at -10.9855 -8.7503) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(J74-Pad1)"))
    (pad 114 smd rect (at 10.9855 -6.2484) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J13-Pad1)"))
    (pad 115 smd rect (at 10.9855 -5.7531) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J14-Pad1)"))
    (pad 116 smd rect (at 10.9855 -5.2451) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J15-Pad1)"))
    (pad 117 smd rect (at 10.9855 -4.7498) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 118 smd rect (at 10.9855 -4.2545) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 119 smd rect (at 10.9855 -3.7465) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J7-Pad1)"))
    (pad 120 smd rect (at 10.9855 -3.2512) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J6-Pad1)"))
    (pad 121 smd rect (at 10.9855 -2.7559) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(J46-Pad1)"))
    (pad 122 smd rect (at 10.9855 -2.2479) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J32-Pad1)"))
    (pad 123 smd rect (at 10.9855 -1.7526) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J31-Pad1)"))
    (pad 124 smd rect (at 10.9855 -1.2573) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(J27-Pad1)"))
    (pad 125 smd rect (at 10.9855 -0.7493) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(J29-Pad1)"))
    (pad 126 smd rect (at 10.9855 -0.254) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(J28-Pad1)"))
    (pad 127 smd rect (at 10.9855 0.254) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J26-Pad1)"))
    (pad 128 smd rect (at 10.9855 0.7493) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J16-Pad1)"))
    (pad 129 smd rect (at 10.9855 1.2573) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J19-Pad1)"))
    (pad 130 smd rect (at 10.9855 1.7526) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 131 smd rect (at 10.9855 2.2479) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 132 smd rect (at 10.9855 2.7559) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J20-Pad1)"))
    (pad 133 smd rect (at 10.9855 3.2512) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J25-Pad1)"))
    (pad 134 smd rect (at 10.9855 3.7465) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(J45-Pad1)"))
    (pad 135 smd rect (at 10.9855 4.2545) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J44-Pad1)"))
    (pad 136 smd rect (at 10.9855 4.7498) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J21-Pad1)"))
    (pad 137 smd rect (at 10.9855 5.2451) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J24-Pad1)"))
    (pad 138 smd rect (at 10.9855 5.7531) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J22-Pad1)"))
    (pad 139 smd rect (at 10.9855 6.2484) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J23-Pad1)"))
    (pad 140 smd rect (at 10.9855 6.7437) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 141 smd rect (at 10.9855 7.2517) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 142 smd rect (at 10.9855 7.747) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 143 smd rect (at 10.9855 8.2423) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 144 smd rect (at 10.9855 8.7503) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -10.9855 8.7503) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(J62-Pad1)"))
    (pad 38 smd rect (at -10.9855 8.2423) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(J87-Pad1)"))
    (pad 39 smd rect (at -10.9855 7.747) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(J99-Pad1)"))
    (pad 40 smd rect (at -10.9855 7.2517) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(J67-Pad1)"))
    (pad 41 smd rect (at -10.9855 6.7437) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(J100-Pad1)"))
    (pad 42 smd rect (at -10.9855 6.2484) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(J105-Pad1)"))
    (pad 43 smd rect (at -10.9855 5.7531) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(J101-Pad1)"))
    (pad 44 smd rect (at -10.9855 5.2451) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(J88-Pad1)"))
    (pad 45 smd rect (at -10.9855 4.7498) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(J89-Pad1)"))
    (pad 46 smd rect (at -10.9855 4.2545) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(J106-Pad1)"))
    (pad 47 smd rect (at -10.9855 3.7465) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -10.9855 3.2512) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 49 smd rect (at -10.9855 2.7559) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J61-Pad1)"))
    (pad 50 smd rect (at -10.9855 2.2479) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(J60-Pad1)"))
    (pad 51 smd rect (at -10.9855 1.7526) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(J90-Pad1)"))
    (pad 52 smd rect (at -10.9855 1.2573) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(J91-Pad1)"))
    (pad 53 smd rect (at -10.9855 0.7493) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(J58-Pad1)"))
    (pad 54 smd rect (at -10.9855 0.254) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(J59-Pad1)"))
    (pad 55 smd rect (at -10.9855 -0.254) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(J52-Pad1)"))
    (pad 56 smd rect (at -10.9855 -0.7493) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(J111-Pad1)"))
    (pad 57 smd rect (at -10.9855 -1.2573) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(J110-Pad1)"))
    (pad 58 smd rect (at -10.9855 -1.7526) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(J57-Pad1)"))
    (pad 59 smd rect (at -10.9855 -2.2479) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J53-Pad1)"))
    (pad 60 smd rect (at -10.9855 -2.7559) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(J56-Pad1)"))
    (pad 61 smd rect (at -10.9855 -3.2512) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(J86-Pad1)"))
    (pad 62 smd rect (at -10.9855 -3.7465) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(J54-Pad1)"))
    (pad 63 smd rect (at -10.9855 -4.2545) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(J55-Pad1)"))
    (pad 64 smd rect (at -10.9855 -4.7498) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 65 smd rect (at -10.9855 -5.2451) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 78 smd rect (at -6.2484 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(J108-Pad1)"))
    (pad 79 smd rect (at -5.7531 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(J107-Pad1)"))
    (pad 80 smd rect (at -5.2451 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(J73-Pad1)"))
    (pad 81 smd rect (at -4.7498 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 82 smd rect (at -4.2545 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 83 smd rect (at -3.7465 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(J69-Pad1)"))
    (pad 84 smd rect (at -3.2512 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(J70-Pad1)"))
    (pad 85 smd rect (at -2.7559 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(J75-Pad1)"))
    (pad 86 smd rect (at -2.2479 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(J76-Pad1)"))
    (pad 87 smd rect (at -1.7526 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(J104-Pad1)"))
    (pad 88 smd rect (at -1.2573 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(J95-Pad1)"))
    (pad 89 smd rect (at -0.7493 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(J79-Pad1)"))
    (pad 90 smd rect (at -0.254 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(J78-Pad1)"))
    (pad 91 smd rect (at 0.254 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(J80-Pad1)"))
    (pad 92 smd rect (at 0.7493 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(J77-Pad1)"))
    (pad 93 smd rect (at 1.2573 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(J84-Pad1)"))
    (pad 94 smd rect (at 1.7526 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(J81-Pad1)"))
    (pad 95 smd rect (at 2.2479 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(J85-Pad1)"))
    (pad 96 smd rect (at 2.7559 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(J82-Pad1)"))
    (pad 97 smd rect (at 3.2512 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(J83-Pad1)"))
    (pad 98 smd rect (at 3.7465 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(J39-Pad1)"))
    (pad 99 smd rect (at 4.2545 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(J38-Pad1)"))
    (pad 100 smd rect (at 4.7498 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J18-Pad1)"))
    (pad 101 smd rect (at 5.2451 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J17-Pad1)"))
    (pad 102 smd rect (at 5.7531 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 103 smd rect (at 6.2484 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 104 smd rect (at 6.7437 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(CON1-Pad5)"))
    (pad 105 smd rect (at 7.2517 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(CON1-Pad3)"))
    (pad 106 smd rect (at 7.747 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(CON1-Pad6)"))
    (pad 107 smd rect (at 8.2423 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(CON1-Pad1)"))
    (pad 108 smd rect (at 8.7503 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(CON1-Pad9)"))
    (pad 73 smd rect (at -8.7503 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(J72-Pad1)"))
    (pad 74 smd rect (at -8.2423 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(J98-Pad1)"))
    (pad 75 smd rect (at -7.747 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 117 "Net-(J102-Pad1)"))
    (pad 76 smd rect (at -7.2517 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(J109-Pad1)"))
    (pad 77 smd rect (at -6.7437 -10.9855) (size 0.254 1.524) (layers B.Cu B.Paste B.Mask)
      (net 118 "Net-(J103-Pad1)"))
    (pad 109 smd rect (at 10.9855 -8.7503) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J11-Pad1)"))
    (pad 110 smd rect (at 10.9855 -8.2423) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J10-Pad1)"))
    (pad 111 smd rect (at 10.9855 -7.747) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J9-Pad1)"))
    (pad 112 smd rect (at 10.9855 -7.2517) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J8-Pad1)"))
    (pad 113 smd rect (at 10.9855 -6.7437) (size 1.524 0.254) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J12-Pad1)"))
    (model smd/tqfp144.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.8488 100.5332)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 470pF (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 164.8714 83.439 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 127.0762 93.1418 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.8488 98.7044)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 2u2 (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 163.6522 92.075 270)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 143.002 80.6704)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1nF (at 0 -0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 153.7208 79.502 180)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.2794 -0.254 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.6456 76.3524 270)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 146.3548 96.4184)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175) (layer F.SilkS))
    (fp_text value 33nF (at 0 -0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 151.892 120.396 270)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 146.4056 94.6912)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175) (layer F.SilkS))
    (fp_text value 33n (at 0 -0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 135.5598 77.6986 90)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 120.28932 106.01452 90)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 118.58752 106.06532 90)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 129.3114 82.0674 90)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33n (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 133.5024 76.3778 90)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.1376 105.156)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 156.2354 105.0798 180)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10pF (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 163.2458 83.4644 90)
    (attr smd)
    (fp_text reference C19 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 143.002 82.3976)
    (attr smd)
    (fp_text reference C20 (at 0 0.3175) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.1122 106.934)
    (attr smd)
    (fp_text reference C21 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 165.4556 92.075 270)
    (attr smd)
    (fp_text reference C22 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 128.778 93.1418 270)
    (attr smd)
    (fp_text reference C23 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer F.Cu) (tedit 53B886C5)
    (at 153.7208 81.28 180)
    (attr smd)
    (fp_text reference C24 (at 0 0.3175 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.381 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 131.2164 82.7278 90)
    (attr smd)
    (fp_text reference C25 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 locked placed (layer B.Cu) (tedit 53B886C5)
    (at 158.4452 76.8096 90)
    (attr smd)
    (fp_text reference C26 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100pF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 139.5984 109.7788)
    (attr smd)
    (fp_text reference C27 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 8p2 (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 142.6464 109.2708 180)
    (attr smd)
    (fp_text reference C28 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 8p2F (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM1812 placed (layer B.Cu) (tedit 53B886C5)
    (at 161.2392 120.1166 270)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference F1 (at -0.74676 0 540) (layer B.SilkS))
    (fp_text value 750mA (at 0.762 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_B placed (layer F.Cu) (tedit 5435403B)
    (at 159.12592 116.69776)
    (tags USB)
    (fp_text reference J33 (at 0 6.35) (layer F.SilkS))
    (fp_text value USB (at -1.77292 -8.11276) (layer F.SilkS))
    (pad 1 thru_hole circle (at 1.27 -4.699) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(J33-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -4.699) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J33-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -2.70002) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J33-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 -2.70002) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 5.99948 0) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C10-Pad1)"))
    (pad 6 thru_hole circle (at -5.99948 0) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C10-Pad1)"))
    (model Connectors/USB_type_B.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 165.3286 64.6176 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(CON1-Pad6)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 156.21 103.378 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 6k81 (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 151.9936 108.6612 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33 (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J33-Pad3)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 153.6192 108.6612 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33 (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J33-Pad2)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53B886C5)
    (at 116.5606 110.49)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k5 (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J41-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical placed (layer F.Cu) (tedit 53B886C6)
    (at 142.1892 108.0008)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend,")
    (fp_text reference X1 (at 0.5588 -0.1778) (layer F.SilkS))
    (fp_text value 12MHz (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C27-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C28-Pad1)"))
  )
  (module "SMD_Packages:DO-214AC(SMA)" placed (layer B.Cu) (tedit 53BB12B6)
    (at 168.8084 122.6058 90)
    (descr "DO-214AC (SMA)  PACKAGE.")
    (tags "DO-214AC SMA")
    (attr smd)
    (fp_text reference D1 (at 0 2.60096 90) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.79908 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.89992 0 90) (size 1.6002 2.19964) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.89992 0 90) (size 1.6002 2.19964) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
    (model smd/do214.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.95 0.95 0.95))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345875)
    (at 128.9558 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 0.0762 0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345829)
    (at 146.4818 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at 0.0889 -0.0762 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434587E)
    (at 136.5758 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at 0.0508 0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J3-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J3-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345811)
    (at 131.2418 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 0.127 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345816)
    (at 133.7818 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at 0.1651 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J5-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J5-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458F9)
    (at 173.0756 86.868 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at -0.0254 0.127 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J6-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J6-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345925)
    (at 184.0484 86.106 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at -0.1778 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J7-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J7-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458F2)
    (at 173.0756 79.248 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J8 (at -0.0254 0.1524 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J8-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J8-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434591D)
    (at 184.0484 78.486 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J9 (at -0.127 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J9-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J9-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458F0)
    (at 173.0756 76.708 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J10 (at 0 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J10-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J10-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434591B)
    (at 184.0484 75.946 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J11 (at 0.0508 0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J11-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J11-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345920)
    (at 184.0484 81.026 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J12 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J12-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J12-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458F4)
    (at 173.0756 81.788 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J13 (at 0.0508 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J13-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J13-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345923)
    (at 184.0484 83.566 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J14 (at 0 0 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J14-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J14-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458F7)
    (at 173.0756 84.328 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J15 (at 0.0508 -0.1016 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J15-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J15-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345909)
    (at 173.0756 97.028 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J16 (at -0.0508 -0.0635 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J16-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J16-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F5E)
    (at 161.29 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J17 (at 0.1651 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J17-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J17-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F63)
    (at 162.814 59.309 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J18 (at -0.0508 0.1016 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J18-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J18-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345937)
    (at 184.0484 98.806 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J19 (at -0.0254 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J19-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J19-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434590B)
    (at 173.0756 99.568 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J20 (at 0.0127 -0.1397 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J20-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J20-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345912)
    (at 173.0756 104.648 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J21 (at -0.0127 0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J21-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J21-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345914)
    (at 173.0756 107.188 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J22 (at -0.0635 -0.2159 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J22-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J22-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345941)
    (at 184.0484 108.966 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J23 (at -0.1143 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J23-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J23-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434593F)
    (at 184.0484 106.426 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J24 (at -0.0635 -0.0635 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J24-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J24-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345939)
    (at 184.0484 101.346 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J25 (at 0 -0.1016 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J25-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J25-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345932)
    (at 184.0484 96.266 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J26 (at 0 0.2032 360) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J26-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J26-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458FF)
    (at 173.0756 91.948 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J27 (at -0.127 -0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(J27-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(J27-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345906)
    (at 173.0756 94.488 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J28 (at 0 -0.0635 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(J28-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(J28-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434592F)
    (at 184.0484 93.726 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J29 (at -0.0254 -0.2286 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J29-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J29-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345892)
    (at 144.1958 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J30 (at 0.127 0 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(J30-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(J30-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434592D)
    (at 184.0484 91.186 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J31 (at -0.0254 0 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(J31-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(J31-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458FC)
    (at 173.0756 89.408 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J32 (at -0.0508 -0.0762 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J32-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J32-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345859)
    (at 149.0218 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J34 (at 0.0635 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J34-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J34-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345896)
    (at 146.7358 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J35 (at 0.0762 -0.1016 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J35-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J35-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345885)
    (at 139.1158 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J36 (at 0.1397 0.1143 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C27-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C27-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434588C)
    (at 141.6558 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J37 (at 0.1778 0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C28-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C28-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F6A)
    (at 158.75 68.58 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J38 (at -0.1016 -0.0508 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J38-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J38-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F58)
    (at 160.274 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J39 (at 0.1524 -0.2032 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J39-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J39-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345871)
    (at 126.4158 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J40 (at 0.1016 0.1143 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J40-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J40-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345825)
    (at 143.9418 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J41 (at 0.0635 -0.0762 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J41-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J41-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345821)
    (at 141.4018 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J42 (at 0.1397 0.2032 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J42-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J42-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345898)
    (at 149.2758 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J43 (at 0.1524 0 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(J43-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(J43-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434593C)
    (at 184.0484 103.886 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J44 (at 0.0889 0.1397 360) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(J44-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(J44-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434590D)
    (at 173.0756 102.108 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J45 (at -0.0381 -0.1016 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(J45-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(J45-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434592B)
    (at 184.0484 88.646 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J46 (at -0.1143 -0.1143 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(J46-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(J46-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434581D)
    (at 138.8618 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J47 (at 0.2286 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(J47-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(J47-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345818)
    (at 136.3218 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J48 (at 0.1397 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(J48-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(J48-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434587B)
    (at 134.0358 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J49 (at 0.0254 0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J49-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J49-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345878)
    (at 131.4958 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J50 (at 0.1016 0.1143 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J50-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J50-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434580E)
    (at 128.7018 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J51 (at 0.0508 0.0889 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J51-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J51-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434579C)
    (at 110.1344 82.169 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J52 (at -0.0127 -0.1778 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J52-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J52-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434578A)
    (at 110.1344 77.089 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J53 (at 0.0127 -0.254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J53-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J53-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458B6)
    (at 120.2944 74.549 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J54 (at 0 0.0127 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J54-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J54-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345780)
    (at 110.1344 72.009 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J55 (at -0.0381 -0.4064 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J55-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J55-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458C5)
    (at 120.2944 77.089 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J56 (at -0.0635 -0.1143 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J56-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J56-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458C8)
    (at 120.2944 79.629 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J57 (at -0.0381 -0.0889 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J57-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J57-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457A1)
    (at 110.1344 84.709 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J58 (at -0.0254 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J58-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J58-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458CF)
    (at 120.2944 84.709 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J59 (at -0.0508 0 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J59-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J59-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458D5)
    (at 120.2944 89.789 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J60 (at -0.0254 -0.1524 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J60-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J60-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457AC)
    (at 110.1344 89.789 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J61 (at -0.0508 0.0127 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J61-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J61-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457C7)
    (at 110.1344 102.489 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J62 (at -0.1651 -0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J62-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J62-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434577B)
    (at 110.1344 69.469 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J63 (at 0.0127 -0.0635 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J63-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J63-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345804)
    (at 123.6218 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J64 (at 0.1524 0.0381 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J64-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J64-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434586C)
    (at 123.8758 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J65 (at 0.127 0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J65-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J65-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458C0)
    (at 120.2944 69.469 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J66 (at 0.0508 -0.0127 360) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J66-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J66-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458DF)
    (at 120.2944 99.949 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J67 (at -0.0762 0.0762 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J67-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J67-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345809)
    (at 126.1618 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J68 (at 0.0762 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J68-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J68-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F22)
    (at 138.43 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J69 (at 0.0762 0.127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J69-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J69-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345FA7)
    (at 142.494 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J70 (at 0.1397 -0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J70-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J70-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345868)
    (at 121.3358 113.2078)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J71 (at 0.0889 0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J71-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J71-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F04)
    (at 128.27 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J72 (at 0.0254 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J72-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J72-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345FA0)
    (at 139.954 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J73 (at 0.0762 -0.1016 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J73-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J73-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F0A)
    (at 129.794 59.309 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J74 (at -0.0762 0.0508 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J74-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J74-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F26)
    (at 140.97 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J75 (at 0.1016 0.127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J75-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J75-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345FAC)
    (at 145.034 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J76 (at 0.0635 -0.0635 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J76-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J76-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F41)
    (at 152.654 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J77 (at 0.1143 -0.1143 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J77-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J77-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F3B)
    (at 150.114 59.309 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J78 (at -0.0889 0.1016 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(J78-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(J78-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F2F)
    (at 146.05 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J79 (at 0.0508 0 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(J79-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(J79-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F35)
    (at 148.59 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J80 (at 0.1016 0.0381 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J80-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J80-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F46)
    (at 155.194 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J81 (at 0.1143 -0.1397 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J81-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J81-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F53)
    (at 157.734 59.309 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J82 (at -0.0762 0.0889 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(J82-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(J82-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F4D)
    (at 156.21 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J83 (at 0.1524 -0.0508 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(J83-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(J83-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F7D)
    (at 151.13 68.58 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J84 (at -0.0762 0.0508 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J84-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J84-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F81)
    (at 153.67 68.58 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J85 (at -0.0127 0.0508 270) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(J85-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(J85-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345785)
    (at 110.1344 74.549 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J86 (at -0.0508 -0.3683 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J86-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J86-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458E2)
    (at 120.2944 102.489 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J87 (at -0.0762 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J87-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J87-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458DC)
    (at 120.2944 94.869 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J88 (at -0.127 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(J88-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(J88-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457B1)
    (at 110.1344 92.329 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J89 (at -0.0635 -0.0635 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(J89-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(J89-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457A7)
    (at 110.1344 87.249 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J90 (at -0.0762 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(J90-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(J90-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458D2)
    (at 120.2944 87.249 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J91 (at 0.0254 -0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(J91-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(J91-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345800)
    (at 121.0818 123.571)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J92 (at 0.0635 0.1524 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(J92-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(J92-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345EFF)
    (at 125.73 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J93 (at 0.1143 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(J93-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(J93-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F8E)
    (at 124.714 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J94 (at 0.1397 0 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(J94-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(J94-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345FAF)
    (at 147.574 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J95 (at 0.0508 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(J95-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(J95-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458BA)
    (at 120.2944 72.009 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J96 (at -0.127 -0.3175 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(J96-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(J96-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F91)
    (at 127.254 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J97 (at 0.127 -0.0127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(J97-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(J97-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F96)
    (at 132.334 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J98 (at 0.0889 -0.0127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(J98-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(J98-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457C3)
    (at 110.1344 99.949 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J99 (at -0.0254 0.1778 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(J99-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(J99-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457BF)
    (at 110.1344 97.409 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J100 (at -0.1016 0 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(J100-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(J100-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543457BB)
    (at 110.1344 94.869 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J101 (at -0.0127 0.1143 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(J101-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(J101-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F0E)
    (at 130.81 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J102 (at 0.0762 0.0762 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(J102-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(J102-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F16)
    (at 133.35 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J103 (at 0.1016 -0.0254 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(J103-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(J103-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F2C)
    (at 143.51 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J104 (at 0.0762 -0.0762 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(J104-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(J104-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458E6)
    (at 120.2944 97.409 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J105 (at 0.0508 -0.0254 360) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(J105-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(J105-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458D9)
    (at 120.2944 92.329 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J106 (at -0.0762 0 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(J106-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(J106-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F1C)
    (at 135.89 68.58)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J107 (at 0.127 -0.0508 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(J107-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(J107-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F9C)
    (at 137.414 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J108 (at 0.1016 -0.0127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(J108-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(J108-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 54345F99)
    (at 134.874 59.309)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J109 (at 0.127 -0.0127 90) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(J109-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(J109-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5434578F)
    (at 110.1344 79.629 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J110 (at -0.0381 -0.0254 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(J110-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(J110-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 543458CA)
    (at 120.2944 82.169 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J111 (at 0.0127 -0.0508 180) (layer F.SilkS))
    (fp_text value JUMP_2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(J111-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(J111-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 550A8FC0)
    (at 163.1696 111.9124)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0 -0.381) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(J33-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53BB12B6)
    (at 153.67 120.396 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10R (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOT223 placed (layer B.Cu) (tedit 53BB12B6)
    (at 173.1899 113.81486 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.762 270) (layer B.SilkS))
    (fp_text value NCP1117ST33T3G (at 0 -0.762 270) (layer B.SilkS))
    (pad 4 smd rect (at 0 3.302 270) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
    (pad 3 smd rect (at 2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
    (pad 1 smd rect (at -2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/SOT223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 550A8F68)
    (at 180.213 113.4364 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C29 (at -0.2286 0 90) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 -2.49936 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 550A8F6F)
    (at 165.6334 107.60964 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C30 (at -0.08636 0.1016 90) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 -2.49936 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 13 3V3))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 54BBE638)
    (at 111.76 60.96)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 0) (layer F.SilkS))
    (fp_text value "HOLE 3mm" (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 54BBE638)
    (at 111.76 121.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 0) (layer F.SilkS))
    (fp_text value "HOLE 3mm" (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 54BBE638)
    (at 182.88 121.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 0) (layer F.SilkS))
    (fp_text value "HOLE 3mm" (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 54BBE638)
    (at 182.88 60.96)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 0) (layer F.SilkS))
    (fp_text value "HOLE 3mm" (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 550054B0)
    (at 169.0116 63.2206 180)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference CON1 (at 0 -7.62 180) (layer F.SilkS) hide)
    (fp_text value AVR-JTAG-10 (at -0.4826 9.017 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 3V3))
    (pad 5 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(CON1-Pad5)"))
    (pad 6 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON1-Pad6)"))
    (pad 7 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole rect (at -1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(CON1-Pad9)"))
    (pad 10 thru_hole rect (at 1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 550054B6)
    (at 175.006 121.8692 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J112 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2x03_PARALLEL (at 1.1176 -8.8138 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 55004DAF)
    (at 176.4792 69.2912 270)
    (fp_text reference S1 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652 450) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.15 -2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 3.15 2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON1-Pad6)"))
    (pad 1 thru_hole rect (at -3.15 -2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -3.15 2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON1-Pad6)"))
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 55004DAF)
    (at 113.03 110.6932 270)
    (fp_text reference S2 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652 450) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.15 -2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J41-Pad1)"))
    (pad 2 thru_hole rect (at 3.15 2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -3.15 -2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J41-Pad1)"))
    (pad 2 thru_hole rect (at -3.15 2.75 270) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module graphics:QR_code (layer F.Cu) (tedit 550052D2)
    (at 136.4488 93.6498)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (dimension 70.612 (width 0.2) (layer Cmts.User)
    (gr_text "2,7800 v" (at 195.21 91.44 270) (layer Cmts.User))
    (feature1 (pts (xy 187.706 126.746) (xy 196.11 126.746)))
    (feature2 (pts (xy 187.706 56.134) (xy 196.11 56.134)))
    (crossbar (pts (xy 194.31 56.134) (xy 194.31 126.746)))
    (arrow1a (pts (xy 194.31 126.746) (xy 193.723579 125.619496)))
    (arrow1b (pts (xy 194.31 126.746) (xy 194.896421 125.619496)))
    (arrow2a (pts (xy 194.31 56.134) (xy 193.723579 57.260504)))
    (arrow2b (pts (xy 194.31 56.134) (xy 194.896421 57.260504)))
  )
  (dimension 80.772 (width 0.2) (layer Cmts.User)
    (gr_text "3,1800 v" (at 147.32 47.868) (layer Cmts.User))
    (feature1 (pts (xy 187.706 56.134) (xy 187.706 46.968)))
    (feature2 (pts (xy 106.934 56.134) (xy 106.934 46.968)))
    (crossbar (pts (xy 106.934 48.768) (xy 187.706 48.768)))
    (arrow1a (pts (xy 187.706 48.768) (xy 186.579496 49.354421)))
    (arrow1b (pts (xy 187.706 48.768) (xy 186.579496 48.181579)))
    (arrow2a (pts (xy 106.934 48.768) (xy 108.060504 49.354421)))
    (arrow2b (pts (xy 106.934 48.768) (xy 108.060504 48.181579)))
  )
  (dimension 70.612 (width 0.2) (layer Cmts.User)
    (gr_text "70,612 mm" (at 190.892 91.44 270) (layer Cmts.User))
    (feature1 (pts (xy 187.706 126.746) (xy 191.792 126.746)))
    (feature2 (pts (xy 187.706 56.134) (xy 191.792 56.134)))
    (crossbar (pts (xy 189.992 56.134) (xy 189.992 126.746)))
    (arrow1a (pts (xy 189.992 126.746) (xy 189.405579 125.619496)))
    (arrow1b (pts (xy 189.992 126.746) (xy 190.578421 125.619496)))
    (arrow2a (pts (xy 189.992 56.134) (xy 189.405579 57.260504)))
    (arrow2b (pts (xy 189.992 56.134) (xy 190.578421 57.260504)))
  )
  (dimension 80.772 (width 0.2) (layer Cmts.User)
    (gr_text "80,772 mm" (at 147.32 52.694) (layer Cmts.User))
    (feature1 (pts (xy 187.706 56.134) (xy 187.706 51.794)))
    (feature2 (pts (xy 106.934 56.134) (xy 106.934 51.794)))
    (crossbar (pts (xy 106.934 53.594) (xy 187.706 53.594)))
    (arrow1a (pts (xy 187.706 53.594) (xy 186.579496 54.180421)))
    (arrow1b (pts (xy 187.706 53.594) (xy 186.579496 53.007579)))
    (arrow2a (pts (xy 106.934 53.594) (xy 108.060504 54.180421)))
    (arrow2b (pts (xy 106.934 53.594) (xy 108.060504 53.007579)))
  )
  (gr_text PA30 (at 146.558 118.491 90) (layer F.SilkS))
  (gr_text PA02 (at 144.526 103.378 90) (layer F.SilkS))
  (gr_text PB10 (at 144.018 118.745 90) (layer F.SilkS))
  (gr_text PB09 (at 141.224 118.491 90) (layer F.SilkS))
  (gr_text PC02 (at 142.113 103.378 90) (layer F.SilkS))
  (gr_text PC03 (at 139.319 103.251 90) (layer F.SilkS))
  (gr_text PB04 (at 138.938 118.745 90) (layer F.SilkS))
  (gr_text PA29 (at 135.763 108.331 90) (layer F.SilkS))
  (gr_text PB03 (at 136.144 118.872 90) (layer F.SilkS))
  (gr_text PB02 (at 134.112 108.458 90) (layer F.SilkS))
  (gr_text PA27 (at 133.858 118.872 90) (layer F.SilkS))
  (gr_text PB01 (at 131.572 108.458 90) (layer F.SilkS))
  (gr_text PA28 (at 131.318 118.745 90) (layer F.SilkS))
  (gr_text PA31 (at 129.032 108.458 90) (layer F.SilkS))
  (gr_text PB00 (at 128.778 118.872 90) (layer F.SilkS))
  (gr_text PB11 (at 126.492 108.458 90) (layer F.SilkS))
  (gr_text PX16 (at 126.365 118.745 90) (layer F.SilkS))
  (gr_text PX13 (at 123.952 108.458 90) (layer F.SilkS))
  (gr_text PX12 (at 123.698 118.745 90) (layer F.SilkS))
  (gr_text PX19 (at 121.412 108.331 90) (layer F.SilkS))
  (gr_text PX40 (at 121.158 118.618 90) (layer F.SilkS))
  (gr_text PA15 (at 161.29 73.279 90) (layer F.SilkS))
  (gr_text PA14 (at 162.941 63.881 90) (layer F.SilkS))
  (gr_text PC01 (at 158.75 73.279 90) (layer F.SilkS))
  (gr_text PC00 (at 160.274 63.881 90) (layer F.SilkS))
  (gr_text PX31 (at 156.21 73.279 90) (layer F.SilkS))
  (gr_text PX30 (at 157.734 63.881 90) (layer F.SilkS))
  (gr_text PX33 (at 153.797 73.279 90) (layer F.SilkS))
  (gr_text PX29 (at 155.194 63.881 90) (layer F.SilkS))
  (gr_text PX32 (at 151.13 73.279 90) (layer F.SilkS))
  (gr_text PX25 (at 152.654 64.008 90) (layer F.SilkS))
  (gr_text PX28 (at 148.59 73.279 90) (layer F.SilkS))
  (gr_text PX26 (at 150.114 63.881 90) (layer F.SilkS))
  (gr_text PX27 (at 146.304 73.406 90) (layer F.SilkS))
  (gr_text PX43 (at 147.574 64.008 90) (layer F.SilkS))
  (gr_text PX52 (at 143.637 73.406 90) (layer F.SilkS))
  (gr_text PX24 (at 145.034 64.008 90) (layer F.SilkS))
  (gr_text PX23 (at 140.97 73.279 90) (layer F.SilkS))
  (gr_text PX18 (at 142.494 63.881 90) (layer F.SilkS))
  (gr_text PA09 (at 179.197 108.966) (layer F.SilkS))
  (gr_text PA10 (at 168.148 107.315) (layer F.SilkS))
  (gr_text PA08 (at 179.197 106.553) (layer F.SilkS))
  (gr_text PA11 (at 168.275 104.775) (layer F.SilkS))
  (gr_text PB07 (at 179.197 104.013) (layer F.SilkS))
  (gr_text PB06 (at 168.275 102.108) (layer F.SilkS))
  (gr_text "PA07\n" (at 179.197 101.473) (layer F.SilkS))
  (gr_text PA12 (at 168.275 99.568) (layer F.SilkS))
  (gr_text PA13 (at 178.943 98.933) (layer F.SilkS))
  (gr_text PA16 (at 168.275 97.028) (layer F.SilkS))
  (gr_text PA06 (at 179.324 96.266) (layer F.SilkS))
  (gr_text PA04 (at 168.275 94.615) (layer F.SilkS))
  (gr_text PA03 (at 179.324 93.726) (layer F.SilkS))
  (gr_text PA05 (at 168.275 91.948) (layer F.SilkS))
  (gr_text 1 (at 170.561 70.739) (layer F.SilkS))
  (gr_text JTAG (at 165.481 63.373 90) (layer F.SilkS))
  (gr_text PA01 (at 179.324 91.313) (layer F.SilkS))
  (gr_text PA00 (at 168.275 89.535) (layer F.SilkS))
  (gr_text PB05 (at 179.324 88.773) (layer F.SilkS))
  (gr_text PA26 (at 168.402 86.868) (layer F.SilkS))
  (gr_text PA25 (at 179.324 86.233) (layer F.SilkS))
  (gr_text PA17 (at 168.275 84.455) (layer F.SilkS))
  (gr_text PA18 (at 179.324 83.693) (layer F.SilkS))
  (gr_text PA19 (at 168.275 81.915) (layer F.SilkS))
  (gr_text PA20 (at 179.324 81.153) (layer F.SilkS))
  (gr_text PA24 (at 168.275 79.502) (layer F.SilkS))
  (gr_text PA23 (at 179.324 78.613) (layer F.SilkS))
  (gr_text PA22 (at 168.148 76.327) (layer F.SilkS))
  (gr_text PA21 (at 179.324 75.946) (layer F.SilkS))
  (gr_text PX17 (at 138.557 73.406 90) (layer F.SilkS))
  (gr_text PX21 (at 139.827 63.881 90) (layer F.SilkS))
  (gr_text PX55 (at 135.89 73.406 90) (layer F.SilkS))
  (gr_text PX56 (at 137.414 63.881 90) (layer F.SilkS))
  (gr_text PX51 (at 133.35 73.279 90) (layer F.SilkS))
  (gr_text PX57 (at 134.874 64.008 90) (layer F.SilkS))
  (gr_text PX50 (at 130.683 73.533 90) (layer F.SilkS))
  (gr_text PX46 (at 132.334 63.881 90) (layer F.SilkS))
  (gr_text PX20 (at 128.27 73.533 90) (layer F.SilkS))
  (gr_text PX22 (at 129.794 63.881 90) (layer F.SilkS))
  (gr_text PX41 (at 123.571 65.913 90) (layer F.SilkS))
  (gr_text PX45 (at 127.254 63.881 90) (layer F.SilkS))
  (gr_text PX42 (at 122.428 59.309 90) (layer F.SilkS))
  (gr_text PX14 (at 120.269 67.056) (layer F.SilkS))
  (gr_text PX11 (at 114.935 69.596) (layer F.SilkS))
  (gr_text PX44 (at 124.968 72.644) (layer F.SilkS))
  (gr_text PX03 (at 114.935 72.263) (layer F.SilkS))
  (gr_text PX02 (at 124.968 74.803) (layer F.SilkS))
  (gr_text PX34 (at 114.935 74.803) (layer F.SilkS))
  (gr_text PX04 (at 124.968 77.343) (layer F.SilkS))
  (gr_text PX01 (at 114.935 77.216) (layer F.SilkS))
  (gr_text PX05 (at 124.968 79.756) (layer F.SilkS))
  (gr_text PX58 (at 114.935 79.883) (layer F.SilkS))
  (gr_text PX59 (at 124.968 82.423) (layer F.SilkS))
  (gr_text PX00 (at 114.935 82.423) (layer F.SilkS))
  (gr_text PX07 (at 124.968 84.963) (layer F.SilkS))
  (gr_text PX06 (at 114.935 84.963) (layer F.SilkS))
  (gr_text PX39 (at 124.968 87.503) (layer F.SilkS))
  (gr_text PX38 (at 114.935 87.503) (layer F.SilkS))
  (gr_text PX08 (at 124.968 89.916) (layer F.SilkS))
  (gr_text PX09 (at 114.935 89.916) (layer F.SilkS))
  (gr_text PX54 (at 124.968 92.329) (layer F.SilkS))
  (gr_text PX37 (at 114.808 92.583) (layer F.SilkS))
  (gr_text PX36 (at 124.968 95.123) (layer F.SilkS))
  (gr_text PX49 (at 114.808 95.123) (layer F.SilkS))
  (gr_text PX53 (at 124.968 97.663) (layer F.SilkS))
  (gr_text PX48 (at 114.808 97.663) (layer F.SilkS))
  (gr_text PX15 (at 124.968 100.076) (layer F.SilkS))
  (gr_text PX47 (at 114.808 100.203) (layer F.SilkS))
  (gr_text PX35 (at 125.095 102.743) (layer F.SilkS))
  (gr_text PX10 (at 114.808 102.743) (layer F.SilkS))
  (gr_text PC04 (at 146.812 103.759 90) (layer F.SilkS))
  (gr_text PC05 (at 149.225 118.872 90) (layer F.SilkS))
  (gr_text PB08 (at 149.606 108.204 90) (layer F.SilkS))
  (gr_text RESET (at 181.61 69.342 90) (layer F.SilkS))
  (gr_text "POWER +5V" (at 175.006 116.713) (layer F.SilkS))
  (gr_text "www.mlab.cz\nKaklik 2015" (at 146.812 87.122) (layer F.SilkS))
  (gr_text AT32TQ14401A (at 146.939 84.836) (layer F.SilkS))
  (gr_line (start 187.706 56.134) (end 106.934 56.134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.706 126.746) (end 187.706 56.134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.934 126.746) (end 187.706 126.746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.934 56.134) (end 106.934 126.746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 55.88) (xy 106.68 127) (xy 187.96 127) (xy 187.96 118.237) (xy 167.513 118.237)
        (xy 167.513 110.363) (xy 187.96 110.363) (xy 187.96 55.88)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.96 127) (xy 106.68 127) (xy 106.68 55.88) (xy 187.96 55.88)
      )
    )
  )
  (zone (net 13) (net_name 3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.706 117.856) (xy 167.894 117.856) (xy 167.894 110.744) (xy 187.706 110.744)
      )
    )
  )
)
