(kicad_pcb (version 4) (host pcbnew 0.201503180816+5524~22~ubuntu14.04.1-product)
  (general
    (links 82)
    (no_connects 0)
    (area 106.666215 95.6945 175.3472 140.903101)
    (thickness 1.6)
    (drawings 19)
    (tracks 247)
    (zones 0)
    (modules 30)
    (nets 26)
  )
  (page A4)
  (title_block
    (title BLE01)
    (date "20. 1. 2015")
    (rev A)
    (company "Mlab www.mlab.cz")
    (comment 1 "Module with the NRF8001 Bluetooth Low Energy chip from Nordic Semiconductor")
    (comment 2 "ondra6ak <ondra6ak@gmail.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.532)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1)
    (via_drill 0.5)
    (via_min_size 1)
    (via_min_drill 0.5)
    (uvia_size 0.5)
    (uvia_drill 0.25)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.25)
    (pcb_text_width 0.127)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.127)
    (mod_text_size 1 1)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.889)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01130_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /AVDD)
  (net 3 "Net-(C8-Pad1)")
  (net 4 /VDD_PA)
  (net 5 /XC2)
  (net 6 /XC1)
  (net 7 /ACTIVE)
  (net 8 /SCK)
  (net 9 /REQN)
  (net 10 /MOSI)
  (net 11 /MISO)
  (net 12 /RDYN)
  (net 13 /TXD)
  (net 14 /RXD)
  (net 15 /RESET)
  (net 16 /ANT2)
  (net 17 /ANT1)
  (net 18 "Net-(R1-Pad2)")
  (net 19 VCC)
  (net 20 "Net-(C7-Pad1)")
  (net 21 "Net-(L1-Pad1)")
  (net 22 "Net-(L1-Pad2)")
  (net 23 "Net-(C6-Pad1)")
  (net 24 "Net-(C8-Pad2)")
  (net 25 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.5)
    (uvia_drill 0.25)
    (add_net /ACTIVE)
    (add_net /ANT1)
    (add_net /ANT2)
    (add_net /AVDD)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RDYN)
    (add_net /REQN)
    (add_net /RESET)
    (add_net /RXD)
    (add_net /SCK)
    (add_net /TXD)
    (add_net /VDD_PA)
    (add_net /XC1)
    (add_net /XC2)
    (add_net GND)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net VCC)
  )
  (module SMD_Packages:SMD-0805 placed (layer B.Cu) (tedit 549FCE36)
    (at 153.6192 109.2962)
    (attr smd)
    (fp_text reference L5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 5.6nH (at 0 -0.381) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /ANT1))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD_PA))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A7A65F)
    (at 134.53872 117.57152 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.429 -0.00508 180) (layer B.SilkS))
    (fp_text value 33nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:QFN-32-1EP placed (layer B.Cu) (tedit 54A7B3EC)
    (at 146.01444 113.51514)
    (descr QFN-32-1EP)
    (attr smd)
    (fp_text reference U1 (at 2.00025 -3.53695) (layer B.SilkS))
    (fp_text value NRF8001 (at 3.937 2.667) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.39776 1.74752) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (pad 2 smd rect (at -2.39776 1.24714) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (pad 3 smd rect (at -2.39776 0.74676) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C7-Pad1)"))
    (pad 4 smd rect (at -2.39776 0.24638) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.39776 -0.25146) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.39776 -0.75184) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 7 /ACTIVE))
    (pad 7 smd rect (at -2.39776 -1.25222) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 13 /TXD))
    (pad 8 smd rect (at -2.39776 -1.7526) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 0.24892 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 10 /MOSI))
    (pad 14 smd rect (at 0.74676 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 11 /MISO))
    (pad 15 smd rect (at 1.24714 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 1.74752 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 12 /RDYN))
    (pad 33 smd rect (at 0 0) (size 3.29946 3.29946) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -1.75006 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (pad 10 smd rect (at -1.24968 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 14 /RXD))
    (pad 11 smd rect (at -0.7493 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 8 /SCK))
    (pad 12 smd rect (at -0.25146 -2.40284) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 9 /REQN))
    (pad 17 smd rect (at 2.39776 -1.74752) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 2.4003 -1.24714) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 2.4003 -0.7493) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 15 /RESET))
    (pad 20 smd rect (at 2.4003 -0.24892) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD_PA))
    (pad 21 smd rect (at 2.4003 0.25146) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 17 /ANT1))
    (pad 22 smd rect (at 2.4003 0.75184) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 16 /ANT2))
    (pad 23 smd rect (at 2.4003 1.25222) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.4003 1.7526) (size 0.59944 0.24892) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 25 smd rect (at 1.75006 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(R1-Pad2)"))
    (pad 26 smd rect (at 1.24968 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 27 smd rect (at 0.7493 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 5 /XC2))
    (pad 28 smd rect (at 0.25146 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 6 /XC1))
    (pad 29 smd rect (at -0.24892 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 30 smd rect (at -0.7493 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -1.24968 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -1.75006 2.4003) (size 0.24892 0.59944) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(L1-Pad1)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A92E01)
    (at 139.98448 116.49456 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.2385 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54BEA8A3)
    (at 137.0838 126.238 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.39852 0.00508 180) (layer B.SilkS))
    (fp_text value 1nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54B27248)
    (at 148.4122 124.2187 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.3655 0 270) (layer B.SilkS))
    (fp_text value 12pF (at 0 -2.1 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /XC2))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54BE06FD)
    (at 143.5608 124.2187 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.31724 0.00508 270) (layer B.SilkS))
    (fp_text value 12pF (at 0 -2.1 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /XC1))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A92DEF)
    (at 134.53872 119.888 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.3782 0.0127 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54BD6535)
    (at 153.6192 116.9162)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.3401 0) (layer B.SilkS))
    (fp_text value 1.8pF (at 0 -2.1) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C8-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54BD6521)
    (at 153.6192 119.4181 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 3.3401 0 180) (layer B.SilkS))
    (fp_text value 1.2pF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A6FC28)
    (at 153.6192 106.5149 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.8735 0 180) (layer B.SilkS))
    (fp_text value 2.2nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD_PA))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A6FC35)
    (at 138.7729 111.0996 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 3.8735 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 54A7B3F5)
    (at 148.9202 101.6508 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -0.01905 1.82245 270) (layer B.SilkS))
    (fp_text value 22uF/6.3V (at 0 -2.1 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 placed (layer B.Cu) (tedit 549FCE2F)
    (at 137.0838 122.0089 180)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uH (at 0 -0.381 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(L1-Pad2)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 placed (layer B.Cu) (tedit 54A704D4)
    (at 137.0838 124.0917)
    (attr smd)
    (fp_text reference L2 (at 0 -0.4572) (layer B.SilkS))
    (fp_text value 15nH (at 0 -0.381) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(L1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 placed (layer B.Cu) (tedit 549FCE24)
    (at 153.6192 114.554 180)
    (attr smd)
    (fp_text reference L3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 3.9nH (at 0 -0.381 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /ANT2))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C8-Pad1)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 placed (layer B.Cu) (tedit 549FCE1B)
    (at 153.6192 111.6584)
    (attr smd)
    (fp_text reference L4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 8.2nH (at 0 -0.381) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /ANT1))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /ANT2))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 54BE0710)
    (at 152.3619 124.2568 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.27914 -0.00508 90) (layer B.SilkS))
    (fp_text value 22k (at 0 -2.1 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(R1-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 54A7D2F2)
    (at 145.98269 120.48109 180)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend,")
    (fp_text reference X1 (at 0 0 450) (layer F.SilkS))
    (fp_text value 16MHz (at 0 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.44094 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 /XC2))
    (pad 2 thru_hole circle (at 2.44094 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 6 /XC1))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 54BEA8B5)
    (at 137.0838 128.4859 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.39852 -0.0127 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer B.Cu) (tedit 54BEA8C5)
    (at 132.05206 127.04572)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -0.00762 1.36652) (layer B.SilkS))
    (fp_text value GREEN (at 0 -1.27) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 54BD63FE)
    (at 151.9809 101.6635 90)
    (attr smd)
    (fp_text reference D2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1N4007 (at 0 -0.381 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 VCC))
    (model SMD_Packages/SMD-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x09 locked (layer F.Cu) (tedit 54BD65E3)
    (at 120.4595 116.9035 180)
    (descr "pin header straight 2x09")
    (tags "pin header straight 2x09")
    (fp_text reference J1 (at 0 -12.7 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2x09_PARALLEL (at 0 12.7 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -10.16 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -10.16 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /ACTIVE))
    (pad 2 thru_hole rect (at 1.27 -10.16 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /ACTIVE))
    (pad 3 thru_hole rect (at -1.27 -7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /TXD))
    (pad 4 thru_hole rect (at 1.27 -7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /TXD))
    (pad 5 thru_hole rect (at -1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXD))
    (pad 6 thru_hole rect (at 1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXD))
    (pad 7 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SCK))
    (pad 8 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SCK))
    (pad 9 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /REQN))
    (pad 10 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /REQN))
    (pad 11 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MOSI))
    (pad 12 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MOSI))
    (pad 13 thru_hole rect (at -1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /MISO))
    (pad 14 thru_hole rect (at 1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /MISO))
    (pad 15 thru_hole rect (at -1.27 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /RDYN))
    (pad 16 thru_hole rect (at 1.27 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /RDYN))
    (pad 17 thru_hole rect (at -1.27 10.16 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /RESET))
    (pad 18 thru_hole rect (at 1.27 10.16 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /RESET))
    (model Pin_Headers/Pin_Header_Straight_2x09.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 locked (layer F.Cu) (tedit 54BD5CC8)
    (at 140.7795 101.6635 270)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J2 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value "1.9V ... 3.6V" (at -3.6195 0 360) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 VCC))
    (pad 4 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 VCC))
    (pad 5 thru_hole rect (at -1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 54BD5BBE)
    (at 120.4595 101.6635)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND))
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 54BD5BB9)
    (at 161.0995 101.6635)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 54BD5BAF)
    (at 120.4595 132.1435)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND))
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 54BD5BB3)
    (at 161.0995 132.1435)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND))
  )
  (module Mlab_Con:SMA6251A13G50 (layer F.Cu) (tedit 54BE09C8)
    (at 161.0868 116.9035)
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value SMA6251A13G50 (at 0 5.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54BD5D2C)
    (at 126.74346 127.05842 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.651 180) (layer B.SilkS))
    (fp_text value 68 (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /ACTIVE))
    (model Resistors_SMD/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 40.386 (width 0.127) (layer Dwgs.User)
    (gr_text "1,5900 v" (at 113.169 116.9035 90) (layer Dwgs.User))
    (feature1 (pts (xy 115.5065 96.7105) (xy 112.165 96.7105)))
    (feature2 (pts (xy 115.5065 137.0965) (xy 112.165 137.0965)))
    (crossbar (pts (xy 114.173 137.0965) (xy 114.173 96.7105)))
    (arrow1a (pts (xy 114.173 96.7105) (xy 114.759421 97.837004)))
    (arrow1b (pts (xy 114.173 96.7105) (xy 113.586579 97.837004)))
    (arrow2a (pts (xy 114.173 137.0965) (xy 114.759421 135.969996)))
    (arrow2b (pts (xy 114.173 137.0965) (xy 113.586579 135.969996)))
  )
  (dimension 50.546 (width 0.127) (layer Dwgs.User)
    (gr_text "1,9900 v" (at 140.7795 91.96) (layer Dwgs.User))
    (feature1 (pts (xy 166.0525 96.7105) (xy 166.0525 90.956)))
    (feature2 (pts (xy 115.5065 96.7105) (xy 115.5065 90.956)))
    (crossbar (pts (xy 115.5065 92.964) (xy 166.0525 92.964)))
    (arrow1a (pts (xy 166.0525 92.964) (xy 164.925996 93.550421)))
    (arrow1b (pts (xy 166.0525 92.964) (xy 164.925996 92.377579)))
    (arrow2a (pts (xy 115.5065 92.964) (xy 116.633004 93.550421)))
    (arrow2b (pts (xy 115.5065 92.964) (xy 116.633004 92.377579)))
  )
  (gr_text RXD (at 124.0155 121.9835) (layer F.SilkS))
  (dimension 50.546 (width 0.127) (layer Dwgs.User)
    (gr_text "50,546 mm" (at 140.7795 139.7896) (layer Dwgs.User))
    (feature1 (pts (xy 115.5065 137.0965) (xy 115.5065 140.7936)))
    (feature2 (pts (xy 166.0525 137.0965) (xy 166.0525 140.7936)))
    (crossbar (pts (xy 166.0525 138.7856) (xy 115.5065 138.7856)))
    (arrow1a (pts (xy 115.5065 138.7856) (xy 116.633004 138.199179)))
    (arrow1b (pts (xy 115.5065 138.7856) (xy 116.633004 139.372021)))
    (arrow2a (pts (xy 166.0525 138.7856) (xy 164.925996 138.199179)))
    (arrow2b (pts (xy 166.0525 138.7856) (xy 164.925996 139.372021)))
  )
  (dimension 40.386 (width 0.127) (layer Dwgs.User)
    (gr_text "40,386 mm" (at 168.7837 116.9035 270) (layer Dwgs.User))
    (feature1 (pts (xy 166.0525 137.0965) (xy 169.7877 137.0965)))
    (feature2 (pts (xy 166.0525 96.7105) (xy 169.7877 96.7105)))
    (crossbar (pts (xy 167.7797 96.7105) (xy 167.7797 137.0965)))
    (arrow1a (pts (xy 167.7797 137.0965) (xy 167.193279 135.969996)))
    (arrow1b (pts (xy 167.7797 137.0965) (xy 168.366121 135.969996)))
    (arrow2a (pts (xy 167.7797 96.7105) (xy 167.193279 97.837004)))
    (arrow2b (pts (xy 167.7797 96.7105) (xy 168.366121 97.837004)))
  )
  (gr_text "BLE01A\nWWW.MLAB.CZ\n2015" (at 145.8468 109.1184) (layer F.SilkS))
  (gr_text ondra6ak (at 152.019 132.334) (layer F.SilkS))
  (gr_text RESET (at 124.0155 106.7435) (layer F.SilkS))
  (gr_text TXD (at 124.0155 124.5235) (layer F.SilkS))
  (gr_text RDYN (at 124.0155 109.2835) (layer F.SilkS))
  (gr_text MISO (at 124.0155 111.8235) (layer F.SilkS))
  (gr_text MOSI (at 124.0155 114.3635) (layer F.SilkS))
  (gr_text REQN (at 124.0155 116.9035) (layer F.SilkS))
  (gr_text SCK (at 124.0155 119.4435) (layer F.SilkS))
  (gr_text ACTIVE (at 124.0155 127.0635) (layer F.SilkS))
  (gr_line (start 166.0525 96.7105) (end 115.5065 96.7105) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.0525 96.7105) (end 166.0525 137.0965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5065 137.0965) (end 166.0525 137.0965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5065 96.7105) (end 115.5065 137.0965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 19) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.5065 96.7105) (xy 166.0525 96.7105) (xy 166.0525 137.0965) (xy 115.5065 137.0965)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.5065 96.72066) (xy 166.0525 96.72066) (xy 166.0525 137.10666) (xy 115.5065 137.10666)
      )
    )
  )
)
