(kicad_pcb (version 20170123) (host pcbnew "(2017-02-05 revision 431abcf)-makepkg")
  (general
    (links 49)
    (no_connects 0)
    (area 0.178999 -40.461001 60.781001 -0.178999)
    (thickness 1.6)
    (drawings 16)
    (tracks 448)
    (zones 0)
    (modules 28)
    (nets 10)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C10-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(C11-Pad2)")
  (net 8 "Net-(C17-Pad1)")
  (net 9 "Net-(C17-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C6-Pad1)")
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 16.002 -20.32)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 21.59 -30.734 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 24.13 -19.304 90)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 43pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 24.384 -30.734 90)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF/16V (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 26.924 -20.32 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 3.9pF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 31.75 -19.304 90)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 30pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 34.544 -20.32 180)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 3.9pF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 58902C63)
    (at 34.29 -31.75 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C10 (at 0.0127 -0.0381 90) (layer B.SilkS))
    (fp_text value 47uF/16V (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 39.37 -19.304 90)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 43pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 37.592 -30.48 90)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF/16V (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 40.132 -30.48 90)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 45.466 -20.32 180)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 58902C63)
    (at 29.21 -31.75 270)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D1 (at 0.254 0 270) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 270) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 270) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -2.14884 0 270) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:SMA6251A13G50 locked (layer F.Cu) (tedit 58902C63)
    (at 10.16 -20.32)
    (fp_text reference J1 (at 0 6.096) (layer F.SilkS))
    (fp_text value SMA6251A13G50 (at 0 5.1) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Mlab_CON:SMA6251A13G50 locked (layer F.Cu) (tedit 58902C63)
    (at 50.8 -20.32)
    (fp_text reference J2 (at 0 7.112) (layer F.SilkS))
    (fp_text value SMA6251A13G50 (at 0 5.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module Mlab_R:SMD-1812 (layer B.Cu) (tedit 58902C63)
    (at 17.526 -27.178 270)
    (tags "CMS SMD")
    (attr smd)
    (fp_text reference L1 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value DL4N-100uH (at 0.762 0 180) (layer B.SilkS))
    (pad 2 smd rect (at 2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 19.304 -20.32 180)
    (attr smd)
    (fp_text reference L2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nH (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 22.098 -19.304 90)
    (attr smd)
    (fp_text reference L3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nH (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 26.924 -22.352 180)
    (attr smd)
    (fp_text reference L4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 29.718 -19.304 90)
    (attr smd)
    (fp_text reference L5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nH (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 34.544 -22.352 180)
    (attr smd)
    (fp_text reference L6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 37.338 -19.304 90)
    (attr smd)
    (fp_text reference L7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 33nH (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58902C63)
    (at 42.164 -20.32)
    (attr smd)
    (fp_text reference L10 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nH (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1812 (layer B.Cu) (tedit 58902C63)
    (at 43.688 -27.178 270)
    (tags "CMS SMD")
    (attr smd)
    (fp_text reference L11 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value DL4N-100uH (at 0.762 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2.286 0 270) (size 1.397 3.81) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 58902C63)
    (at 55.88 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 58902C63)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 58902C63)
    (at 55.88 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 58902C63)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 in" (at 30.48 -43.9204) (layer Dwgs.User))
    (feature1 (pts (xy 60.706 -40.132) (xy 60.706 -45.2704)))
    (feature2 (pts (xy 0.254 -40.132) (xy 0.254 -45.2704)))
    (crossbar (pts (xy 0.254 -42.5704) (xy 60.706 -42.5704)))
    (arrow1a (pts (xy 60.706 -42.5704) (xy 59.579496 -41.983979)))
    (arrow1b (pts (xy 60.706 -42.5704) (xy 59.579496 -43.156821)))
    (arrow2a (pts (xy 0.254 -42.5704) (xy 1.380504 -41.983979)))
    (arrow2b (pts (xy 0.254 -42.5704) (xy 1.380504 -43.156821)))
  )
  (dimension 39.878 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5700 in" (at 65.866 -20.193 90) (layer Dwgs.User))
    (feature1 (pts (xy 60.452 -40.132) (xy 67.216 -40.132)))
    (feature2 (pts (xy 60.452 -0.254) (xy 67.216 -0.254)))
    (crossbar (pts (xy 64.516 -0.254) (xy 64.516 -40.132)))
    (arrow1a (pts (xy 64.516 -40.132) (xy 65.102421 -39.005496)))
    (arrow1b (pts (xy 64.516 -40.132) (xy 63.929579 -39.005496)))
    (arrow2a (pts (xy 64.516 -0.254) (xy 65.102421 -1.380504)))
    (arrow2b (pts (xy 64.516 -0.254) (xy 63.929579 -1.380504)))
  )
  (gr_text OUT (at 50.8 -26.67) (layer F.SilkS))
  (gr_text IN (at 10.16 -26.67) (layer F.SilkS))
  (gr_text 2017 (at 39.878 -6.604) (layer F.SilkS))
  (gr_text JACHO,KAKLIK (at 39.878 -9.398) (layer F.SilkS))
  (gr_text BP01B (at 15.24 -35.052) (layer F.SilkS))
  (gr_text MLAB.CZ (at 15.24 -37.592) (layer F.SilkS))
  (gr_text JACHO,KAKLIK (at 20.32 -9.398) (layer B.Cu))
  (gr_text 2017 (at 20.32 -6.35) (layer B.Cu))
  (gr_text BP01B (at 44.704 -6.35) (layer B.Cu))
  (gr_text MLAB.CZ (at 44.704 -9.398) (layer B.Cu))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.706 -0.254) (end 0.254 -0.254) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.706 -40.386) (end 60.706 -0.254) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 60.706 -40.386) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.27 -41.656) (xy 62.23 -41.656) (xy 62.484 3.556) (xy -5.842 5.08)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.81 -42.926) (xy 66.548 -43.688) (xy 66.04 8.89) (xy -11.684 9.652)
      )
    )
  )
)
