(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 76)
    (no_connects 0)
    (area -6.604 -45.4585 38.892929 4.826001)
    (thickness 1.6)
    (drawings 33)
    (tracks 178)
    (zones 0)
    (modules 31)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /TX)
  (net 5 /RX)
  (net 6 /#RES)
  (net 7 /#WAK)
  (net 8 /G0)
  (net 9 /G1)
  (net 10 /G2)
  (net 11 /G3)
  (net 12 /G4)
  (net 13 /G5)
  (net 14 /G6)
  (net 15 "Net-(J15-Pad2)")
  (net 16 /SDA)
  (net 17 /SCL)
  (net 18 /G7)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net /#RES)
    (add_net /#WAK)
    (add_net /G0)
    (add_net /G1)
    (add_net /G2)
    (add_net /G3)
    (add_net /G4)
    (add_net /G5)
    (add_net /G6)
    (add_net /G7)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(J15-Pad2)")
    (add_net VCC)
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 5513237A)
    (at 13.97 -35.56 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132330)
    (at 5.08 -13.589)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /TX))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /TX))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132333)
    (at 5.08 -11.049)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RX))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RX))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132329)
    (at 5.08 -18.669 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /#RES))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /#RES))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5513232D)
    (at 5.08 -16.129)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /#WAK))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /#WAK))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 551313A2)
    (at 25.4 -27.305)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J6 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5513233F)
    (at 11.557 -4.826 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /G0))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /G0))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132341)
    (at 14.097 -4.826 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /G1))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /G1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132345)
    (at 16.637 -4.826 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /G2))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /G2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5513234A)
    (at 19.177 -4.826 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /G3))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /G3))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5513230D)
    (at 5.08 -27.432 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /G4))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /G4))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132311)
    (at 5.08 -24.892)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /G5))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /G5))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132318)
    (at 5.08 -22.352 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J13 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /G6))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /G6))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55132309)
    (at 5.08 -29.972)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J14 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /G7))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /G7))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 5513139C)
    (at 16.51 -20.574 270)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J15 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 5.08 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54 270) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 0 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J15-Pad2)"))
    (pad 1 thru_hole rect (at 0 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5513139F)
    (at 25.4 -15.748)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J16 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA))
    (pad 5 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J15-Pad2)"))
    (pad 6 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J15-Pad2)"))
    (pad 7 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCL))
    (pad 8 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCL))
    (pad 9 thru_hole rect (at -1.27 5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole rect (at 1.27 5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 55102FC1)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 55102FD0)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 55102FC4)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 55102FCC)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 14.732 -24.892 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 270) (layer B.SilkS))
    (fp_text value LE33CD (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.59 -16.891 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J15-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.59 -13.081 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J15-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.017 -18.796 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 450) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /#WAK))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 11.176 -18.796 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /#RES))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 5511013C)
    (at 20.574 -24.638 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0.635 0 90) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 55110149)
    (at 12.573 -29.972)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 18.288 -18.034)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 55110174)
    (at 19.558 -29.972)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -3.556) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -25.654 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 55110194)
    (at 16.129 -13.843 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -0.127 -0.508 180) (layer B.SilkS))
    (fp_text value SC18IM700 (at 0 -3.55 180) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /G0))
    (pad 2 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 /G1))
    (pad 3 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /#RES))
    (pad 4 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 /G2))
    (pad 6 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /G3))
    (pad 7 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA))
    (pad 8 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 /SCL))
    (pad 9 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /RX))
    (pad 10 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /TX))
    (pad 11 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /G6))
    (pad 12 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 13 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 /#WAK))
    (pad 14 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /G5))
    (pad 15 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 /G4))
    (pad 16 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 18 /G7))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 v" (at 33.6715 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 35.0215 -40.386)))
    (feature2 (pts (xy 30.226 -0.254) (xy 35.0215 -0.254)))
    (crossbar (pts (xy 32.3215 -0.254) (xy 32.3215 -40.386)))
    (arrow1a (pts (xy 32.3215 -40.386) (xy 32.907921 -39.259496)))
    (arrow1b (pts (xy 32.3215 -40.386) (xy 31.735079 -39.259496)))
    (arrow2a (pts (xy 32.3215 -0.254) (xy 32.907921 -1.380504)))
    (arrow2b (pts (xy 32.3215 -0.254) (xy 31.735079 -1.380504)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 v" (at 15.24 -43.9585) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 30.226 -45.3085)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -45.3085)))
    (crossbar (pts (xy 0.254 -42.6085) (xy 30.226 -42.6085)))
    (arrow1a (pts (xy 30.226 -42.6085) (xy 29.099496 -42.022079)))
    (arrow1b (pts (xy 30.226 -42.6085) (xy 29.099496 -43.194921)))
    (arrow2a (pts (xy 0.254 -42.6085) (xy 1.380504 -42.022079)))
    (arrow2b (pts (xy 0.254 -42.6085) (xy 1.380504 -43.194921)))
  )
  (gr_text JACHO (at 20.574 -35.814 90) (layer B.Cu))
  (gr_text 2015 (at 9.017 -35.56 270) (layer F.SilkS))
  (gr_text MLAB.cz (at 19.939 -34.544 90) (layer F.SilkS))
  (gr_text I2C232V01A (at 1.524 -21.209 90) (layer F.SilkS))
  (gr_text G3 (at 17.78 -8.509) (layer F.SilkS))
  (gr_text G1 (at 14.097 -7.62 90) (layer F.SilkS))
  (gr_text G2 (at 16.637 -7.62 90) (layer F.SilkS))
  (gr_text G0 (at 11.938 -7.62 90) (layer F.SilkS))
  (gr_text 3.3V (at 19.304 -22.352 90) (layer F.SilkS))
  (gr_text Vin (at 14.0335 -22.2885 90) (layer F.SilkS))
  (gr_text VI2C (at 16.5735 -22.225 90) (layer F.SilkS))
  (gr_text "3.3 V" (at 29.083 -27.305 90) (layer F.SilkS))
  (gr_text Vin (at 13.97 -31.75) (layer F.SilkS))
  (gr_text POWER (at 14.097 -39.243) (layer F.SilkS))
  (gr_text GND (at 22.479 -10.668) (layer F.SilkS))
  (gr_text SCL (at 22.479 -13.208) (layer F.SilkS))
  (gr_text VI2C (at 22.479 -15.875) (layer F.SilkS))
  (gr_text SDA (at 22.479 -18.161) (layer F.SilkS))
  (gr_text I2C (at 29.083 -15.748 90) (layer F.SilkS))
  (gr_text RX (at 7.8105 -10.8585) (layer F.SilkS))
  (gr_text TX (at 7.9375 -13.335) (layer F.SilkS))
  (gr_text "#WAK" (at 7.874 -15.875) (layer F.SilkS))
  (gr_text "#RES" (at 7.874 -18.161) (layer F.SilkS))
  (gr_text G6 (at 7.874 -22.352) (layer F.SilkS))
  (gr_text G5 (at 7.874 -24.892) (layer F.SilkS))
  (gr_text G4 (at 7.874 -27.432) (layer F.SilkS))
  (gr_text G7 (at 7.874 -29.972) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.226 -40.386) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.397 -40.894) (xy 34.544 -40.64) (xy 33.528 2.667) (xy -2.286 2.413)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.794 -41.91) (xy 36.703 -42.672) (xy 35.433 4.826) (xy -6.604 3.937) (xy -5.715 3.81)
      )
    )
  )
)
