(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 111)
    (no_connects 0)
    (area 0.205999 -30.274001 40.434001 9.954001)
    (thickness 1.6)
    (drawings 48)
    (tracks 216)
    (zones 0)
    (modules 38)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /#RES)
  (net 4 /#INT)
  (net 5 /SCL)
  (net 6 /SDA)
  (net 7 /A0)
  (net 8 /Vccp)
  (net 9 /P01)
  (net 10 /P00)
  (net 11 /P07)
  (net 12 /P06)
  (net 13 /P02)
  (net 14 /P05)
  (net 15 /P04)
  (net 16 /P03)
  (net 17 /P11)
  (net 18 /P10)
  (net 19 /P17)
  (net 20 /P16)
  (net 21 /P12)
  (net 22 /P15)
  (net 23 /P14)
  (net 24 /P13)
  (net 25 "Net-(J2-Pad3)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /#INT)
    (add_net /#RES)
    (add_net /A0)
    (add_net /P00)
    (add_net /P01)
    (add_net /P02)
    (add_net /P03)
    (add_net /P04)
    (add_net /P05)
    (add_net /P06)
    (add_net /P07)
    (add_net /P10)
    (add_net /P11)
    (add_net /P12)
    (add_net /P13)
    (add_net /P14)
    (add_net /P15)
    (add_net /P16)
    (add_net /P17)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(J2-Pad3)")
  )
  (net_class vdd ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /Vccp)
    (add_net VDD)
  )
  (module Hrebinky:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 54758468)
    (at 35.56 -15.24 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at 1.778 10.922 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 8.89 -3.937 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCL))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 11.303 -13.335 90)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /#INT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 8.89 -7.62 90)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /SDA))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 13.716 -13.335 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /#RES))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 29.21 -26.67 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /P07))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 11.43 6.477 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 /P17))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 26.67 -26.67 270)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /P06))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 21.59 6.477 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /P13))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 24.13 -26.67 270)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /P05))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 16.51 6.477 90)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 /P15))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 21.59 -26.67 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /P04))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 19.05 6.477 90)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /P14))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 19.05 -26.67 270)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /P03))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 13.97 6.477 90)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 /P16))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 13.97 -26.67 270)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 /P01))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 16.51 -26.67 270)
    (attr smd)
    (fp_text reference R16 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /P02))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 24.13 6.477 90)
    (attr smd)
    (fp_text reference R17 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 /P12))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 11.43 -26.67 270)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 /P00))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D2AF)
    (at 26.67 6.477 90)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /P11))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5469D57A)
    (at 29.21 6.477 90)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.016 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 /P10))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module IO:TSSOP-28 (layer B.Cu) (tedit 5469DD7B)
    (at 21.082 -9.398)
    (descr TSSOP-28)
    (attr smd)
    (fp_text reference U1 (at 0 -0.508) (layer B.SilkS))
    (fp_text value TCA6416A (at 0 1.143) (layer B.SilkS))
    (pad 7 smd rect (at -0.32512 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 16 /P03))
    (pad 8 smd rect (at 0.32512 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 15 /P04))
    (pad 9 smd rect (at 0.97536 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 14 /P05))
    (pad 10 smd rect (at 1.6256 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 12 /P06))
    (pad 21 smd rect (at -2.26568 2.794) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 7 /A0))
    (pad 4 smd rect (at -2.27584 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 10 /P00))
    (pad 5 smd rect (at -1.6256 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 9 /P01))
    (pad 6 smd rect (at -0.97536 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 13 /P02))
    (pad 14 smd rect (at 2.27584 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 17 /P11))
    (pad 15 smd rect (at 1.6256 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 21 /P12))
    (pad 16 smd rect (at 0.97536 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 24 /P13))
    (pad 17 smd rect (at 0.32512 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 23 /P14))
    (pad 18 smd rect (at -0.32512 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 22 /P15))
    (pad 19 smd rect (at -0.97536 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 20 /P16))
    (pad 11 smd rect (at 2.27584 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 11 /P07))
    (pad 20 smd rect (at -1.6256 2.794) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 19 /P17))
    (pad 3 smd rect (at -2.92608 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 3 /#RES))
    (pad 12 smd rect (at 2.92608 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.92608 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 18 /P10))
    (pad 22 smd rect (at -2.92608 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCL))
    (pad 2 smd rect (at -3.57378 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 23 smd rect (at -3.57378 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 6 /SDA))
    (pad 1 smd rect (at -4.22402 -2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 4 /#INT))
    (pad 24 smd rect (at -4.22402 2.79908) (size 0.4191 1.47066) (layers B.Cu B.Paste B.Mask)
      (net 8 /Vccp))
    (model smd/smd_dil/tssop-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54748171)
    (at 11.303 -8.636 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J8 (at 2.54 32.893 90) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500C0F4)
    (at 5.08 5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500C0BB)
    (at 35.56 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500C0BF)
    (at 5.05 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500C0B6)
    (at 35.56 5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Hrebinky:Pin_Header_Straight_2x02 placed (layer F.Cu) (tedit 54758675)
    (at 5.08 -16.51 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 8.128 10.922 270) (layer F.SilkS) hide)
    (fp_text value JUMP_2X2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /#RES))
    (pad 2 thru_hole rect (at 1.27 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /#INT))
    (pad 3 thru_hole rect (at 1.27 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /#INT))
    (pad 4 thru_hole rect (at -1.27 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /#RES))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 54758679)
    (at 5.08 -6.35 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at 0.127 -9.271 90) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 1.27 0 90) (layer F.SilkS) hide)
    (pad 9 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL))
    (pad 5 thru_hole rect (at 5.08 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad3)"))
    (pad 6 thru_hole rect (at 5.08 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.08 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL))
    (pad 4 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDA))
    (pad 10 thru_hole rect (at -5.08 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDA))
    (pad 8 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54758671)
    (at 14.097 -8.636 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at -2.032 19.812 270) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole rect (at 1.27 0.127 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /Vccp))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x08 placed (layer F.Cu) (tedit 5475866D)
    (at 20.32 -21.59)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at -25.527 7.747) (layer F.SilkS) hide)
    (fp_text value JUMP_8X2 (at 5.08 0) (layer F.SilkS) hide)
    (pad 15 thru_hole rect (at -6.35 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /P01))
    (pad 16 thru_hole rect (at -8.89 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 /P00))
    (pad 8 thru_hole rect (at 8.89 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 /P07))
    (pad 7 thru_hole rect (at 6.35 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /P06))
    (pad 14 thru_hole rect (at -3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 /P02))
    (pad 6 thru_hole rect (at 3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 /P05))
    (pad 12 thru_hole rect (at 1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 15 /P04))
    (pad 9 thru_hole rect (at 8.89 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 /P07))
    (pad 5 thru_hole rect (at 1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 15 /P04))
    (pad 3 thru_hole rect (at -3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 /P02))
    (pad 11 thru_hole rect (at 3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 /P05))
    (pad 1 thru_hole rect (at -8.89 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 /P00))
    (pad 2 thru_hole rect (at -6.35 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /P01))
    (pad 4 thru_hole rect (at -1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /P03))
    (pad 10 thru_hole rect (at 6.35 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /P06))
    (pad 13 thru_hole rect (at -1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /P03))
    (model Pin_Headers/Pin_Header_Straight_2x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x08 placed (layer F.Cu) (tedit 5475866A)
    (at 20.32 1.27 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at 29.845 19.558 180) (layer F.SilkS) hide)
    (fp_text value JUMP_8X2 (at 5.08 0 180) (layer F.SilkS) hide)
    (pad 15 thru_hole rect (at -6.35 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 17 /P11))
    (pad 16 thru_hole rect (at -8.89 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 18 /P10))
    (pad 8 thru_hole rect (at 8.89 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 19 /P17))
    (pad 7 thru_hole rect (at 6.35 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 20 /P16))
    (pad 14 thru_hole rect (at -3.81 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 /P12))
    (pad 6 thru_hole rect (at 3.81 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 22 /P15))
    (pad 12 thru_hole rect (at 1.27 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 23 /P14))
    (pad 9 thru_hole rect (at 8.89 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 19 /P17))
    (pad 5 thru_hole rect (at 1.27 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 23 /P14))
    (pad 3 thru_hole rect (at -3.81 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 /P12))
    (pad 11 thru_hole rect (at 3.81 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 22 /P15))
    (pad 1 thru_hole rect (at -8.89 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 18 /P10))
    (pad 2 thru_hole rect (at -6.35 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 17 /P11))
    (pad 4 thru_hole rect (at -1.27 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 24 /P13))
    (pad 10 thru_hole rect (at 6.35 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 20 /P16))
    (pad 13 thru_hole rect (at -1.27 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 24 /P13))
    (model Pin_Headers/Pin_Header_Straight_2x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5475DA3A)
    (at 34.417 -6.35)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 8.255 -2.667) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /#RES))
    (pad 2 thru_hole rect (at 1.27 0.127) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5475DBFA)
    (at 34.417 -3.556 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J9 (at -11.176 -1.27 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0.127 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A0))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5475D670)
    (at 27.178 -7.366 270)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /A0))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5475D7F0)
    (at 27.178 -11.176 90)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5475D7F0)
    (at 29.972 -11.176 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 54928708)
    (at 29.972 -16.002)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0.254 2.286) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ":X 0x23" (at 26.035 -10.033) (layer F.SilkS))
  (gr_text Vcc (at 11.303 -3.175 90) (layer F.SilkS))
  (gr_text VCCP (at 13.97 -5.842 90) (layer F.SilkS))
  (gr_text VDD (at 11.176 -12.446) (layer F.SilkS))
  (gr_text I2CIO01A (at 35.56 0.254) (layer B.Cu))
  (gr_text MLAB.CZ (at 31.1785 4.8895 90) (layer B.Cu))
  (gr_text 2015 (at 35.306 0) (layer F.SilkS))
  (gr_text JACHO (at 5.08 -20.32) (layer F.SilkS))
  (gr_text I2CIO01A (at 20.828 -10.16 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 18.542 -10.16 90) (layer F.SilkS))
  (gr_text P07 (at 29.21 -24.892 90) (layer F.SilkS))
  (gr_text P06 (at 26.67 -24.892 90) (layer F.SilkS))
  (gr_text P05 (at 24.13 -24.892 90) (layer F.SilkS))
  (gr_text P04 (at 21.59 -24.892 90) (layer F.SilkS))
  (gr_text P03 (at 19.05 -24.892 90) (layer F.SilkS))
  (gr_text P02 (at 16.51 -24.892 90) (layer F.SilkS))
  (gr_text "P01\n" (at 13.97 -24.892 90) (layer F.SilkS))
  (gr_text P00 (at 11.43 -24.892 90) (layer F.SilkS))
  (gr_text P10 (at 29.21 4.572 90) (layer F.SilkS))
  (gr_text P11 (at 26.67 4.572 90) (layer F.SilkS))
  (gr_text P12 (at 24.13 4.572 90) (layer F.SilkS))
  (gr_text P13 (at 21.59 4.572 90) (layer F.SilkS))
  (gr_text P14 (at 19.05 4.572 90) (layer F.SilkS))
  (gr_text P15 (at 16.51 4.572 90) (layer F.SilkS))
  (gr_text P16 (at 13.97 4.572 90) (layer F.SilkS))
  (gr_text P17 (at 11.43 4.572 90) (layer F.SilkS))
  (gr_text "MAX 3.6V" (at 39.37 -15.494 90) (layer F.SilkS))
  (gr_text POWER (at 35.56 -20.32) (layer F.SilkS))
  (gr_text SCL (at 1.397 -1.524 90) (layer F.SilkS))
  (gr_text SDA (at 1.524 -6.731 90) (layer F.SilkS))
  (gr_text GND (at 8.636 -10.16 90) (layer F.SilkS))
  (gr_text GND (at 5.08 1.016) (layer F.SilkS))
  (gr_text "#INT" (at 8.382 -15.24) (layer F.SilkS))
  (gr_text "#RES" (at 8.382 -17.78) (layer F.SilkS))
  (gr_text ": 0x21\nY 0x20" (at 28.956 -4.191) (layer F.SilkS))
  (gr_text ADDRESS (at 26.797 -13.335) (layer F.SilkS))
  (gr_text "SET ADR" (at 34.544 -8.636) (layer F.SilkS))
  (gr_text "YX 0x22" (at 25.781 -6.985) (layer F.SilkS))
  (gr_text "Y: 0x26" (at 26.035 -8.509) (layer F.SilkS))
  (gr_text ":: 0x27\n" (at 26.289 -11.557) (layer F.SilkS))
  (gr_text Y (at 30.607 -3.683) (layer F.SilkS))
  (gr_text X (at 30.607 -6.223) (layer F.SilkS))
  (gr_line (start 0.256 9.904) (end 0.256 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -30.224) (end 40.384 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.384 9.904) (end 40.384 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 9.904) (end 40.384 9.904) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.445 -33.782) (xy -5.334 11.938) (xy 50.292 13.208) (xy 48.26 -39.116)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.879 11.43) (xy -2.159 10.922) (xy -1.905 -32.512) (xy 47.117 -32.385)
      )
    )
  )
)
