(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 83)
    (no_connects 0)
    (area 0.205999 -30.274001 50.594001 -0.205999)
    (thickness 1.6)
    (drawings 19)
    (tracks 266)
    (zones 0)
    (modules 39)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.13)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 GND)
  (net 4 V+)
  (net 5 "Net-(C4-Pad1)")
  (net 6 V-)
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C11-Pad2)")
  (net 10 "Net-(C12-Pad2)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "Net-(C13-Pad2)")
  (net 13 "Net-(C14-Pad2)")
  (net 14 /#SHDN)
  (net 15 /+Ubias)
  (net 16 /K)
  (net 17 /A)
  (net 18 "Net-(C15-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /#SHDN)
    (add_net /+Ubias)
    (add_net /A)
    (add_net /K)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net V+)
    (add_net V-)
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.685 -11.684 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2M (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /A))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 26.035 -15.875 90)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.732 -18.542 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4u7 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /K))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54F98308)
    (at 24.13 -8.255 270)
    (attr smd)
    (fp_text reference C2 (at -0.0254 -1.2192 270) (layer B.SilkS))
    (fp_text value 12p (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 40.005 -23.495 90)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.465 -23.495 90)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.94 -9.525)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.305 -12.573 180)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 330nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 28.575 -15.875 90)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.9146 -7.6708)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.941 -11.557 90)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 510pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.672 -13.716 90)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 560pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.1348 -19.3802 90)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 150pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.878 -20.3708)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 330nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C14-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 5482DC61)
    (at 6.35 -16.51 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 5.0165 1.778 180) (layer F.SilkS))
    (fp_text value JUMP_3X2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 15 /+Ubias))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 15 /+Ubias))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 53F5A718)
    (at 30.2768 -3.81)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at 7.9502 -3.4925) (layer F.SilkS))
    (fp_text value JUMP_5X2 (at 1.27 0) (layer F.SilkS) hide)
    (pad 9 thru_hole rect (at -2.54 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 V-))
    (pad 5 thru_hole rect (at 5.08 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (pad 3 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 V+))
    (pad 6 thru_hole rect (at 5.08 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at -5.08 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at -2.54 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 V-))
    (pad 4 thru_hole rect (at 2.54 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 V-))
    (pad 10 thru_hole rect (at -5.08 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 7 thru_hole rect (at 2.54 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 V-))
    (pad 8 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 V+))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5469CB53)
    (at 25.654 -22.86 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 0 -2.286 90) (layer F.SilkS))
    (fp_text value CONN1_2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 /#SHDN))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 V+))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 5482DC61)
    (at 46.4566 -16.8656 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at -5.0546 1.2954 180) (layer F.SilkS))
    (fp_text value Out (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad2)"))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad2)"))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 55134324)
    (at 45.72 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 3 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5513432A)
    (at 45.72 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 3 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5513431C)
    (at 5.08 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 3 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 55134321)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 3 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.732 -22.225 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.2743 -16.51 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /+Ubias))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.988 -11.43 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3556 90) (layer B.SilkS))
    (fp_text value 3k3 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 38.354 -11.557 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.401 -11.43 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1k5 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 locked (layer B.Cu) (tedit 54799E0C)
    (at 40.386 -13.716 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.1348 -16.0274 90)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.1668 -17.6276 90)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 3k9 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.5196 -17.526 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SOT-23 (layer B.Cu) (tedit 54836E42)
    (at 21.59 -16.51)
    (tags SOT23)
    (fp_text reference Q1 (at 1.99898 0.09906 270) (layer B.SilkS))
    (fp_text value BF862 (at 0.0635 0) (layer B.SilkS))
    (pad 3 smd rect (at 0 1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 17 /A))
    (pad 2 smd rect (at 0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 1 smd rect (at -0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Hrebinky:CONN_3_2 (layer F.Cu) (tedit 54837E65)
    (at 17.145 -14.605)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at 5.334 0.0635) (layer F.SilkS))
    (fp_text value CONN1_2 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /K))
    (pad 2 thru_hole rect (at 2.54 0) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SOT-23-6 (layer B.Cu) (tedit 54843902)
    (at 23.368 -12.573 180)
    (fp_text reference U1 (at -0.2032 0.0254 450) (layer B.SilkS))
    (fp_text value MAX4475 (at 0.0635 0 180) (layer B.SilkS))
    (pad 6 smd rect (at -0.9525 1.27 180) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 5 smd rect (at 0 1.27 180) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 14 /#SHDN))
    (pad 4 smd rect (at 0.9525 1.27 180) (size 0.50104 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 17 /A))
    (pad 3 smd rect (at 0.9525 -1.27 180) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0 -1.27 180) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (pad 1 smd rect (at -0.9525 -1.27 180) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 22.225 -8.255 90)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2M (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 11.2776 -19.2151 90)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1u (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 11.303 -14.605 180)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /K))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C15-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:2pF_PCB (layer F.Cu) (tedit 5511B4FF)
    (at 14.2494 -7.5311)
    (fp_text reference C4 (at -0.0254 0.1143) (layer F.SilkS))
    (fp_text value 2pF (at 0 5.715) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 9.480265 9.480265) (layers F.Cu)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd circle (at 0 0) (size 9.480265 9.480265) (layers B.Cu)
      (net 17 /A))
  )
  (module SMD_Packages:SOIC-8-N (layer B.Cu) (tedit 0)
    (at 33.02 -18.415 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value AD8692 (at 0 -1.27 180) (layer B.SilkS))
    (pad 8 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 4 V+))
    (pad 7 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (pad 6 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 5 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 6 V-))
    (pad 3 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (model SMD_Packages/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 v" (at 53.8264 -15.24 90) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -30.226) (xy 55.1764 -30.226)))
    (feature2 (pts (xy 50.546 -0.254) (xy 55.1764 -0.254)))
    (crossbar (pts (xy 52.4764 -0.254) (xy 52.4764 -30.226)))
    (arrow1a (pts (xy 52.4764 -30.226) (xy 53.062821 -29.099496)))
    (arrow1b (pts (xy 52.4764 -30.226) (xy 51.889979 -29.099496)))
    (arrow2a (pts (xy 52.4764 -0.254) (xy 53.062821 -1.380504)))
    (arrow2b (pts (xy 52.4764 -0.254) (xy 51.889979 -1.380504)))
  )
  (dimension 50.292 (width 0.3) (layer Dwgs.User)
    (gr_text "1,9800 v" (at 25.4 -34.878) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -30.226) (xy 50.546 -36.228)))
    (feature2 (pts (xy 0.254 -30.226) (xy 0.254 -36.228)))
    (crossbar (pts (xy 0.254 -33.528) (xy 50.546 -33.528)))
    (arrow1a (pts (xy 50.546 -33.528) (xy 49.419496 -32.941579)))
    (arrow1b (pts (xy 50.546 -33.528) (xy 49.419496 -34.114421)))
    (arrow2a (pts (xy 0.254 -33.528) (xy 1.380504 -32.941579)))
    (arrow2b (pts (xy 0.254 -33.528) (xy 1.380504 -34.114421)))
  )
  (gr_text PCRD01A (at 33.02 -14.7955) (layer F.SilkS))
  (gr_text 2015 (at 15.4305 -24.4475) (layer F.SilkS))
  (gr_text MLAB.cz (at 15.494 -26.9875) (layer F.SilkS))
  (gr_text Power (at 30.4165 -9.7155) (layer F.SilkS))
  (gr_text - (at 32.893 -7.366) (layer F.SilkS))
  (gr_text + (at 30.226 -7.6835) (layer F.SilkS))
  (gr_text - (at 27.7495 -7.366) (layer F.SilkS))
  (gr_text GND (at 22.5425 -3.81 90) (layer F.SilkS))
  (gr_text GND (at 38.1635 -3.7465 90) (layer F.SilkS))
  (gr_text Output (at 42.2275 -16.7005 90) (layer F.SilkS))
  (gr_text "#SHDN" (at 28.448 -22.352 90) (layer F.SilkS))
  (gr_text Sensor (at 17.272 -17.4625) (layer F.SilkS))
  (gr_text Ubias (at 2.3495 -16.383 90) (layer F.SilkS))
  (gr_line (start 0.256 -30.224) (end 50.544 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.544 -30.224) (end 50.544 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -0.256) (end 50.544 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -0.256) (end 0.256 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.31 -40.64) (xy 63.246 4.953) (xy 21.844 4.445) (xy 21.844 1.143) (xy -1.016 1.143)
        (xy -0.381 -33.528) (xy 25.019 -30.353) (xy 27.305 -33.528) (xy 67.31 -40.64)
      )
    )
    (polygon
      (pts        (xy 26.797 -8.382) (xy 26.797 -16.002) (xy 25.019 -16.002) (xy 22.7076 -20.193) (xy 12.32916 -20.15236)
        (xy 12.34948 -16.85036) (xy 4.318 -16.891) (xy 4.318 -15.3416) (xy 9.271 -15.3416) (xy 9.271 -11.43)
        (xy 8.382 -10.541) (xy 8.382 -1.778) (xy 21.2344 -1.778) (xy 21.2344 -8.382) (xy 26.797 -8.382)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.826 -32.004) (xy 65.532 -31.877) (xy 64.262 2.921) (xy -5.207 2.921)
      )
    )
  )
)
