(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 60)
    (no_connects 0)
    (area -3.556 -42.672 43.180001 2.540001)
    (thickness 1.6)
    (drawings 12)
    (tracks 168)
    (zones 0)
    (modules 34)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.7)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /K)
  (net 2 /A)
  (net 3 GNDA)
  (net 4 GND)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A)
    (add_net /K)
    (add_net GND)
    (add_net GNDA)
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 21.844 -28.448)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D1 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 21.844 -23.876)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D2 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 29.972 -23.876)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D3 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 5.588 -19.304)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D4 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 37.084 -26.416 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D5 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 5.588 -23.876)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D6 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -23.876)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D7 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 29.972 -10.16)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D8 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -5.08)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D9 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 29.972 -28.448)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D10 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 27.432 -35.052 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D11 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -28.448)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D12 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 12.192 -35.052 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D13 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 21.844 -19.304)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D14 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 29.972 -19.304)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D15 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -19.304)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D16 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 17.272 -35.052 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D17 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 22.352 -35.052 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D18 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 5.588 -28.448)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D19 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 29.972 -14.732)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D20 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 21.336 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.876 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /K))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /K))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 26.416 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GNDA))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 28.956 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 4 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -14.732)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D21 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 5.588 -14.732)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D22 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 21.844 -14.732)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D23 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 21.844 -10.16)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D24 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 13.716 -10.16)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D25 (at -0.0635 0.0127) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:DIL (layer B.Cu) (tedit 57A82D64)
    (at 37.084 -17.272 90)
    (descr DIL)
    (tags "DIL - BPW34S ")
    (attr smd)
    (fp_text reference D26 (at -0.0635 0.0127 90) (layer B.SilkS))
    (fp_text value BPW34S (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -3.05 0 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /A))
    (pad 1 smd rect (at 3.05 0 90) (size 1.4 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /K))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 28.956 -9.144 90) (layer F.SilkS))
  (gr_text GNDA (at 26.416 -9.144 90) (layer F.SilkS))
  (gr_text K (at 23.876 -7.62 90) (layer F.SilkS))
  (gr_text A (at 21.336 -7.62 90) (layer F.SilkS))
  (gr_text 2016 (at 33.528 -18.796) (layer F.SilkS))
  (gr_text JACHO (at 33.528 -20.828) (layer F.SilkS))
  (gr_text PIND01A (at 13.716 -30.48) (layer F.SilkS))
  (gr_text MLAB.CZ (at 13.716 -32.512) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -0.254) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -40.386) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 40.386 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.656 1.524) (xy -1.524 1.524) (xy -1.524 -41.148) (xy 41.656 -41.148) (xy 41.656 1.524)
      )
    )
  )
  (zone (net 3) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.592 -3.048) (xy 3.048 -3.048) (xy 3.048 -37.592) (xy 37.592 -37.592) (xy 37.592 -3.048)
      )
    )
  )
  (zone (net 3) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.18 2.54) (xy -3.556 2.54) (xy -3.556 -42.672) (xy 43.18 -42.672) (xy 43.18 2.54)
      )
    )
  )
)
