(kicad_pcb (version 20160815) (host pcbnew 201609251018+7233~55~ubuntu16.04.1-)
  (general
    (links 38)
    (no_connects 0)
    (area 35.155715 18.255 84.886716 56.60832)
    (thickness 1.6)
    (drawings 11)
    (tracks 89)
    (zones 0)
    (modules 18)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GNDA)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(J4-Pad1)")
  (net 7 "Net-(P1-Pad2)")
  (net 8 "Net-(R3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net GNDA)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 54.356 38.1 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 48.895 45.339 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 57ECEDA2)
    (at 54.483 30.353 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.3 90) (layer F.Fab))
    (fp_text user K (at -2.9 2.95 90) (layer F.SilkS))
    (fp_text user A (at 2.9 2.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer B.Cu) (tedit 57ECEDA2)
    (at 48.895 30.607 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 5.08 180) (layer B.SilkS) hide)
    (fp_text value HEADER_2x03_PARALLEL (at 0 -5.08 180) (layer B.SilkS) hide)
    (fp_text user 1 (at -2.921 2.54 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 2 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 1 VDD))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 1 VDD))
    (pad 5 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 6 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer B.Cu) (tedit 57ECEDA2)
    (at 67.183 40.64)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value INTENSITY (at 0 -2.54) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer B.Cu) (tedit 57ECEDA2)
    (at 67.183 43.18)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value RESET (at 0 -2.54) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(J3-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer B.Cu) (tedit 57ECEDA2)
    (at 67.183 38.1)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value INT_OUT (at 0 -2.54) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(J4-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ECEDA2)
    (at 71.12 30.48)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ECEDA2)
    (at 40.64 50.8)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ECEDA2)
    (at 40.64 30.48)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ECEDA2)
    (at 71.12 50.8)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Con:SMA6251A13G50 (layer B.Cu) (tedit 57ECEDA2)
    (at 42.672 40.64)
    (fp_text reference P1 (at 0 5.1) (layer B.SilkS))
    (fp_text value SMA (at 0 -5.1) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57ECEDA2)
    (at 52.705 45.466 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 48.9585 43.18 180)
    (attr smd)
    (fp_text reference R1 (at 0 -0.3175 180) (layer F.SilkS))
    (fp_text value 10k (at 0.127 0.381 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 56.388 48.7045 270)
    (attr smd)
    (fp_text reference R2 (at 0 -0.3175 270) (layer F.SilkS))
    (fp_text value 10M (at 0.127 0.381 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 57.3405 36.957)
    (attr smd)
    (fp_text reference R3 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value 10M (at 0.127 0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57ECEDA2)
    (at 60.96 36.957)
    (attr smd)
    (fp_text reference R4 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value 1M (at 0.127 0.381) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 57ECEDA2)
    (at 57.531 41.402 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value MCP6002 (at 0 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 5 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 7 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J4-Pad1)"))
    (pad 8 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Pulse_catch01A (at 55.88 50.4952) (layer B.SilkS))
  (gr_text INT_OUT (at 59.69 38.1) (layer B.SilkS))
  (gr_text INTENSITY (at 58.7248 40.7416) (layer B.SilkS))
  (gr_text RESET (at 60.6044 43.3324) (layer B.SilkS))
  (gr_text POWER (at 53.594 30.5308 90) (layer B.SilkS))
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 in" (at 79.201 40.64 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.946 25.654) (xy 80.551 25.654)))
    (feature2 (pts (xy 75.946 55.626) (xy 80.551 55.626)))
    (crossbar (pts (xy 77.851 55.626) (xy 77.851 25.654)))
    (arrow1a (pts (xy 77.851 25.654) (xy 78.437421 26.780504)))
    (arrow1b (pts (xy 77.851 25.654) (xy 77.264579 26.780504)))
    (arrow2a (pts (xy 77.851 55.626) (xy 78.437421 54.499496)))
    (arrow2b (pts (xy 77.851 55.626) (xy 77.264579 54.499496)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 55.88 19.605) (layer Dwgs.User))
    (feature1 (pts (xy 75.946 25.654) (xy 75.946 18.255)))
    (feature2 (pts (xy 35.814 25.654) (xy 35.814 18.255)))
    (crossbar (pts (xy 35.814 20.955) (xy 75.946 20.955)))
    (arrow1a (pts (xy 75.946 20.955) (xy 74.819496 21.541421)))
    (arrow1b (pts (xy 75.946 20.955) (xy 74.819496 20.368579)))
    (arrow2a (pts (xy 35.814 20.955) (xy 36.940504 21.541421)))
    (arrow2b (pts (xy 35.814 20.955) (xy 36.940504 20.368579)))
  )
  (gr_line (start 75.946 25.654) (end 35.814 25.654) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.946 55.626) (end 75.946 25.654) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 35.814 55.626) (end 75.946 55.626) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 35.814 25.654) (end 35.814 55.626) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.814 55.626) (xy 35.814 25.654) (xy 75.946 25.654) (xy 75.946 55.626)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.814 25.654) (xy 75.946 25.654) (xy 75.946 55.626) (xy 35.814 55.626)
      )
    )
  )
)
