(kicad_pcb (version 20160815) (host pcbnew 201609251018+7233~55~ubuntu16.04.1-)
  (general
    (links 36)
    (no_connects 0)
    (area 78.0288 58.6232 137.388516 108.051601)
    (thickness 1.6)
    (drawings 11)
    (tracks 71)
    (zones 0)
    (modules 18)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GNDA)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(P1-Pad1)")
  (net 7 "Net-(R3-Pad2)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "Net-(R5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net GNDA)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net VDD)
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer B.Cu) (tedit 57ED2017)
    (at 110.1344 83.5152 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 2.6 90) (layer B.SilkS))
    (fp_text value MCP6002 (at 0 -2.6 90) (layer B.Fab))
    (pad 1 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 5 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 6 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (pad 7 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 8 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 57ED2017)
    (at 114.046 81.1784)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 57ED2017)
    (at 104.7496 86.7664 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.667 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard locked (layer B.Cu) (tedit 57ED2017)
    (at 107.2388 71.5772 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 1 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 57ED2017)
    (at 100.3554 71.3486 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2x03_PARALLEL (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57ED2017)
    (at 120.269 83.0072 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value INTENSITY (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 locked (layer F.Cu) (tedit 57ED2017)
    (at 120.269 80.4672 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value INT_OUT (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J3-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J3-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ED2017)
    (at 91.44 91.44)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ED2017)
    (at 91.44 71.12)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ED2017)
    (at 121.92 71.12)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57ED2017)
    (at 121.92 91.44)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Con:SMA6251A13G50 (layer F.Cu) (tedit 57ED2017)
    (at 93.091 81.915)
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value SMA (at 0 5.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 98.679 82.042 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 104.7496 82.9056 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 10M (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 108.9152 78.232)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 112.2172 78.232)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10M (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 104.7496 76.0984 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0.1524 1.778 270) (layer B.SilkS))
    (fp_text value 10M (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57ED2017)
    (at 104.7496 79.502 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 10M (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 30.48 (width 0.3) (layer Dwgs.User)
    (gr_text "1,2000 in" (at 131.7028 81.28 90) (layer Dwgs.User))
    (feature1 (pts (xy 127 66.04) (xy 133.0528 66.04)))
    (feature2 (pts (xy 127 96.52) (xy 133.0528 96.52)))
    (crossbar (pts (xy 130.3528 96.52) (xy 130.3528 66.04)))
    (arrow1a (pts (xy 130.3528 66.04) (xy 130.939221 67.166504)))
    (arrow1b (pts (xy 130.3528 66.04) (xy 129.766379 67.166504)))
    (arrow2a (pts (xy 130.3528 96.52) (xy 130.939221 95.393496)))
    (arrow2b (pts (xy 130.3528 96.52) (xy 129.766379 95.393496)))
  )
  (dimension 40.640032 (width 0.3) (layer Dwgs.User)
    (gr_text "1,6000 in" (at 106.674688 61.816504 0.07161968709) (layer Dwgs.User))
    (feature1 (pts (xy 127 66.04) (xy 126.993001 60.441105)))
    (feature2 (pts (xy 86.36 66.0908) (xy 86.353001 60.491905)))
    (crossbar (pts (xy 86.356376 63.191903) (xy 126.996376 63.141103)))
    (arrow1a (pts (xy 126.996376 63.141103) (xy 125.870606 63.728931)))
    (arrow1b (pts (xy 126.996376 63.141103) (xy 125.86914 62.556091)))
    (arrow2a (pts (xy 86.356376 63.191903) (xy 87.483612 63.776915)))
    (arrow2b (pts (xy 86.356376 63.191903) (xy 87.482146 62.604075)))
  )
  (gr_text "Kaklik 2016" (at 106.8324 94.0816) (layer F.SilkS))
  (gr_text Pulse_catch01B (at 106.7816 91.0844) (layer F.SilkS))
  (gr_text INT_OUT (at 112.522 80.518) (layer F.SilkS))
  (gr_text INTENSITY (at 111.7092 83.312) (layer F.SilkS))
  (gr_text POWER (at 104.4448 71.374 90) (layer F.SilkS))
  (gr_line (start 86.614 96.266) (end 86.614 66.294) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.746 96.266) (end 86.614 96.266) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.746 66.294) (end 126.746 96.266) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.614 66.294) (end 126.746 66.294) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.36 66.04) (xy 86.36 96.52) (xy 127 96.52) (xy 127 66.04) (xy 86.4108 66.0908)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.9376 60.198) (xy 78.0288 108.0516) (xy 134.1628 103.8352) (xy 132.08 58.6232)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.0064 74.9808) (xy 102.0064 82.3468) (xy 103.4288 85.0392) (xy 106.3244 85.1408) (xy 106.3244 74.9808)
      )
    )
  )
)
