(kicad_pcb (version 4) (host pcbnew "(2015-05-13 BZR 5653)-product")
  (general
    (links 36)
    (no_connects 0)
    (area 0.203999 -9.448001 40.436001 0.304001)
    (thickness 1.6)
    (drawings 15)
    (tracks 99)
    (zones 0)
    (modules 19)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 /SCL)
  (net 7 /SDA)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net VDD)
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 38.735 -4.572 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 2 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1 0 270) (size 1 1) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole rect (at 1 0 270) (size 1 1) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer B.Cu) (tedit 5593DD71)
    (at 5.08 -4.572)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 4) (layer B.SilkS) hide)
    (fp_text value HOLE (at 0 -4) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer B.Cu) (tedit 5535DB2C)
    (at 25.4 -4.572)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 4) (layer B.SilkS) hide)
    (fp_text value HOLE (at 0 -4) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_IO:FN (layer B.Cu) (tedit 55950D99)
    (at 33.655 -4.699 180)
    (tags " TCS37717")
    (fp_text reference X1 (at 0.0762 -0.381 360) (layer B.SilkS))
    (fp_text value TCS37717 (at 0.0889 1.8796 180) (layer B.SilkS) hide)
    (pad 6 smd rect (at 0.75 0.65 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 7 /SDA))
    (pad 5 smd rect (at 0.75 0 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 4 smd rect (at 0.75 -0.65 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at -0.75 -0.65 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 0 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (pad 1 smd rect (at -0.75 0.65 180) (size 1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 55950446)
    (at 15.367 -3.302 90)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J1 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 4 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 5 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 6 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 7 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA))
    (pad 8 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA))
    (pad 9 thru_hole rect (at -1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole rect (at 1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.687 -1.524 90)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uf (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 31.115 -7.747 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.607 -1.524 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.655 -1.524 90)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.401 -7.747 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 22R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 55950439)
    (at 13.335 -7.366)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 4.572 0) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 559504F5)
    (at 31.115 -4.699)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2) (layer F.SilkS) hide)
    (fp_text user 1 (at -1 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:SMD_1x1 (layer F.Cu) (tedit 5594D1EF)
    (at 34.925 -3.175)
    (fp_text reference J4 (at -0.1016 2.9972) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -0.2032 -1.778) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module Mlab_Pin_Headers:SMD_1x1 (layer F.Cu) (tedit 5594D1EF)
    (at 34.925 -8.001)
    (fp_text reference J5 (at -0.1016 2.9972) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -0.2032 -1.778) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCL))
  )
  (module Mlab_Pin_Headers:SMD_1x1 (layer F.Cu) (tedit 5594D1EF)
    (at 34.925 -5.842)
    (fp_text reference J6 (at -0.1016 2.9972) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -0.2032 -1.778) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDA))
  )
  (module Mlab_Pin_Headers:SMD_1x1 (layer F.Cu) (tedit 5594D1EF)
    (at 34.925 -1.016)
    (fp_text reference J7 (at -0.1016 2.9972) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -0.2032 -1.778) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Mlab_D:LED_0805 (layer B.Cu) (tedit 559504FC)
    (at 37.465 -4.572 270)
    (attr smd)
    (fp_text reference D2 (at -1.016 1.3843 270) (layer B.SilkS))
    (fp_text value LL-S170IRC-2A (at 1.4351 1.3716 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.0668 -1.2954 270) (layer B.SilkS))
    (fp_text user A (at -0.9906 -1.27 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 38.481 -7.493 180)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.814 -7.747 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text MLAB (at 6.477 -8.382) (layer B.Cu))
  (gr_text RGBC01A (at 1.27 -4.826 90) (layer B.Cu))
  (gr_text SDA (at 17.907 -7.62 90) (layer F.SilkS))
  (gr_text VDD (at 15.367 -7.62 90) (layer F.SilkS))
  (gr_text SCL (at 12.827 -7.62 90) (layer F.SilkS))
  (gr_text GND (at 10.287 -7.62 90) (layer F.SilkS))
  (gr_text SCL (at 30.607 -8.255) (layer F.SilkS))
  (gr_text SDA (at 30.607 -6.35) (layer F.SilkS))
  (gr_text GND (at 30.607 -1.016) (layer F.SilkS))
  (gr_text VDD (at 30.607 -2.921) (layer F.SilkS))
  (gr_text K (at 38.989 -1.397) (layer F.SilkS))
  (gr_line (start 0.254 -9.398) (end 0.254 0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -9.398) (end 40.386 -9.398) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 0.254) (end 40.386 -9.398) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 0.254) (end 40.386 0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.286 -12.192) (xy 44.577 -12.192) (xy 44.704 1.651) (xy -0.762 0.889)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.191 -14.605) (xy 47.244 -14.478) (xy 47.625 5.334) (xy -4.191 4.445) (xy -4.191 -14.605)
      )
    )
  )
)
