(kicad_pcb (version 4) (host pcbnew 0.201601041403+6416~40~ubuntu15.10.1-stable)
  (general
    (links 43)
    (no_connects 0)
    (area 103.030001 65.668 168.471428 130.170001)
    (thickness 1.6)
    (drawings 32)
    (tracks 134)
    (zones 0)
    (modules 19)
    (nets 9)
  )
  (page A4)
  (title_block
    (title "Rotational Position Sensor")
    (rev 01A)
    (company MLAB.cz)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 /SCL)
  (net 4 /SDA)
  (net 5 /PWM)
  (net 6 /A2)
  (net 7 /A1)
  (net 8 /VDD3V)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.254)
    (trace_width 0.3)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A1)
    (add_net /A2)
    (add_net /PWM)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VDD3V)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.5)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net VDD)
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 55D1E9F8)
    (at 135.16 99.76 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer B.SilkS))
    (fp_text value AS5048B (at -0.381 -0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /SDA))
    (pad 2 smd rect (at -2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /SCL))
    (pad 3 smd rect (at -2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /A2))
    (pad 4 smd rect (at -2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 /A1))
    (pad 5 smd rect (at -2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 12 smd rect (at 2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /VDD3V))
    (pad 13 smd rect (at 2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /PWM))
    (pad "" np_thru_hole circle (at 0 0 180) (size 4 4) (drill 4) (layers *.Cu F.Mask))
    (model Housings_SSOP/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 129.191 99.887 90)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /VDD3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 127.54 99.887 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 55125659)
    (at 133.89 77.916 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 1.27 0 180) (layer F.SilkS) hide)
    (pad 9 thru_hole rect (at -2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SCL))
    (pad 5 thru_hole rect (at 5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 3 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (pad 6 thru_hole rect (at 5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SCL))
    (pad 4 thru_hole rect (at 2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA))
    (pad 10 thru_hole rect (at -5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at 2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA))
    (pad 8 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 55125655)
    (at 141.51 77.916)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /PWM))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /PWM))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 55126217)
    (at 130.08 109.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 5512621C)
    (at 140.24 109.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 55126201)
    (at 140.24 89.6)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 551261F5)
    (at 130.08 89.6)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762) (layer F.SilkS) hide)
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 128.81 103.2525 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /VDD3V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 134.144 103.697 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /A1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /VDD3V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 137.065 104.586 90)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /A1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 134.144 105.729 180)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /A2))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /VDD3V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 135.16 108.523 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /A2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 135.16 94.553 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /SDA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 137.573 94.553 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /SCL))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:SMD_JUMP1X5 (layer B.Cu) (tedit 5512564D)
    (at 142.526 99.506 180)
    (fp_text reference J3 (at 14.859 3.81 180) (layer B.SilkS) hide)
    (fp_text value JUMP_5X2 (at -0.127 6.477 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0 -4 180) (size 4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2 180) (size 4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 3 smd rect (at 0 0 180) (size 4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 /SCL))
    (pad 4 smd rect (at 0 2 180) (size 4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 /SDA))
    (pad 5 smd rect (at 0 4 180) (size 4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 /PWM))
  )
  (module Mlab_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54BBE393)
    (at 131.5786 82.996 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C3 (at 0 3.556 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 54BBE0AF)
    (at 137.41298 82.996 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ADR (at 135.128 91.44) (layer F.SilkS))
  (gr_text 0x40 (at 135.128 93.726) (layer F.SilkS))
  (gr_text 5V (at 135.128 110.49) (layer F.SilkS))
  (gr_text 3V3 (at 133.096 113.03) (layer F.SilkS))
  (gr_text "4 x Hole for M3 screw.\nD = 3.2mm " (at 155 120) (layer Dwgs.User))
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "10,160 mm" (at 137.7 128.97) (layer Dwgs.User))
    (feature1 (pts (xy 140.24 109.92) (xy 140.24 129.13)))
    (feature2 (pts (xy 130.08 109.92) (xy 130.08 129.13)))
    (crossbar (pts (xy 130.08 126.43) (xy 140.24 126.43)))
    (arrow1a (pts (xy 140.24 126.43) (xy 139.113496 127.016421)))
    (arrow1b (pts (xy 140.24 126.43) (xy 139.113496 125.843579)))
    (arrow2a (pts (xy 130.08 126.43) (xy 131.206504 127.016421)))
    (arrow2b (pts (xy 130.08 126.43) (xy 131.206504 125.843579)))
  )
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "20,320 mm" (at 109.68 99.76 90) (layer Dwgs.User))
    (feature1 (pts (xy 130.08 89.6) (xy 108.33 89.6)))
    (feature2 (pts (xy 130.08 109.92) (xy 108.33 109.92)))
    (crossbar (pts (xy 111.03 109.92) (xy 111.03 89.6)))
    (arrow1a (pts (xy 111.03 89.6) (xy 111.616421 90.726504)))
    (arrow1b (pts (xy 111.03 89.6) (xy 110.443579 90.726504)))
    (arrow2a (pts (xy 111.03 109.92) (xy 111.616421 108.793496)))
    (arrow2b (pts (xy 111.03 109.92) (xy 110.443579 108.793496)))
  )
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "10,160 mm" (at 117.38 102.3 90) (layer Dwgs.User))
    (feature1 (pts (xy 130.08 99.76) (xy 118.49 99.76)))
    (feature2 (pts (xy 130.08 109.92) (xy 118.49 109.92)))
    (crossbar (pts (xy 121.19 109.92) (xy 121.19 99.76)))
    (arrow1a (pts (xy 121.19 99.76) (xy 121.776421 100.886504)))
    (arrow1b (pts (xy 121.19 99.76) (xy 120.603579 100.886504)))
    (arrow2a (pts (xy 121.19 109.92) (xy 121.776421 108.793496)))
    (arrow2b (pts (xy 121.19 109.92) (xy 120.603579 108.793496)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "5,08 mm" (at 135.16 121.35) (layer Dwgs.User))
    (feature1 (pts (xy 135.16 109.92) (xy 135.16 120.24)))
    (feature2 (pts (xy 130.08 109.92) (xy 130.08 120.24)))
    (crossbar (pts (xy 130.08 117.54) (xy 135.16 117.54)))
    (arrow1a (pts (xy 135.16 117.54) (xy 134.033496 118.126421)))
    (arrow1b (pts (xy 135.16 117.54) (xy 134.033496 116.953579)))
    (arrow2a (pts (xy 130.08 117.54) (xy 131.206504 118.126421)))
    (arrow2b (pts (xy 130.08 117.54) (xy 131.206504 116.953579)))
  )
  (dimension 19.812 (width 0.3) (layer Dwgs.User)
    (gr_text "19,812 mm" (at 135.16 67.168) (layer Dwgs.User))
    (feature1 (pts (xy 145.066 74.614) (xy 145.066 65.818)))
    (feature2 (pts (xy 125.254 74.614) (xy 125.254 65.818)))
    (crossbar (pts (xy 125.254 68.518) (xy 145.066 68.518)))
    (arrow1a (pts (xy 145.066 68.518) (xy 143.939496 69.104421)))
    (arrow1b (pts (xy 145.066 68.518) (xy 143.939496 67.931579)))
    (arrow2a (pts (xy 125.254 68.518) (xy 126.380504 69.104421)))
    (arrow2b (pts (xy 125.254 68.518) (xy 126.380504 67.931579)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 153.6804 94.68 90) (layer Dwgs.User))
    (feature1 (pts (xy 145.066 74.614) (xy 155.0304 74.614)))
    (feature2 (pts (xy 145.066 114.746) (xy 155.0304 114.746)))
    (crossbar (pts (xy 152.3304 114.746) (xy 152.3304 74.614)))
    (arrow1a (pts (xy 152.3304 74.614) (xy 152.916821 75.740504)))
    (arrow1b (pts (xy 152.3304 74.614) (xy 151.743979 75.740504)))
    (arrow2a (pts (xy 152.3304 114.746) (xy 152.916821 113.619496)))
    (arrow2b (pts (xy 152.3304 114.746) (xy 151.743979 113.619496)))
  )
  (gr_text GND (at 138.97 83.25 90) (layer F.SilkS))
  (gr_text GND (at 128.81 83.25 90) (layer F.SilkS))
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 v" (at 148.702 94.68 90) (layer Dwgs.User))
    (feature1 (pts (xy 145.066 74.614) (xy 150.052 74.614)))
    (feature2 (pts (xy 145.066 114.746) (xy 150.052 114.746)))
    (crossbar (pts (xy 147.352 114.746) (xy 147.352 74.614)))
    (arrow1a (pts (xy 147.352 74.614) (xy 147.938421 75.740504)))
    (arrow1b (pts (xy 147.352 74.614) (xy 146.765579 75.740504)))
    (arrow2a (pts (xy 147.352 114.746) (xy 147.938421 113.619496)))
    (arrow2b (pts (xy 147.352 114.746) (xy 146.765579 113.619496)))
  )
  (dimension 19.812 (width 0.3) (layer Dwgs.User)
    (gr_text "0,7800 v" (at 135.16 71.486) (layer Dwgs.User))
    (feature1 (pts (xy 145.066 74.614) (xy 145.066 70.136)))
    (feature2 (pts (xy 125.254 74.614) (xy 125.254 70.136)))
    (crossbar (pts (xy 125.254 72.836) (xy 145.066 72.836)))
    (arrow1a (pts (xy 145.066 72.836) (xy 143.939496 73.422421)))
    (arrow1b (pts (xy 145.066 72.836) (xy 143.939496 72.249579)))
    (arrow2a (pts (xy 125.254 72.836) (xy 126.380504 73.422421)))
    (arrow2b (pts (xy 125.254 72.836) (xy 126.380504 72.249579)))
  )
  (gr_text RPS01A (at 129.191 99.252 90) (layer F.SilkS))
  (gr_text MLAB (at 126.778 99.252 90) (layer F.SilkS))
  (gr_text PWM (at 141.51 80.964 90) (layer F.SilkS))
  (gr_text SDA (at 131.35 83.25 90) (layer F.SilkS))
  (gr_text SCL (at 136.43 81.218 90) (layer F.SilkS))
  (gr_text VI2C (at 133.89 80.964 90) (layer F.SilkS))
  (gr_text GND (at 144.558 103.697) (layer F.SilkS))
  (gr_text VI2C (at 144.558 101.538) (layer F.SilkS))
  (gr_text SCL (at 144.558 99.506) (layer F.SilkS))
  (gr_text SDA (at 144.558 97.474) (layer F.SilkS))
  (gr_text PWM (at 144.685 95.569) (layer F.SilkS))
  (gr_line (start 125.256 114.744) (end 125.256 74.616) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.256 74.616) (end 145.064 74.616) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.064 74.616) (end 145.064 114.744) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.256 114.744) (end 145.064 114.744) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.619 74.106) (xy 145.701 74.106) (xy 145.701 115.762) (xy 124.619 115.762)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.349 73.471) (xy 149.13 73.471) (xy 149.13 118.302) (xy 123.349 118.429)
      )
    )
  )
)
