{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["CT01A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CT01A","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["CT01A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R6",1,"RL140","RR 1R","110-001",0.8,"Odpor 0.6W"]
[2,"R14, R18",100,"R0805","RR-100R SMD","901-002",1]
[4,"R5, R11, R13, R15","1k","R0805","RR-1K SMD","901-029",1]
[1,"R10","1k2","R0805","RR-1K2 SMD","901-031",1]
[7,"R2, R3, R7, R8, R9, R12, R17","10k","R0805","RR-10K SMD","901-003",1]
[1,"R16","47k","R0805","RR-47K SMD","901-112",1]
[1,"R1","180k","R0805","RR-180K SMD","901-025",1]
[3,"R4, R19, R20","220k","R0805","RR-220K SMD","901-054",1]
["Odporové trimry"]
[3,"P1, P2, P3","47k/PT10MVK047","PT10V","PT10VK050","112-053",8,"Trimr na ležato"]
["Keramické kondenzátory"]
[1,"C9","#","C0805"]
[1,"C6","10nF","C0805","CK-10N X7R","906-089",2]
[13,"C2, C3, C4, C5, C7, C8, C10, C11, C12, C13, C14, C15, C16","100nF","C0805","CK-100N X7R","906-096",2,"Může být i Y5V nebo Z5U"]
["Elektrolytické kondenzátory"]
[1,"C1","100M/16V","CE025X6/L","E100M/16V","123-113",1]
["Diody"]
[1,"D1","1N4007","DO41","1N4007","220-002",1]
[1,"D2","BZX85_5V6","DO41","BZX85V005.6","222-234",1.5,"Zenerova dioda 1.3W, může být i 0.5W"]
["Tranzistory"]
[1,"Q1","MOS-N-ENH-D","TO263_3",null,null,null,"N-FET s Vt kolem 2V, v pouzdru TO263"]
[1,"Q2","BD136","TO126/L","BD136-16","211-084",6.5,"PNP tranzistor v TO126"]
["Integrované obvody"]
[1,"U1","LM7805T","TO220/L",7805,"330-001",8]
[1,"U2","LM358","DIP8_300","LM358","310-014",5,"Dvojtý OZ pro s nízkým napaájením"]
[1,"U3","PIC16F88/P","DIP18_300","PIC16F88-I/P","434-234",88]
[1,"U4","SC1602A","LCD_SC1602A",null,null,null,"Dvouřádkový displej www.hw.cz"]
[1,"U5","MAX232","SO16_150","MAX232 SMD",null,null,"Pouzdro SO16 úzké"]
["Mechanické součástky"]
[2,"SW1, SW2","P-B1720","PUSH050x050"]
[1,"J1","K375A","K375A"]
[1,"J2","JUMP4","JUMP4"]
[1,"J3","JUMP2X1","JUMP2X1"]
[1,"J4","JUMP3","JUMP3"]
[1,"J5","PIC_ISP","PIC_ISP"]
[1,"J6","RS232DB9M","DB9M_90"]
["Konstrukční součástky"]
[1,null,"Patice DIL 8 obyčejná",null,"SOKL 8",null,null,"Patice obyčejná DIL 8"]
[1,null,"Patice DIL 18 obyčejná",null,"SOKL 18",null,null,"Patice obyčejná DIL 18"]
[4,null,"Šroub M3x12 křížový s válcovou hlavou",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Distanční sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]
["Dodatečné součástky (viz ERRATA)"]
[4,null,"100nF","C0805","CK-100N X7R","906-096",2,"Může být i Y5V nebo Z5U"]
[1,null,"47uF/6.3V"]