{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"č.m.","Ib","Ub","Ik","Uk"]
[null,1,"6mA","0,63V","40mA","3,38V"]
[null,2]
[]
[]
[null,"Ib=6mA; Ub=0,63V"]
[null,"Uk (V)","Ik (mA)"]
[null,2,0]
[null,5,21,null,"2 údery"]
[null,6,22,null,"3 úderz"]
[null,7,25.5,null,1]
[null,8,31.5,null,0]
[null,9,38.5,null,0]
[null,10,55.5,null,0]
[null,11,76.4,null,0]
[null,12,126.7,null,0]
[null,13,245,null,0]
[null,14,361,null,0]
[]
[null,"Ib-10mA; Ub=0,66V"]
[null,"Uk","Ik"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}