{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":66,"n_cols":4,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["seznam součástek USB_PART_IRMRAK4 , IRMRAK4"]
[]
["USB_PART_IRMRAK4 "]
[]
["Quantity","Reference","Part","PCB Footprint"]
[]
["kondenzátory"]
[2,"C1,C2","1u","C0805"]
[8,"C3,C5,C6,C7,C8,C9,C10,C11","100nF","C0805"]
[1,"C4","4u7/6.3V","ELYTB"]
["diody"]
[1,"D1","BAR43SSMD","SOT23"]
[1,"D2","SMB","SMB"]
[4,"D3,D4,D5,D6","transil","SMB"]
[1,"D7","LED3mm_RED","2003-01-01"]
[1,"D8","LED3mm_GREEN","2003-01-01"]
["mechanika"]
[1,"J1","LOAD_POWER","ARK210/2"]
[1,"J2","DOME","ARK210/2"]
[1,"J3","POWER","ARK210/3"]
[1,"J4","USB_B_01","USB_B_01"]
[1,"J5","RS232","ARK210/3"]
[4,"M1","HOLE_M3","HOLE_M3"]
["optočlen"]
[1,"Q1","TLP127-SMD","MFSOP6"]
["tranzistory"]
[1,"Q2","BC817SMD","SOT23"]
["odpory"]
[1,"R1",150,"R0805"]
[1,"R2",180,"R0805"]
[2,"R5,R3","10k","R0805"]
[1,"R4","4k7","R0805"]
[2,"R6,R7",270,"R0805"]
["IO"]
[1,"U1","FT232RL","SSO28_210"]
[1,"U2","MAX232SMD","SO16_150"]
[]
[]
[]
["IRMRAK4"]
[]
["Quantity","Reference","Part","PCB Footprint "]
[]
["kondenzátory"]
[9,"C1,C2,C3,C4,C5,C6,C7,C9,C11","100nF","C0805"]
[1,"C8","10u/16V","ELYTB"]
[1,"C10","2.2u/6.3V_tantal","ELYTA"]
["diody"]
[4,"D1,D2,D3,D5","transil","SMB"]
[1,"D4","SMB","SMB"]
["mechanika"]
[1,"J2","PIC_ISP","PIC_ISP"]
[1,"J3","RS232","ARK210/3"]
[1,"J4","POWER","ARK210/3"]
[2,"M2,M1","HOLE_M3","HOLE_M3"]
["tranzistor"]
[1,"Q1","IRF7413SMD","SO8_FET"]
["rezistory"]
[3,"R1,R3,R4",100,"R0805"]
[1,"R2","47/5W","R5W"]
[2,"R7,R6","10k","R0805"]
["IO"]
[1,"U1","MAX232SMD","SO16_150"]
[1,"U2","PIC16F88_SO18","SO18_300"]
[1,"U3","LE33CD_SO8","SO8_150"]
[1,"U4","MLX90614_TO39","TO39_4"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}