{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["katalog","ks","co","skl. č.","cena","Σ","patro","pozn."]
["KONPC-SPK-3",20,"dutinky 3pin ","840-003",1,20,null,"kaklik"]
["FS18701-BL",20,"Faston 4,8 x 0,8 do DPS nastojato","834-021",0.9,18]
["L-53SRD-H",10,"LED 5mm červená 640nm difusní, max. 1500mcd@20mA, 60°","511-858",5,50]
["LED 5MM CYL. WHITE500mcd/100°",2,"LED 5MM CYL. WHITE500mcd/100°","511-459",15,30]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]
[{"$nulls":5},0]

{"sheet":"List2","index":1,"n_rows":2,"n_cols":8,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["katalog","ks","co","skl. č.","cena","Σ","patro","pozn."]
["CAB401",2,"kabel DB25V/DB25V","652-009",55]

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}