{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,"číslo měření","C přidané [nF]","C celkove [nF]","T vyp[ms]","T zap [ms]","f [Hz]"]
["k=",1,0,15,0.1,0.3,2500]
[15,2,34,49,3.6,5,116.27906976744185]
["nF",3,40,55,3.6,5.2,113.63636363636363]
[null,4,50,65,4,5.6,104.16666666666667]
[null,5,60,75,4.8,6,92.59259259259258]
[null,6,70,85,5.2,6.4,86.20689655172413]
[null,7,100,115,6.8,6.8,73.52941176470588]
[null,8,200,215,11.6,8.8,49.01960784313726]
[null,9,300,315,16.8,10.4,36.76470588235294]
[null,10,400,415,22,11.6,29.76190476190476]
[null,11,1000,1015,52,18,14.285714285714285]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}