{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":3,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,1,0,4]],"flags":["formulas_cached_only"]}
[null,"Žárovka 60W"]
[null,"r","U(33R2)mV"," I(33R2)mA","U(60R4)mV","I(60R4)mA","Ik (mA)"]
[null,0.1,1000,30.12048192771084,1900,31.456953642384107,36.6]
[]
[null,0.2,150,4.518072289156626,335,5.54635761589404,7.2]
[null,0.3,74,2.228915662650602,132.5,2.1937086092715234,3]
[null,0.4,41,1.2349397590361444,75.4,1.2483443708609272,1.6]
[null,0.5,27.2,0.8192771084337348,53.9,0.8923841059602649,1.1]
[null,0.6,21.3,0.641566265060241,37.4,0.619205298013245,0.8]
[null,0.7,16.9,0.5090361445783131,29.3,0.4850993377483444,0.6]
[null,0.8,12.6,0.37951807228915657,23.3,0.38576158940397354,0.5]
[null,0.9,10.8,0.3253012048192771,19.8,0.32781456953642385,0.4]
[null,1,9.6,0.2891566265060241,17.3,0.28642384105960267,0.3]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}