{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["VZOR"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"VZOR","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["VZOR"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[null,"R2,R6",100,null,null,null,1]
[null,"R1",68,null,null,null,1]
[null,"R3,R5",300]
[]
[]
["Odporové trimry"]
[null,"P1,P2","100k",null,null,null,13]
["Keramické kondenzátory"]
[null,"C3",56]
[null,"C4",22]
[null,"C13",270]
[null,"C5,C7,C6","10nF"]
[null,"C10",39]
[]
["Elektrolytické kondenzátory"]
[1,"C1","1000uF/6.3V"]
[1,"C4","10G/16V"]
["Indukčnosti"]
[1,"TR1","L-TR-1P1S_DOT"]
["Diody"]
[1,"D1","BZV55C5.6SMD"]
[2,"D2,D3","SK54ASMD"]
["Tranzistory"]
[1,"Q1","IRF7301"]
[1,"Q2","2N7002SMD"]
["Integrované obvody"]
[1,"U1","PIC16F88/SO"]
[1,"U2","LM385-1.2_SO8"]
["Mechanické součástky "]
[1,"J1","BAT"]
[3,"J2,J3,J6","JUMP2"]
[]
[]
[]
["Úkony:"]
[null,"Uložit pod novým jménem"]
[null,"Přejmenovat list"]
[null,"Přepsat jméno modulu na první řádce tabulky"]
[null,"Otevřít seznam jako další tabulku (textový soubor s tabulátory jako oddělovači)"]
[null,"Seřadit řádky v tabulce, seřadit reference podle logického pořadí."]
[null,"Nakopírovat příslušná data do vzorové tabulky"]
[null,"Vymazat pomocný list"]
[null,"Vymazat tento návod"]
[null,"Uložit seznam"]