{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["MBA81001A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"MBA81001A","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["MBA81001A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[1,"R2",1,"RL090","RR 1R","110-001",0.8,"Miniaturní odpor"]
[1,"R1",56,"RL090","RR 56R","110-043",0.8,"Miniaturní odpor"]
[1,"R3",100,"RL090","RR 100R","110-049",0.8,"Miniaturní odpor"]
["Potenciometry"]
[1,"P1","100k/log","PC1621","PC16MGK100","113-002",25,"Logaritmický potenciometr do plošných spojů, raději kovový"]
["Kondenzátory"]
[1,"C6",470,"CK050","CK 470P/500V","120-037",1,"Keramický kondenzátor"]
[1,"C5","2n7","CK050","CK 2N7/500V","120-047",1,"Keramický kondenzátor"]
[2,"C7,C10","100nF","CK050","CK 100N/63V","120-060",1,"Keramický kondenzátor"]
[1,"C1","1uF","MKT050X072X045","CF-1M0/J","121-340",6.5,"Fóliový kondenzátor"]
[3,"C3,C4,C9","100uF/25V","CE025X6","E100M/25V","123-117",1,"Elektrolytický kondenzátor"]
[1,"C2","500uF/25V","CE050X10","E470M/25V","123-157",2.5,"Elektrolytický kondenzátor"]
[1,"C8","1000uF/25V","CE050X13","E1000M/35V","123-178",6,"Elektrolytický kondenzátor"]
["Integrované obvody"]
[1,"U1","MBA810DS/DAS","K408/K409","K408/K409","ze zásob",null,"Zesilovač 5W TESLA"]
["Mechnaické součásti"]
[2,"J1,J2","JUMP3","JUMP3","S1G20","832-017",4,"Lámací hřebínek jednořadý, délka dle potřeby"]
[1,"J3","JUMP4","JUMP4","\"","\"",null,"Lámací hřebínek, délka dle potřeby"]
["Konstrukční díly"]
[1,null,"P-S8859",null,"P-S8859","624-085",11,"Knoflík pro potenciometr"]
[2,null,"KONPC-SPK-3",null,"KONPC-SPK-3","840-003",1,"Konektor pro jumper 1x3, včetně dutinek"]
[1,null,"KONPC-SPK-4",null,"KONPC-SPK-4","840-004",1,"Konektor pro jumper 1x4, včetně dutinek"]
[4,null,"DI5M3X5",null,"DI5M3X5","623-026",2.5,"Sloupek M3"]
[4,null,"M3x12",null,"Železářství","není",null,"Šroub M3x12 s válcovou hlavou křížový pozinkovaný"]
[4,null,"Podložka M3",null,"Železářství","není",null,"Podložka M3 pozinkovaná"]
[1,null,null,null,"Výroba PCB","není",null,"Plošný spoj MBA81001A"]