{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["USB232R01B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"USB232R01B","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["USB232R01B"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[2,"R4, R5","270R","R0805","R0805 270R","901-063",2]
[1,"R3","1k","R0805","R0805 1K","901-029",2]
[1,"R1","4k7","R0805","R0805 4K7","901-115",2]
[1,"R2","10k","R0805","R0805 10K","901-003",2]
["Keramické kondenzátory"]
[1,"C1","10nF","C0805","CK-10N X7R","906-089",2.5]
["5","C3, C4, C5, C6, C7","100nF","C0805","CK-100N X7R","906-096",2.5]
["Elektrolytické kondenzátory"]
[1,"C2","4u7/6.3V","ELYTB","CTS10M/6.3VB","907-109",3,"Nejbližší větší kapacita v pouzdru B"]
["Indukčnosti"]
[1,"L1","MI0805K400R-10","R0805","BLM21P300SPT","www.tme.cz",1.5,"Feritová perla 3A velikost 0805, Murata BLM21PG300SN1D, možno nahradit"]
["Diody"]
[1,"D1","1N4007SMD","MELF","1N4007SMD","917-005",1,"Obyčejná dioda 1A"]
[2,"D2, D3","LED3mm_RED","LED3","L-HLMP-1700FAI","511-396",3,"Červená LED 3mm pro malý proud"]
["Tranzistory"]
[1,"Q1","IRF7416SMD","SO8_FET","IRF7416 SMD","915-023",27,"Single P-FET SO8 Vtg < 2V"]
["Integrované obvody"]
[1,"U1","FT232RL","SSO28_210","FT232RL","nebrat od GM",120,"Dodavatel www.asix.cz"]
["Mechanické součástky "]
[1,"J1","USB_B_01","USB_B_01","USB-1X90B PCB","832-120",5,"USB zásuvka B do plošných spojů"]
[1,"J2","JUMP2X8","JUMP2X8","S2G40","832-050",8,"Lámat dle potřeby"]
[2,"J3, J4","JUMP2X3","JUMP2X3",null,null,null,"Lámat dle potřeby"]
[3,"J5, J6, J8","JUMP3","JUMP3","S1G20","832-017",4,"Lámat dle potřeby"]
["1","J7","JUMP2","JUMP2",null,null,null,"Lámat dle potřeby"]
["Konstrukční součásti"]
["4",null,"Šroub M3x12",null,"Železářství",null,null,"Válcová hlava, pozinkovaný"]
["4",null,"Podložka M3",null,"Železářství",null,null,"Podložka, pozinkovaná"]
["4",null,"Sloupek M3x5",null,"DI5M3X05","623-029",2.5,"Sloupek M3 vysoký 5mm"]
["1",null,"Jumper",null,"JUMP-RT RED","832-012",1,"Propojka 2.54mm"]
["1",null,"PCB",{"$nulls":4},"Plošný spoj modulu"]