{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["LCD2L4P01A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LCD2L4P01A","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["LCD2L4P01A"]
[]
["Počet","Reference","Název","Pouzdro","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
[4,"R1,R2,R3,R4","1k","R0805","RR-1K SMD","901-029",1,"SMD Odpor"]
[4,"R6,R7,R8,R9","10k","R0805","RR-10K SMD","901-003",1,"SMD Odpor"]
[1,"R5","47k","R0805","RR-47K SMD","901-112",1,"SMD Odpor"]
["Odporové trimry"]
[1,"P1","47k","PT10V","PT10VK050","112-053",8,"Trimr ležatý"]
["Keramické kondenzátory"]
[1,"C1","100nF","C0805","CK-100N Z5U","906-110",2,"SMD kondenzátor"]
["Polovodiče"]
[1,"D1","1N4004","DO41","1N4007","220-002",1,"Dioda 1A"]
[1,"U1","LCD_MODULE","LCD_SC1602A","SC1602A","www.hw.cz",120,"LCD displej 2 řádky po 16 znacích SC1602A"]
["Mechanické součástky"]
[4,"SW1,SW2,SW3,SW4","P-DT6GE","PUSH120","P-DT6GE","630-041",12,"Kulaté tlačítko"]
[1,"J4","JUMP1","JUMP1","S1G20","832-017",4,"Jumper 1 pin, lámou se dle potřeby"]
[2,"J5,J7","JUMP2","JUMP2","\"",null,0,"Jumper 2 piny, lámou se dle potřeby"]
[1,"J6","JUMP3","JUMP3","\"",null,0,"Jumper 3 piny, lámou se dle potřeby"]
[1,"J1+J2","JUMP2X3","JUMP2X3","S2G20","832-023",4,"Jumper dvouřadý 2x3 piny, lámou se dle potřeby"]
[2,"J8,J9","JUMP2X4","JUMP2X4","\"",null,0,"Jumper dvouřadý 2x4 piny, lámou se dle potřeby"]
[1,"J3","JUMP2X8","JUMP2X8","\"",null,0,"Jumper dvouřadý 2x8 pinů, lámou se dle potřeby"]
["Konstrukční součástky"]
[2,null,"Jumper",null,"JUMP-SW BLACK","832-013",1,"Propojka"]
[4,null,"Šroub M2.5x8, válcová hlava",null,"Železářství",null,null,"Šrouby pro připevnění LCD displeje"]
[4,null,"Matice M2.5",null,"Železářství",null,null,"Matice pro připevnění LCD displeje"]
[4,null,"Matice M3",null,"Železářství",null,null,"Distanční podložka pod LCD displej"]
[4,null,"Šroub M3x12, křížový, válcová hlava",null,"Železářství",null,null,"Rohový šroub"]
[4,null,"Podložka M3",null,"Železářství",null,null,"Podložka pod rohový šroub"]
[4,null,"Sloupek M3x5",null,"DI5M3X05","623-026",2.5,"Rohový sloupek"]