{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":4,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":41,"n_cols":17,"rows_kept":41,"cut":false,"hidden":false,"merged":[[30,1,34,1],[25,1,29,1],[20,1,24,1],[15,1,19,1],[10,1,14,1],[5,1,9,1]],"flags":["formulas_cached_only"]}
[]
[null,"Rč =",0.1297]
[]
[]
[null,"d [mm]","U [V]","I [mA]","P [mW]","S [VA]","Z [W]","L [H]","cosj"]
[null,0,1.64,2,0.5188,0.00328,820,2.61014103405685,0.158170731707317,null,null,null,"2 mA","4 mA","6 mA","8 mA","10 mA"]
[null,null,3.49,4,2.0752,0.01396,872.5,2.77725372626797,0.14865329512894,null,null,0,0.5188,2.0752,4.6692,8.3008,12.97]
[null,null,5.42,6,4.6692,0.03252,903.333333333333,2.87539927555536,0.143579335793358,null,null,0.5,0.5188,2.0752,4.6692,8.3008,12.97]
[null,null,7.4,8,8.3008,0.0592,925,2.94436641825608,0.140216216216216,null,"P",1,0.5188,2.0752,4.6692,8.3008,12.97]
[null,null,9.4,10,12.97,0.094,940,2.99211290164552,0.137978723404255,null,null,1.5,0.5188,2.0752,4.6692,8.3008,12.97]
[null,0.5,1.45,2,0.5188,0.0029,725,2.30774663790395,0.178896551724138,null,null,2,0.5188,2.0752,4.6692,8.3008,12.97]
[null,null,3.06,4,2.0752,0.01224,765,2.43507059430837,0.169542483660131,null,null,2.5,0.5188,2.0752,4.6692,8.3008,12.97]
[null,null,4.7,6,4.6692,0.0282,783.333333333333,2.49342740759449,0.165574468085106]
[null,null,6.42,8,8.3008,0.05136,802.5,2.55443680326269,0.161619937694704]
[null,null,8.17,10,12.97,0.0817,817,2.60059173735145,0.15875152998776,null,null,null,"2 mA","4 mA","6 mA","8 mA","10 mA"]
[null,1,1.1,2,0.5188,0.0022,550,1.75070432533232,0.235818181818182,null,null,0,820,872.5,903.333333333333,925,940]
[null,null,2.3,4,2.0752,0.0092,575,1.83028179899473,0.225565217391304,null,null,0.5,725,765,783.333333333333,802.5,817]
[null,null,3.55,6,4.6692,0.0213,591.666666666667,1.88333344800364,0.219211267605634,null,null,1,550,575,591.666666666667,610,605]
[null,null,4.88,8,8.3008,0.03904,610,1.94169026183065,0.212622950819672,null,"Z",1.5,475,500,508.333333333333,516.25,520]
[null,null,6.05,10,12.97,0.0605,605,1.92577476715873,0.214380165289256,null,null,2,450,445,458.333333333333,462.5,465]
[null,1.5,0.95,2,0.5188,0.0019,475,1.5119719030084,0.273052631578947,null,null,2.5,400,425,433.333333333333,437.5,440]
[null,null,2,4,2.0752,0.008,500,1.59154937737258,0.2594]
[null,null,3.05,6,4.6692,0.0183,508.333333333333,1.61807520209904,0.255147540983607]
[null,null,4.13,8,8.3008,0.03304,516.25,1.64327473556292,0.251234866828087,null,null,null,"2 mA","4 mA","6 mA","8 mA","10 mA"]
[null,null,5.2,10,12.97,0.052,520,1.65521135666881,0.249423076923077,null,null,0,2.61014103405685,2.77725372626797,2.87539927555536,2.94436641825608,2.99211290164552]
[null,2,0.9,2,0.5188,0.0018,450,1.43239442833108,0.288222222222222,null,"L",0.5,2.30774663790395,2.43507059430837,2.49342740759449,2.55443680326269,2.60059173735145]
[null,null,1.78,4,2.0752,0.00712,445,1.4164789333534,0.291460674157303,null,null,1,1.75070432533232,1.83028179899473,1.88333344800364,1.94169026183065,1.92577476715873]
[null,null,2.75,6,4.6692,0.0165,458.333333333333,1.45892025326148,0.282981818181818,null,null,1.5,1.5119719030084,1.59154937737258,1.61807520209904,1.64327473556292,1.65521135666881]
[null,null,3.7,8,8.3008,0.0296,462.5,1.47218316571206,0.280432432432432,null,null,2,1.43239442833108,1.4164789333534,1.45892025326148,1.47218316571206,1.48014091317788]
[null,null,4.65,10,12.97,0.0465,465,1.48014091317788,0.278924731182796,null,null,2.5,1.2732394778021914,1.35281695328537,1.37934277834548,1.39260569085822,1.40056343836052]
[null,2.5,0.8,2,0.5188,0.0016,400,1.2732394778021914,0.32425]
[null,null,1.7,4,2.0752,0.0068,425,1.35281695328537,0.305176470588235]
[null,null,2.6,6,4.6692,0.0156,433.333333333333,1.37934277834548,0.299307692307692,null,null,null,"2 mA","4 mA","6 mA","8 mA","10 mA"]
[null,null,3.5,8,8.3008,0.028,437.5,1.39260569085822,0.296457142857143,null,null,0,0.158170731707317,0.14865329512894,0.143579335793358,0.140216216216216,0.137978723404255]
[null,null,4.4,10,12.97,0.044,440,1.40056343836052,0.294772727272727,null,null,0.5,0.178896551724138,0.169542483660131,0.165574468085106,0.161619937694704,0.15875152998776]
[{"$nulls":10},"cos fí",1,0.235818181818182,0.225565217391304,0.219211267605634,0.212622950819672,0.214380165289256]
[{"$nulls":11},1.5,0.273052631578947,0.2594,0.255147540983607,0.251234866828087,0.249423076923077]
[{"$nulls":11},2,0.288222222222222,0.291460674157303,0.282981818181818,0.280432432432432,0.278924731182796]
[{"$nulls":4},"f(P)",{"$nulls":6},2.5,0.32425,0.305176470588235,0.299307692307692,0.296457142857143,0.294772727272727]
[{"$nulls":4},"f(L)"]
[{"$nulls":4},"f(cos)"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}