{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":44,"n_cols":4,"rows_kept":44,"cut":false,"hidden":false,"merged":[[2,1,2,3],[26,1,26,3],[46,1,46,3]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Tabulečička 1 - LED dioda [zelená]"]
[null,"č. m.","U [V]","I [mA]"]
[null,1,0,0]
[null,2,0.31,0]
[null,3,0.62,0]
[null,4,0.93,"0, 00008"]
[null,5,1.24,0.00012]
[null,6,1.55,0.00014]
[null,7,1.86,0.00018]
[null,8,2.17,0.00022]
[null,9,2.48,0.00166]
[null,10,2.5,0.0017]
[null,11,2.65,0.025]
[null,12,2.7,0.0778]
[null,13,2.75,0.254]
[null,14,2.79,0.659]
[null,15,2.85,2.07]
[null,16,2.9,4.39]
[null,17,2.95,7.32]
[null,18,3,11.4]
[null,19,3.05,16.64]
[null,20,3.078,19.99]
[]
[]
[null,"Tabulečička 2 - LED dioda [bílá]"]
[null,"č. m.","U [V]","I [mA]"]
[null,1,0,0]
[null,2,0.31,3e-05]
[null,3,0.62,5e-05]
[null,4,0.93,9e-05]
[null,5,1.24,0.00011]
[null,6,1.55,0.00014]
[null,7,1.86,0.0002]
[null,8,2.17,0.00084]
[null,9,2.48,0.08]
[null,10,2.5,0.13]
[null,11,2.6,0.84]
[null,12,2.7,2.91]
[null,13,2.79,5.67]
[null,14,2.85,8.47]
[null,15,2.95,14.09]
[null,16,3.04,19.99]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}