{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[null,null,"E [lx]","Ik [uA] (cca.)","Ik/U ","U [V]","Au (cca.)","citlivost rozsahu","mV/lx","UoutMAX [V] "]
[null,null,20,0.2,"1M",0.2,19,190,"mV/lx",3.8000000000000003]
[null,null,200,2,"M1",0.2,19,19,"mV/lx",3.8000000000000003]
[null,null,2000,20,"10k",0.2,19,1.9,"mV/lx",3.8000000000000003]
[null,null,20000,200,"1k",0.2,19,190,"mV/klx",3.8000000000000003]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}